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	Date:
	Oct 27-28, 2020

	Vehicle:
	CTD

	Location:
	[bookmark: Text2] Monterey Bay  

	Major Objective:
	 MBTS Diamond    

	Dive Plan:
	[bookmark: Text4] MBTS Diamond Pattern, gulp location provided by M.Blum    



Accomplishments:
· Nominal Launch and Recovery
· [bookmark: _GoBack]Mission completed (Mission Filename: Diamond_07042020.cfg)

Vehicle Issues:
[bookmark: Text6]     



Note(s):
· Mission failed to start because HydroScat commented out because the instrument wasn’t installed. This caused “AdaptiveSampling” to abort the mission because the program was expecting the HydroScat to be running.
· There is suspicion that during the 4th leg from SC back to ML there were a couple of kelp hang ups since there was a large grouping of GPS hits. Further investigation is needed.
· The HydroScat was not part of this mission and a 3lb weight was put in the vehicle to make up for the absence and a trim check was done.
· Batteries: Pack 30 in the AFT Battery Ball was turned off (or never was turned on). Laughlin looked into it further and it seems that it’s a random single pack shut-off/fail-to-start and no correlation to pack number, 
· The #2-5 Gulper Triggers were replaced on the motors, #1 still needs to be replaced. 
· It looks like the tubes to the sensors were plugged at depth and eventually cleared up (See IMAGES 01-03 below)
	IMAGES 01-03: Orange rectangles indicate section of the mission that the tubes were plugged up.
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IMAGE 01: Oxygen
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IMAGE 02: Salinity

	[image: ]
IMAGE 03: Nitrate
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