From: Ken Scussel 
Sent: Friday, March 12, 2010 5:12 PM
To: Adam Lipper
Subject: info on binary output 0 control line
 

ATZm – Command to locally set and clear binary output 0 control line.  This control line is available on J3 pin 6.

  m – State to set the line to. 

                0 – set the line low (0vdc)

1 - Set the line high (3.3vdc)

 

AT$Zn,m – Command to acoustically set and clear the binary output 0 control line.  This control line is available on J3 pin 6.  The receiving modem will acoustically acknowledge receipt of this command.

 n – Address of the modem

 m – State to set the line to. 

      0 – set the line low (0vdc)

1-      Set the line high (3.3vdc)

