Gulper Pin Puller Bench Test								30 Mar 2011





Required equipment





	Power Supply, 28V 1Amp


	Test Cable Assembly with PogoStick pins


	High Side LED, Relay and Hall Effect Switch board


	RS232 – RS485 Converter


	Computer with Hyperterm and RS-232 serial port


	Oscilloscope


	Digital Multimeter





Set Up





	 Inspect board for solder bridges, unsoldered connections, missing components


	See that the Hex switch is set to position “0”


	Plug in white Hirose connector to P3


	Position P2 Pins assembly into place guided by screws into PCB mounting holes


	Connect banana jacks into 28V power supply


	Connect a DB9 male into the RS-485 converter


	Hook up the RS-232 side of the converter to the computer's RS-232 serial port


	Run hyperterminal


		9600 8-N-1


		Send line ends with line feeds


		Echo typed characters locally


	Turn on the 28V power supply


	Current draw should be approx 20 – 40 mA





Procedure





	Ensure green Power On LED D6 is lit


	Type in $001Sff


		Response *0000


	Type in $001Fff


		Relay should click


		High Side red LED should be lit for approx ½ sec


	Push the Hall Effect Switch


	Type in $001Qff


		Response *003666


		( number of milliseconds between firing and Hall Effect switch closure )


	Type in $001Sff


		Response *000e


	Type in $001Rff


	Type in $001Sff


		Response *0000


	Remove DB9 and plug in the other DB9


	Repeat preceeding steps
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