2007 August 27, Internal Wave Test Plan
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2007-08-27


04:35 PDT  -0.65 feet  Low Tide


05:35 PDT   Moonset


06:33 PDT   Sunrise

0630 Meet on board

0700 Underway

0800 Launch at MISO_Inshore and run Mission_One.cfg.


11:04 PDT   4.19 feet  High Tide

1200 Recover AUV at MISO_Inshore and commence fast charge

1500 Launch at 25M_Curve_MISO and start overnight Mission_Two.cfg.

16:10 PDT   1.77 feet  Low Tide


19:30 PDT   Moonrise


19:42 PDT   Sunset


22:15 PDT   5.83 feet  High Tide

2007-08-28


03:37 PDT   Full Moon


05:09 PDT  -0.53 feet  Low Tide

0630 Meet on board


06:34 PDT   Sunrise


06:46 PDT   Moonset

0800 Underway

0930 Meet Vehicle at MISO_Inshore
1000 Recover Vehicle at 25M_Curve_MISO


11:32 PDT   4.48 feet  High Tide


16:59 PDT   1.38 feet  Low Tide


19:41 PDT   Sunset


19:58 PDT   Moonrise


23:03 PDT   5.63 feet  High Tide
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Waypoint Listing

	Waypoint Name
	Latitude
	Longitude
	Depth (meters/fathoms)

	25M_Curve_MISO
	36°37'0.00"N
	121°52'30.00"W
	25m / 14 fath

	MISO_Inshore
	36°38'15.00"N
	121°53'20.00"W
	62m / 34 fath

	MISO_Offshore
	36°39'60.00"N
	121°55'20.00"W
	86m / 47 fath

	
	
	
	


	Leg
	Distance
	Time to run
	Course

	25M_Curve_MISO to 

MISO_Inshore
	2600 m
	2000s or 33.33 min
	330º or 150º true

	MISO_Inshore to

MISO_Offshore
	4400 m
	3384s or 56.41 min
	317º or 137º true


List of missions available:

	Name
	Purpose

	“Mission_One.cfg”
	Yoyo to measure full water column temps over entire survey line
Time : Waypoint List

Launch at MISO_Inshore

0800 : MISO_Inshore
0835 : 25M_Curve_MISO

0910 : MISO_Inshore

1010 : MISO_Offshore

1110 : MISO_Inshore

1145 : 25M_Curve_MISO

Recovery at 25M_Curve_MISO



	“Mission_Two.cfg”
	Temperature Following to capture internal wave along time series survey line and connect it to phenomena near MISO facility at NPS.

Time : Waypoint List

Launch at 25M_Curve_MISO.
1500 : 25M_Curve_MISO

1535 : MISO_Inshore
1635 : MISO_Offshore
1735 : MISO_Inshore
1835 : MISO_Offshore
1935 : MISO_Inshore
2035 : MISO_Offshore
2135 : MISO_Inshore
2235 : MISO_Offshore
2335 : MISO_Inshore
0035 : MISO_Offshore
0135 : MISO_Inshore
0235 : MISO_Offshore
0335 : MISO_Inshore
0435 : MISO_Offshore
0535 : MISO_Inshore
0635 : MISO_Offshore
0735 : MISO_Inshore
0835 : MISO_Offshore
0935 : MISO_Inshore
1010 : 25M_Curve_MISO
Recovery at 25M_Curve_MISO



	“GoBack.cfg”
	Contingency use to reposition AUV to waypoint.  Must edit waypoint into file before use.
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