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These instructions should allow you to start and stop sampling with the LISST-HOLO instrument. This instrument has a serial port connection to the vehicle, which is connected to the sci4-dmo1 terminal server in the nose, at port 14001. If the instrument is connected via the ethernet cable, then you can find it at 134.89.32.44. There is a basic set of serial commands which the instrument understands, as well as a suite of standard UNIX shell commands. 
 
Before disconnecting the instrument ethernet connection:
1)telnet to the instrument ("telnet 134.89.32.44", login with username "root", password "40Smiles").
2)synchronize the time by using ntpdate ("ntpdate 134.89.32.117").
3)check free space on the filesystem using the "df" command, look at the free space on /mnt/flash1
4)disconnect the ethernet cable. If you power cycle the instrument after this point, then you'll need to repeat step 1-2 to resync the time.
 
Starting the instrument:
 
1)telnet to the sci4-dmo1 terminal server, port 14001 ("telnet sci4-dmo1 14001"). This can be done either on the laptop, if the vehicle is connected to the network, or by telnet'ing first to mvc-dmo1.
2)hit return to get a prompt. If prompted for a login username/password, use "root", password "40Smiles".
3)start sampling("/usr/sbin/holo start 1")
 
Stopping the instrument:
1)repeat steps 1 & 2 above to log in to the instrument
2)stop sampling ("/usr/sbin/holo stop")
 
Downloading data:
1)connect the ethernet cable to the instrument and plug in to the ship network
2)ftp to the instrument ("ncftp 134.89.32.44" or "ftp 134.89.32.44"). The instrument accepts an anonymous login.
3)cd into the images directory ("cd images")
4)get the relevant files
 
If you want to change sampling parameters, this is best done from the instrument web page (http://134.89.32.44).

