Bioacoustics Charging 
1.Hook up bioacoustics charge cable.
2. Turn ON I2 Map low current Tether
3.Remove bioacoustics magnet
4. Remote desktop into bioacoustics sphere.
6. Open Charge window.
5. Preview bioacoustics charge cable power supply. 
6. Verify power supply is set to 17.2V and 3 amps.
7. Check current draw on remote desktop then raise current limit to 5amps
8. Monitor Charge voltage and current (If you can’t monitor charging lower charge current to 2amps).
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Bioacoustics Shutdown
1. On via remote desktop shutdown bioacoustics sphere computer.
2. Install bioacoustics sphere magnet.
3. Turnoff bioacoustics sphere charge tether powersupply.
