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Procedure:
1. Bring vehicle on board
2. Proceed with shutdown procedure on AUV computer
a. Check to see if mission is still running
$ ps -ef   //this checks to see if the mission is still running
         //if you see a process called supervisor still running, then you do the following

$ slay supervisor

b. Check if recordings give indication of being successful
Check on browser 134.89.32.54 and click on "All Clips", makes sure you have 14 videos 6-8 minutes long 

c. Shut down camera system gracefully
$ carlTest 

 6  //Shut off recorder 
 3  //Shut off camera
 4  //Check status of Camera to make sure it is off, 0 indicates off, 1 indicates on
 7  //Check status of the recorder to make sre it is off

 1 //This exits the carlTest

d. Check environmental monitoring 
$ fanTest
 r

e. Check and turn off battery
telnet 134.89.32.121 10003
@99AF //turns off battery
			
3. Connect vehicle to tether 
a. Check if power supplies are off and that the voltage and current are setup correctly V<36 & I>10A 
b. Attach Tether to vehicle, then turn power supply on

4. Log back onto the vehicle
$ telnet mvc-dmo1

5. Check Camera system
$ carlTest 

//check on browser 134.89.32.54 and click on "All Clips", makes ure you have 14 videos 6-8 mintues long

 6 //turn recorder off
 3 // turn off camera (should be off already)
 7 //check recorder, =0
 4 //check camera, = 0
 1 //exit



6. [bookmark: _GoBack]Download log files
Note: Color indicates different Cygwin Windows
$ echo $AUV/logs //enter, this shows you the path of the log files
Open a second Cygwin terminal
//go to the directory that you want the logs to be downloaded into
$ ncftp -u dorado1 mvc-dmo1 
 ncftp /home/dorado1 > cd //insert directory that came from "echo $AUV.."command
 ls //find the latest directory Ex:2018.065.02/
 get -r //insert the latest directory
Close out


7. Center Tail cone
$ td newTailCone //we need to center the tail cone duct
e 0
r 0

Close Out

8. Turn off Tracking on Ranger 2
a. This prevents the system from just sitting and pinging in the harbor until someone notices.
b. Note: When your done in the control room please shut down power to the racks, turn off the overhead lights and close the control room door.
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