AUV Laptop Dovekie Network Setup

To have dovekie (autonomy laptop) talk directly to mvc-dmo1 we need to do the following.

1. on trex2:etc/rc.local add (this has been done already)
route add -network 10.250.32.0 gw 134.89.32.26 netmask 255.255.255.0 dev eth0
(first IP is dmo1's assigned 10.X address, second IP is dmo-1's assigned cabled IP). This ensures a static route to the 10.X between trex2 and dmo1

2. on dovekie: /etc/rc.local add (this has been done already)

ifconfig eth0:0 10.250.32.4 netmask 255.255.255.0

(first IP is dovekie's assigned IP on the 10.X Freewave modem network. Note 0 is zero)

3. check dovekie's address with:

% ifconfig eth0:0

(you should see the 10.X address on this interface)

4. when the cable connection with dmo1 is severed and the Freewave modem needs to be activated then on dovekie do:

% route add 134.89.32.39 gw 10.250.32.1 

which physically adds a route to the 10.X gateway

5. check to see if this is actually done by:

% route -v

which should show something like the following in a tabular output

trex2    10.250.32.1   UGH .......

Connection between dovekie and trex2 via dmo1 should be working at this stage.

