CTD_AUV Pre-Launch Checklist

· RESET DROPWEIGHT

· Visual Check of Capture Line and Pole

· Remove fairings, check foam packs

· Check Battery and Tailcone Comps

· Listen for Bathy Pump Sound

· Be sure Fairings and Rings are Secure

· Turn Strobe On

· Remove PTT Magnet

· Dummy Off The Tether 

· Check connector O-Rings

· Verify Access Door is Secure

· Check nose latch for free play

· Remove CTD Wetting Tubes

· Be sure all batteries are discharging
· Soak, then fanTest and Iridium Test
CTD_AUV Post-Recovery Checklist

· RESET DROPWEIGHT

· Park Tailcone off Zero

· USBL Pole Up

· Rinse Instruments, Install Wetting Tubes 

· Place Batteries On Charge

· Inspect Tailcone mechanical couplings

· Check Tailcone Compensation

· Check Sphere Pressure

· Turn Off USBL, Strobe

· Install PTT Magnet

· Clean LISST Windows 

· Turn off Hydroscat (telnet sci2-dmo1 140002 sleep)
· Upload Data & Fill out Gulper Sheet
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