	Command
	Expected Result

	Actuation Voltage Time

$AA1ACC

	Time elapsed: fire to pin puller retracted

*Note: Reports 0 if pin puller does not retract prior to proximity sensor interrupt

	Fire 

$AA1FCC

	Gulper fires and red LED lights

	Query Actuation Time

$AA1QCC

	Time elapsed: fire to proximity sensor activation

	Reset

$AA1RCC

	Invokes watchdog reset (CPU reset)

	Status

$AA1SCC

	Bit
1.) Sample fired 1=True 0=False (MSB)
2.) Pin-puller 1=Retracted 0=Not retracted
3.) Prox sensor 1=Activated properly 0=Not activated

4.) Prox error 1=Activated before firing 0=No error (LSB)
0xE – normal post-fire status
0xC – fired properly but did not fill

0x9 – commanded fire failed after previous misfire

0x8 – commanded fire failed

0x1 – misfire
All other values should not be possible without multiple failures


	Version

$AA1VCC

	Version of firmware loaded

	Invalid Command
	?AA COMMAND ERROR


