# Static Call Graph for image .\flash\i2c_master.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Nov 19 18:12:54 2013

### Maximum Stack Usage = 312 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ c_entry ⇒ debug_frmwrk_init ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SystemInit from system_lpc17xx.o(.text) referenced from startup_lpc17xx.o(.text)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UARTGetChar from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutChar from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutDec from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutDec16 from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutDec32 from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutHex from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutHex16 from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPutHex32 from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPuts from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - UARTPuts_ from debug_frmwrk.o(.text) referenced from debug_frmwrk.o(.text)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc17xx.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - main from master.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CLKPWR_SetPCLKDiv (Thumb, 106 bytes, Stack size 8 bytes, lpc17xx_clkpwr.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLKPWR_SetPCLKDiv
  [Called By]
  - >> I2C_Init

  CLKPWR_GetPCLKSEL (Thumb, 32 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> CLKPWR_GetPCLK

  CLKPWR_GetPCLK (Thumb, 58 bytes, Stack size 16 bytes, lpc17xx_clkpwr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLKPWR_GetPCLK
  [Calls]
  - >> CLKPWR_GetPCLKSEL
  [Called By]
  - >> uart_set_divisors
  - >> I2C_SetClock

  CLKPWR_ConfigPPWR (Thumb, 50 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> UART_DeInit
  - >> UART_Init
  - >> I2C_DeInit
  - >> I2C_Init

  CLKPWR_Sleep (Thumb, 10 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepSleep (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_PowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepPowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> uart_set_divisors
  - >> _printf_core
  - >> _fp_digits

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> c_entry

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  SystemCoreClockUpdate (Thumb, 312 bytes, Stack size 0 bytes, system_lpc17xx.o(.text), UNUSED)

  SystemInit (Thumb, 296 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  I2C_Init (Thumb, 126 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = I2C_Init ⇒ I2C_SetClock ⇒ CLKPWR_GetPCLK
  [Calls]
  - >> check_failed
  - >> CLKPWR_SetPCLKDiv
  - >> CLKPWR_ConfigPPWR
  - >> I2C_SetClock
  [Called By]
  - >> c_entry

  I2C_DeInit (Thumb, 90 bytes, Stack size 8 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> check_failed
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> c_entry

  I2C_Cmd (Thumb, 82 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_Cmd
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry

  I2C_IntCmd (Thumb, 92 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_IntCmd
  [Calls]
  - >> NVIC_DisableIRQ
  - >> NVIC_EnableIRQ
  [Called By]
  - >> I2C_SlaveTransferData
  - >> I2C_MasterTransferData
  - >> I2C_SlaveHandler
  - >> I2C_MasterHandler

  I2C_MasterHanleStates (Thumb, 438 bytes, Stack size 32 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_MasterHanleStates
  [Calls]
  - >> I2C_GetByte
  - >> I2C_SendByte
  - >> I2C_Stop
  [Called By]
  - >> I2C_MasterTransferData
  - >> I2C_MasterHandler

  I2C_SlaveHanleStates (Thumb, 298 bytes, Stack size 20 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Called By]

  - >> I2C_SlaveTransferData
  - >> I2C_SlaveHandler

  I2C_MasterHandler (Thumb, 144 bytes, Stack size 24 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_MasterHanleStates
  - >> I2C_IntCmd
  - >> I2C_getNum

  I2C_SlaveHandler (Thumb, 148 bytes, Stack size 32 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_SlaveHanleStates
  - >> I2C_IntCmd
  - >> I2C_getNum

  I2C_MasterTransferData (Thumb, 214 bytes, Stack size 32 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = I2C_MasterTransferData ⇒ I2C_MasterHanleStates
  [Calls]
  - >> I2C_MasterHanleStates
  - >> I2C_IntCmd
  - >> I2C_Start
  - >> I2C_getNum
  [Called By]
  - >> c_entry

  I2C_SlaveTransferData (Thumb, 206 bytes, Stack size 40 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_SlaveHanleStates
  - >> I2C_IntCmd
  - >> I2C_getNum

  I2C_SetOwnSlaveAddr (Thumb, 170 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  I2C_MonitorModeConfig (Thumb, 92 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  I2C_MonitorModeCmd (Thumb, 126 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  I2C_MonitorGetDatabuffer (Thumb, 42 bytes, Stack size 8 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  I2C_MonitorHandler (Thumb, 40 bytes, Stack size 12 bytes, lpc17xx_i2c.o(.text), UNUSED)

  I2C_MasterTransferComplete (Thumb, 30 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_getNum

  I2C_SlaveTransferComplete (Thumb, 30 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_getNum

  UART_Init (Thumb, 440 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> uart_set_divisors
  - >> check_failed
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> debug_frmwrk_init

  UART_TxCmd (Thumb, 190 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_TxCmd
  [Calls]
  - >> check_failed
  [Called By]
  - >> debug_frmwrk_init
  - >> UART_DeInit

  UART_DeInit (Thumb, 66 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> UART_TxCmd
  - >> check_failed
  - >> CLKPWR_ConfigPPWR

  UART_ConfigStructInit (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> debug_frmwrk_init

  UART_SendByte (Thumb, 58 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SendByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Send

  UART_ReceiveByte (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_ReceiveByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Receive

  UART_Send (Thumb, 150 bytes, Stack size 56 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_SendByte
  [Called By]
  - >> UARTPutChar

  UART_Receive (Thumb, 122 bytes, Stack size 40 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_ReceiveByte
  [Called By]
  - >> UARTGetChar

  UART_ForceBreak (Thumb, 68 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IntConfig (Thumb, 260 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_GetLineStatus (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_GetIntId (Thumb, 52 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_CheckBusy (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text), UNUSED)

  UART_FIFOConfig (Thumb, 272 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_FIFOConfigStructInit (Thumb, 14 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text), UNUSED)

  UART_ABCmd (Thumb, 192 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_ABClearIntPending (Thumb, 66 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UARTPutChar (Thumb, 18 bytes, Stack size 16 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_Send
  [Called By]
  - >> UARTPutHex32
  - >> UARTPutHex16
  - >> UARTPutHex
  - >> UARTPutDec32
  - >> UARTPutDec16
  - >> UARTPutDec
  - >> UARTPuts
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTGetChar (Thumb, 26 bytes, Stack size 16 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = UARTGetChar ⇒ UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_Receive
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPuts (Thumb, 28 bytes, Stack size 16 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = UARTPuts ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPutChar
  [Called By]
  - >> UARTPutHex32
  - >> UARTPutHex16
  - >> UARTPutHex
  - >> UARTPuts_
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPuts_ (Thumb, 24 bytes, Stack size 16 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = UARTPuts_ ⇒ UARTPuts ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPuts
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutDec (Thumb, 96 bytes, Stack size 24 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = UARTPutDec ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutDec16 (Thumb, 160 bytes, Stack size 32 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = UARTPutDec16 ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutDec32 (Thumb, 280 bytes, Stack size 56 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = UARTPutDec32 ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutHex (Thumb, 66 bytes, Stack size 24 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = UARTPutHex ⇒ UARTPuts ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPuts
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutHex16 (Thumb, 66 bytes, Stack size 24 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = UARTPutHex16 ⇒ UARTPuts ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPuts
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  UARTPutHex32 (Thumb, 66 bytes, Stack size 24 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = UARTPutHex32 ⇒ UARTPuts ⇒ UARTPutChar ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTPuts
  - >> UARTPutChar
  [Address Reference Count : 1]
  - debug_frmwrk.o(.text)

  debug_frmwrk_init (Thumb, 158 bytes, Stack size 24 bytes, debug_frmwrk.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = debug_frmwrk_init ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> PINSEL_ConfigPin
  - >> UART_ConfigStructInit
  - >> UART_TxCmd
  - >> UART_Init
  [Called By]
  - >> c_entry

  PINSEL_ConfigTraceFunc (Thumb, 34 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_SetI2C0Pins (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_ConfigPin (Thumb, 36 bytes, Stack size 8 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = PINSEL_ConfigPin ⇒ set_ResistorMode
  [Calls]
  - >> set_OpenDrainMode
  - >> set_ResistorMode
  - >> set_PinFunc
  [Called By]
  - >> c_entry
  - >> debug_frmwrk_init

  print_menu (Thumb, 14 bytes, Stack size 8 bytes, master.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = print_menu
  [Called By]
  - >> c_entry

  Buffer_Init (Thumb, 42 bytes, Stack size 0 bytes, master.o(.text))
  [Called By]

  - >> c_entry

  c_entry (Thumb, 1420 bytes, Stack size 152 bytes, master.o(.text))
  [Stack]

  - Max Depth = 312
  - Call Chain = c_entry ⇒ debug_frmwrk_init ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_ui2d
  - >> __aeabi_ddiv
  - >> Buffer_Init
  - >> print_menu
  - >> PINSEL_ConfigPin
  - >> debug_frmwrk_init
  - >> I2C_MasterTransferData
  - >> I2C_Cmd
  - >> I2C_DeInit
  - >> I2C_Init
  - >> __2sprintf
  [Called By]
  - >> main

  main (Thumb, 4 bytes, Stack size 0 bytes, master.o(.text))
  [Stack]

  - Max Depth = 312
  - Call Chain = main ⇒ c_entry ⇒ debug_frmwrk_init ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> c_entry
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  check_failed (Thumb, 4 bytes, Stack size 0 bytes, master.o(.text))
  [Called By]

  - >> UART_ABClearIntPending
  - >> UART_ABCmd
  - >> UART_FIFOConfig
  - >> UART_GetIntId
  - >> UART_GetLineStatus
  - >> UART_IntConfig
  - >> UART_ForceBreak
  - >> UART_ReceiveByte
  - >> UART_SendByte
  - >> UART_DeInit
  - >> UART_TxCmd
  - >> UART_Init
  - >> I2C_MonitorGetDatabuffer
  - >> I2C_MonitorModeCmd
  - >> I2C_MonitorModeConfig
  - >> I2C_SetOwnSlaveAddr
  - >> I2C_Cmd
  - >> I2C_DeInit
  - >> I2C_Init
  - >> I2C_SetClock

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> c_entry
  - >> _fp_digits

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 26 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> _double_epilogue
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 164 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_epilogue
  - >> _double_round
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 38 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 92 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> c_entry

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  I2C_getNum (Thumb, 38 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_SlaveTransferComplete
  - >> I2C_MasterTransferComplete
  - >> I2C_SlaveTransferData
  - >> I2C_MasterTransferData
  - >> I2C_SlaveHandler
  - >> I2C_MasterHandler

  I2C_Start (Thumb, 32 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_MasterTransferData

  I2C_Stop (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_MasterHanleStates

  I2C_SendByte (Thumb, 62 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_MasterHanleStates

  I2C_GetByte (Thumb, 32 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_MasterHanleStates

  I2C_SetClock (Thumb, 98 bytes, Stack size 16 bytes, lpc17xx_i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_SetClock ⇒ CLKPWR_GetPCLK
  [Calls]
  - >> check_failed
  - >> CLKPWR_GetPCLK
  [Called By]
  - >> I2C_Init

  NVIC_EnableIRQ (Thumb, 24 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_IntCmd

  NVIC_DisableIRQ (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_i2c.o(.text))
  [Called By]

  - >> I2C_IntCmd

  uart_set_divisors (Thumb, 464 bytes, Stack size 80 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  - >> CLKPWR_GetPCLK
  [Called By]
  - >> UART_Init

  set_PinFunc (Thumb, 60 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_PinFunc
  [Called By]
  - >> PINSEL_ConfigPin

  set_ResistorMode (Thumb, 62 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_ResistorMode
  [Called By]
  - >> PINSEL_ConfigPin

  set_OpenDrainMode (Thumb, 44 bytes, Stack size 12 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = set_OpenDrainMode
  [Called By]
  - >> PINSEL_ConfigPin

  _fp_digits (Thumb, 326 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_ddiv
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1762 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf

  _printf_post_padding (Thumb, 38 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 48 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols