# Static Call Graph for image .\Flash\uart_int.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Aug 27 16:33:59 2013

### Maximum Stack Usage = 176 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SystemInit from system_lpc17xx.o(.text) referenced from startup_lpc17xx.o(.text)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from uart_interrupt_test.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc17xx.o(.text)
  - main from uart_interrupt_test.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CLKPWR_SetPCLKDiv (Thumb, 106 bytes, Stack size 8 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_GetPCLKSEL (Thumb, 32 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> CLKPWR_GetPCLK

  CLKPWR_GetPCLK (Thumb, 58 bytes, Stack size 16 bytes, lpc17xx_clkpwr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLKPWR_GetPCLK
  [Calls]
  - >> CLKPWR_GetPCLKSEL
  [Called By]
  - >> uart_set_divisors

  CLKPWR_ConfigPPWR (Thumb, 50 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> UART_DeInit
  - >> UART_Init

  CLKPWR_Sleep (Thumb, 10 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepSleep (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_PowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepPowerDown (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> uart_set_divisors

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  SystemCoreClockUpdate (Thumb, 312 bytes, Stack size 0 bytes, system_lpc17xx.o(.text), UNUSED)

  SystemInit (Thumb, 296 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  PINSEL_ConfigTraceFunc (Thumb, 34 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_SetI2C0Pins (Thumb, 16 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_ConfigPin (Thumb, 36 bytes, Stack size 8 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = PINSEL_ConfigPin ⇒ set_ResistorMode
  [Calls]
  - >> set_OpenDrainMode
  - >> set_ResistorMode
  - >> set_PinFunc
  [Called By]
  - >> c_entry

  UART_Init (Thumb, 440 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> check_failed
  - >> uart_set_divisors
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> c_entry

  UART_TxCmd (Thumb, 190 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_TxCmd
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry
  - >> UART_DeInit

  UART_DeInit (Thumb, 66 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_DeInit ⇒ UART_TxCmd
  [Calls]
  - >> check_failed
  - >> UART_TxCmd
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> c_entry

  UART_ConfigStructInit (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> c_entry

  UART_SendByte (Thumb, 58 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SendByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Send

  UART_ReceiveByte (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_ReceiveByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Receive

  UART_Send (Thumb, 150 bytes, Stack size 56 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_SendByte
  [Called By]
  - >> UART_IntTransmit

  UART_Receive (Thumb, 122 bytes, Stack size 40 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_ReceiveByte
  [Called By]
  - >> UART_IntReceive

  UART_ForceBreak (Thumb, 68 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IntConfig (Thumb, 260 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_IntConfig
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry
  - >> UARTReceive
  - >> UARTSend
  - >> UART_IntTransmit

  UART_GetLineStatus (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_GetLineStatus
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART0_IRQHandler

  UART_GetIntId (Thumb, 52 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_GetIntId
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART0_IRQHandler

  UART_CheckBusy (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> c_entry
  - >> UART_IntTransmit

  UART_FIFOConfig (Thumb, 272 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_FIFOConfig
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry

  UART_FIFOConfigStructInit (Thumb, 14 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> c_entry

  UART_ABCmd (Thumb, 192 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_ABClearIntPending (Thumb, 66 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IntTransmit (Thumb, 132 bytes, Stack size 8 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = UART_IntTransmit ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_CheckBusy
  - >> UART_IntConfig
  - >> UART_Send
  [Called By]
  - >> UARTSend
  - >> UART0_IRQHandler

  UART_IntReceive (Thumb, 74 bytes, Stack size 16 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_IntReceive ⇒ UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_Receive
  [Called By]
  - >> UART0_IRQHandler

  UART_IntErr (Thumb, 4 bytes, Stack size 0 bytes, uart_interrupt_test.o(.text))
  [Called By]

  - >> UART0_IRQHandler

  UART0_IRQHandler (Thumb, 60 bytes, Stack size 16 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = UART0_IRQHandler ⇒ UART_IntTransmit ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_IntErr
  - >> UART_IntReceive
  - >> UART_IntTransmit
  - >> UART_GetIntId
  - >> UART_GetLineStatus
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UARTSend (Thumb, 106 bytes, Stack size 24 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = UARTSend ⇒ UART_IntTransmit ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_IntTransmit
  - >> UART_IntConfig
  [Called By]
  - >> c_entry
  - >> print_menu

  UARTReceive (Thumb, 94 bytes, Stack size 24 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UARTReceive ⇒ UART_IntConfig
  [Calls]
  - >> UART_IntConfig
  [Called By]
  - >> c_entry

  print_menu (Thumb, 60 bytes, Stack size 16 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = print_menu ⇒ UARTSend ⇒ UART_IntTransmit ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UARTSend
  [Called By]
  - >> c_entry

  c_entry (Thumb, 296 bytes, Stack size 40 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> print_menu
  - >> UARTReceive
  - >> UARTSend
  - >> UART_FIFOConfigStructInit
  - >> UART_FIFOConfig
  - >> UART_CheckBusy
  - >> UART_IntConfig
  - >> UART_ConfigStructInit
  - >> UART_DeInit
  - >> UART_TxCmd
  - >> UART_Init
  - >> PINSEL_ConfigPin
  [Called By]
  - >> main

  main (Thumb, 4 bytes, Stack size 0 bytes, uart_interrupt_test.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = main ⇒ c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> c_entry
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  check_failed (Thumb, 4 bytes, Stack size 0 bytes, uart_interrupt_test.o(.text))
  [Called By]

  - >> UART_ABClearIntPending
  - >> UART_ABCmd
  - >> UART_FIFOConfig
  - >> UART_GetIntId
  - >> UART_GetLineStatus
  - >> UART_IntConfig
  - >> UART_ForceBreak
  - >> UART_ReceiveByte
  - >> UART_SendByte
  - >> UART_DeInit
  - >> UART_TxCmd
  - >> UART_Init

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  set_PinFunc (Thumb, 60 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_PinFunc
  [Called By]
  - >> PINSEL_ConfigPin

  set_ResistorMode (Thumb, 62 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_ResistorMode
  [Called By]
  - >> PINSEL_ConfigPin

  set_OpenDrainMode (Thumb, 44 bytes, Stack size 12 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = set_OpenDrainMode
  [Called By]
  - >> PINSEL_ConfigPin

  uart_set_divisors (Thumb, 464 bytes, Stack size 80 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_uldivmod
  - >> CLKPWR_GetPCLK
  [Called By]
  - >> UART_Init

  ### Undefined Global Symbols