| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Mouse Device
USB examples

## Detailed Description

Example description
This example implements a HID device which is used for mouse configuration.

When the example is run and the board is connected to a PC with a USB cable it will enumerate on the PC as a HID mouse device and the joystick (SW2) on the EA Baseboard will generate mouse movement on your PC.

Special connection requirements

- EA1788 and EA4088 Developer's Kits
  - Short jumper JP15 near 20 pin JTAG connector

Build procedures:
LPC17xx/40xx example quickstart for Keil uVision4
LPC17xx/40xx example quickstart for IAR EWARM
LPC17xx/40xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Embedded Artists' LPC1788 Developer's Kit
Embedded Artists' LPC4088 Developer's Kit

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Main definitions