| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
usbd_hw.h
Go to the documentation of this file.
1 /*
2 * @brief USB ROM based hardware function prototypes
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #include "error.h"
33 #include "usbd.h"
34 #include "usbd_core.h"
35
36 #ifndef __USBHW_H__
37 #define __USBHW_H__
38
39
50 enum USBD_EVENT_T {
51 USB_EVT_SETUP =1,
52 USB_EVT_OUT,
53 USB_EVT_IN,
54 USB_EVT_OUT_NAK,
55 USB_EVT_IN_NAK,
56 USB_EVT_OUT_STALL,
57 USB_EVT_IN_STALL,
58 USB_EVT_OUT_DMA_EOT,
59 USB_EVT_IN_DMA_EOT,
60 USB_EVT_OUT_DMA_NDR,
61 USB_EVT_IN_DMA_NDR,
62 USB_EVT_OUT_DMA_ERR,
63 USB_EVT_IN_DMA_ERR,
64 USB_EVT_RESET,
65 USB_EVT_SOF,
66 USB_EVT_DEV_STATE,
67 USB_EVT_DEV_ERROR,
68 };
69
77 typedef struct USBD_HW_API
78 {
90 uint32_t (*GetMemSize)(USBD_API_INIT_PARAM_T* param);
91
106 ErrorCode_t (*Init)(USBD_HANDLE_T* phUsb, USB_CORE_DESCS_T* pDesc, USBD_API_INIT_PARAM_T* param);
107
121 void (*Connect)(USBD_HANDLE_T hUsb, uint32_t con);
122
134 void (*ISR)(USBD_HANDLE_T hUsb);
135
146 void (*Reset)(USBD_HANDLE_T hUsb);
147
159 void (*ForceFullSpeed )(USBD_HANDLE_T hUsb, uint32_t cfg);
160
178 void (*WakeUpCfg)(USBD_HANDLE_T hUsb, uint32_t cfg);
179
195 void (*SetAddress)(USBD_HANDLE_T hUsb, uint32_t adr);
196
211 void (*Configure)(USBD_HANDLE_T hUsb, uint32_t cfg);
212
228 void (*ConfigEP)(USBD_HANDLE_T hUsb, USB_ENDPOINT_DESCRIPTOR *pEPD);
229
244 void (*DirCtrlEP)(USBD_HANDLE_T hUsb, uint32_t dir);
245
256 void (*EnableEP)(USBD_HANDLE_T hUsb, uint32_t EPNum);
257
268 void (*DisableEP)(USBD_HANDLE_T hUsb, uint32_t EPNum);
269
280 void (*ResetEP)(USBD_HANDLE_T hUsb, uint32_t EPNum);
281
292 void (*SetStallEP)(USBD_HANDLE_T hUsb, uint32_t EPNum);
293
304 void (*ClrStallEP)(USBD_HANDLE_T hUsb, uint32_t EPNum);
305
322 ErrorCode_t (*SetTestMode)(USBD_HANDLE_T hUsb, uint8_t mode);
323
336 uint32_t (*ReadEP)(USBD_HANDLE_T hUsb, uint32_t EPNum, uint8_t *pData);
337
352 uint32_t (*ReadReqEP)(USBD_HANDLE_T hUsb, uint32_t EPNum, uint8_t *pData, uint32_t len);
353
366 uint32_t (*ReadSetupPkt)(USBD_HANDLE_T hUsb, uint32_t EPNum, uint32_t *pData);
367
381 uint32_t (*WriteEP)(USBD_HANDLE_T hUsb, uint32_t EPNum, uint8_t *pData, uint32_t cnt);
382
396 void (*WakeUp)(USBD_HANDLE_T hUsb);
397
413 ErrorCode_t (*EnableEvent)(USBD_HANDLE_T hUsb, uint32_t EPNum, uint32_t event_type,
414 uint32_t enable);
415
416 } USBD_HW_API_T;
417
418
419
420
421 #endif /* __USBHW_H__ */