| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Functions
creg_18xx_43xx.h File Reference

Go to the source code of this file.

## Data Structures
struct | LPC_CREG_T
| CREG Register Block. More...

## Functions
STATIC INLINE uint32_t | Chip_CREG_OnChipFlashIsPresent (void)
| Identifies whether on-chip flash is present.
STATIC INLINE void | Chip_CREG_SetFlashAcceleration (uint32_t Hz)
| Configures the onboard Flash Accelerator in flash-based LPC18xx/LPC43xx parts.
STATIC INLINE void | Chip_CREG_EnableUSB0Phy (bool Enable)
| Enables the USB0 high-speed PHY on LPC18xx/LPC43xx parts.
STATIC INLINE void | Chip_CREG_ConfigureBODaR (uint32_t BODVL, uint32_t BORVL)
| Configures the BOD and Reset on LPC18xx/LPC43xx parts.