| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Typedefs
chip_lpc18xx.h File Reference
`#include "lpc_types.h"`
`#include "sys_config.h"`
`#include "adc_001.h"`
`#include "atimer_001.h"`
`#include "ccan_001.h"`
`#include "dac_001.h"`
`#include "emc_001.h"`
`#include "enet_001.h"`
`#include "gima_001.h"`
`#include "gpdma_001.h"`
`#include "gpiogrpint_001.h"`
`#include "gpiopinint_001.h"`
`#include "gpio_001.h"`
`#include "i2c_001.h"`
`#include "i2s_001.h"`
`#include "lcd_001.h"`
`#include "mcpwm_001.h"`
`#include "pmc_001.h"`
`#include "qei_001.h"`
`#include "regfile_001.h"`
`#include "ritimer_001.h"`
`#include "rtc_001.h"`
`#include "sct_001.h"`
`#include "sdmmc_001.h"`
`#include "ssp_001.h"`
`#include "timer_001.h"`
`#include "usart_001.h"`
`#include "usbhs_001.h"`
`#include "wwdt_001.h"`
`#include "rgu_18xx_43xx.h"`
`#include "cguccu_18xx_43xx.h"`
`#include "eeprom_002.h"`
`#include "clock_18xx_43xx.h"`
`#include "gpio_18xx_43xx.h"`
`#include "uart_18xx_43xx.h"`
`#include "gpdma_18xx_43xx.h"`
`#include "enet_18xx_43xx.h"`
`#include "i2c_18xx_43xx.h"`
`#include "i2s_18xx_43xx.h"`
`#include "ssp_18xx_43xx.h"`
`#include "rtc_18xx_43xx.h"`
`#include "evrt_18xx_43xx.h"`
`#include "atimer_18xx_43xx.h"`
`#include "wwdt_18xx_43xx.h"`
`#include "ritimer_18xx_43xx.h"`
`#include "emc_18xx_43xx.h"`
`#include "lcd_18xx_43xx.h"`
`#include "adc_18xx_43xx.h"`
`#include "dac_18xx_43xx.h"`
`#include "sdif_18xx_43xx.h"`
`#include "sdmmc_18xx_43xx.h"`
`#include "timer_18xx_43xx.h"`
`#include "creg_18xx_43xx.h"`
`#include "scu_18xx_43xx.h"`
`#include "sct_18xx_43xx.h"`
`#include "ccan_18xx_43xx.h"`
`#include "pmc_18xx_43xx.h"`
`#include "otp_18xx_43xx.h"`
`#include "aes_18xx_43xx.h"`
`#include "eeprom_18xx_43xx.h"`

Go to the source code of this file.

## Macros
#define | LPC_SCT_BASE 0x40000000
#define | LPC_GPDMA_BASE 0x40002000
#define | LPC_SDMMC_BASE 0x40004000
#define | LPC_EMC_BASE 0x40005000
#define | LPC_USB0_BASE 0x40006000
#define | LPC_USB1_BASE 0x40007000
#define | LPC_LCD_BASE 0x40008000
#define | LPC_ETHERNET_BASE 0x40010000
#define | LPC_ATIMER_BASE 0x40040000
#define | LPC_REGFILE_BASE 0x40041000
#define | LPC_PMC_BASE 0x40042000
#define | LPC_CREG_BASE 0x40043000
#define | LPC_EVRT_BASE 0x40044000
#define | LPC_OTP_BASE 0x40045000
#define | LPC_RTC_BASE 0x40046000
#define | LPC_CGU_BASE 0x40050000
#define | LPC_CCU1_BASE 0x40051000
#define | LPC_CCU2_BASE 0x40052000
#define | LPC_RGU_BASE 0x40053000
#define | LPC_WWDT_BASE 0x40080000
#define | LPC_USART0_BASE 0x40081000
#define | LPC_USART2_BASE 0x400C1000
#define | LPC_USART3_BASE 0x400C2000
#define | LPC_UART1_BASE 0x40082000
#define | LPC_SSP0_BASE 0x40083000
#define | LPC_SSP1_BASE 0x400C5000
#define | LPC_TIMER0_BASE 0x40084000
#define | LPC_TIMER1_BASE 0x40085000
#define | LPC_TIMER2_BASE 0x400C3000
#define | LPC_TIMER3_BASE 0x400C4000
#define | LPC_SCU_BASE 0x40086000
#define | LPC_GPIO_PIN_INT_BASE 0x40087000
#define | LPC_GPIO_GROUP_INT0_BASE 0x40088000
#define | LPC_GPIO_GROUP_INT1_BASE 0x40089000
#define | LPC_MCPWM_BASE 0x400A0000
#define | LPC_I2C0_BASE 0x400A1000
#define | LPC_I2C1_BASE 0x400E0000
#define | LPC_I2S0_BASE 0x400A2000
#define | LPC_I2S1_BASE 0x400A3000
#define | LPC_C_CAN1_BASE 0x400A4000
#define | LPC_RITIMER_BASE 0x400C0000
#define | LPC_QEI_BASE 0x400C6000
#define | LPC_GIMA_BASE 0x400C7000
#define | LPC_DAC_BASE 0x400E1000
#define | LPC_C_CAN0_BASE 0x400E2000
#define | LPC_ADC0_BASE 0x400E3000
#define | LPC_ADC1_BASE 0x400E4000
#define | LPC_GPIO_PORT_BASE 0x400F4000
#define | LPC_SPI_BASE 0x40100000
#define | LPC_SGPIO_BASE 0x40101000
#define | LPC_EEPROM_BASE 0x4000E000
#define | LPC_SCT ((IP_SCT_001_T *) LPC_SCT_BASE)
#define | LPC_GPDMA ((IP_GPDMA_001_T *) LPC_GPDMA_BASE)
#define | LPC_SDMMC ((IP_SDMMC_001_T *) LPC_SDMMC_BASE)
#define | LPC_EMC ((IP_EMC_001_T *) LPC_EMC_BASE)
#define | LPC_USB0 ((IP_USBHS_001_T *) LPC_USB0_BASE)
#define | LPC_USB1 ((IP_USBHS_001_T *) LPC_USB1_BASE)
#define | LPC_LCD ((IP_LCD_001_T *) LPC_LCD_BASE)
#define | LPC_ETHERNET ((IP_ENET_001_T *) LPC_ETHERNET_BASE)
#define | LPC_ATIMER ((IP_ATIMER_001_T *) LPC_ATIMER_BASE)
#define | LPC_REGFILE ((IP_REGFILE_001_T *) LPC_REGFILE_BASE)
#define | LPC_PMC ((IP_PMC_001_T *) LPC_PMC_BASE)
#define | LPC_EVRT ((LPC_EVRT_T *) LPC_EVRT_BASE)
#define | LPC_RTC ((IP_RTC_001_T *) LPC_RTC_BASE)
#define | LPC_CGU ((LPC_CGU_T *) LPC_CGU_BASE)
#define | LPC_CCU1 ((LPC_CCU1_T *) LPC_CCU1_BASE)
#define | LPC_CCU2 ((LPC_CCU2_T *) LPC_CCU2_BASE)
#define | LPC_CREG ((LPC_CREG_T *) LPC_CREG_BASE)
#define | LPC_RGU ((LPC_RGU_T *) LPC_RGU_BASE)
#define | LPC_WWDT ((IP_WWDT_001_T *) LPC_WWDT_BASE)
#define | LPC_USART0 ((IP_USART_001_T *) LPC_USART0_BASE)
#define | LPC_USART2 ((IP_USART_001_T *) LPC_USART2_BASE)
#define | LPC_USART3 ((IP_USART_001_T *) LPC_USART3_BASE)
#define | LPC_UART1 ((IP_USART_001_T *) LPC_UART1_BASE)
#define | LPC_SSP0 ((IP_SSP_001_T *) LPC_SSP0_BASE)
#define | LPC_SSP1 ((IP_SSP_001_T *) LPC_SSP1_BASE)
#define | LPC_TIMER0 ((IP_TIMER_001_T *) LPC_TIMER0_BASE)
#define | LPC_TIMER1 ((IP_TIMER_001_T *) LPC_TIMER1_BASE)
#define | LPC_TIMER2 ((IP_TIMER_001_T *) LPC_TIMER2_BASE)
#define | LPC_TIMER3 ((IP_TIMER_001_T *) LPC_TIMER3_BASE)
#define | LPC_SCU ((LPC_SCU_T *) LPC_SCU_BASE)
#define | LPC_GPIO_PIN_INT ((IP_GPIOPININT_001_T *) LPC_GPIO_PIN_INT_BASE)
#define | LPC_GPIO_GROUP_INT0 ((IP_GPIOGROUPINT_001_T *) LPC_GPIO_GROUP_INT0_BASE)
#define | LPC_GPIO_GROUP_INT1 ((IP_GPIOGROUPINT_001_T *) LPC_GPIO_GROUP_INT1_BASE)
#define | LPC_MCPWM ((IP_MCPWM_001_T *) LPC_MCPWM_BASE)
#define | LPC_I2C0 ((IP_I2C_001_T *) LPC_I2C0_BASE)
#define | LPC_I2C1 ((IP_I2C_001_T *) LPC_I2C1_BASE)
#define | LPC_I2S0 ((IP_I2S_001_T *) LPC_I2S0_BASE)
#define | LPC_I2S1 ((IP_I2S_001_T *) LPC_I2S1_BASE)
#define | LPC_C_CAN1 ((IP_CCAN_001_T *) LPC_C_CAN1_BASE)
#define | LPC_RITIMER ((IP_RITIMER_001_T *) LPC_RITIMER_BASE)
#define | LPC_QEI ((IP_QEI_001_T *) LPC_QEI_BASE)
#define | LPC_GIMA ((IP_GIMA_001_T *) LPC_GIMA_BASE)
#define | LPC_DAC ((IP_DAC_001_T *) LPC_DAC_BASE)
#define | LPC_C_CAN0 ((IP_CCAN_001_T *) LPC_C_CAN0_BASE)
#define | LPC_ADC0 ((IP_ADC_001_T *) LPC_ADC0_BASE)
#define | LPC_ADC1 ((IP_ADC_001_T *) LPC_ADC1_BASE)
#define | LPC_GPIO_PORT ((IP_GPIO_001_T *) LPC_GPIO_PORT_BASE)
#define | LPC_EEPROM ((IP_EEPROM_002_T *) LPC_EEPROM_BASE)

## Typedefs
typedef IP_SCT_001_T | LPC_SCT_T
typedef IP_GPDMA_001_T | LPC_GPDMA_T
typedef IP_SDMMC_001_T | LPC_SDMMC_T
typedef IP_EMC_001_T | LPC_EMC_T
typedef IP_USBHS_001_T | LPC_USBHS_T
typedef IP_ENET_001_T | LPC_ENET_T
typedef IP_ATIMER_001_T | LPC_ATIMER_T
typedef IP_REGFILE_001_T | LPC_REGFILE_T
typedef IP_PMC_001_T | LPC_PMC_T
typedef IP_RTC_001_T | LPC_RTC_T
typedef IP_WWDT_001_T | LPC_WWDT_T
typedef IP_USART_001_T | LPC_USART_T
typedef IP_SSP_001_T | LPC_SSP_T
typedef IP_TIMER_001_T | LPC_TIMER_T
typedef IP_GPIOPININT_001_T | LPC_GPIOPININT_T
typedef IP_MCPWM_001_T | LPC_MCPWM_T
typedef IP_I2C_001_T | LPC_I2C_T
typedef IP_I2S_001_T | LPC_I2S_T
typedef IP_CCAN_001_T | LPC_CCAN_T
typedef IP_RITIMER_001_T | LPC_RITIMER_T
typedef IP_QEI_001_T | LPC_QEI_T
typedef IP_GIMA_001_T | LPC_GIMA_T
typedef IP_DAC_001_T | LPC_DAC_T
typedef IP_ADC_001_T | LPC_ADC_T
typedef IP_GPIO_001_T | LPC_GPIO_T
typedef IP_LCD_001_T | LPC_LCD_T
typedef IP_EEPROM_002_T | LPC_EEPROM_T