| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
FLASH_COPY_RAM_TO_FLASH_COMMAND_T Struct Reference
IP: Flash/EEPROM programming

## Detailed Description

[Copy Ram to Flash] command parameter table structure

Definition at line 195 of file flash_001.h.

`#include "flash_001.h"`

## Data Fields
uint32_t | cmd
uint32_t | dst
uint32_t | src
uint32_t | byteNum
uint32_t | cclk

## Field Documentation

uint32_t byteNum

Number of bytes to be written. Should be 256 | 512 | 1024 | 4096.

Definition at line 199 of file flash_001.h.

uint32_t cclk

System Clock Frequency (CCLK) in kHz.

Definition at line 200 of file flash_001.h.

uint32_t cmd

Command code

Definition at line 196 of file flash_001.h.

uint32_t dst

Destination flash address where data bytes are to be written (256 byte boundary)

Definition at line 197 of file flash_001.h.

uint32_t src

Source RAM address from which data bytes are to be read (a word boudary).

Definition at line 198 of file flash_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/flash_001.h