| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - c -

- C_GLCD_H_SIZE : board_keil_mcb_18574357.h
- C_GLCD_V_SIZE : board_keil_mcb_18574357.h
- CableNumber : MIDIClassCommon.h
- CalculateCountOfClusters() : fatutil.c , fatutil.h
- calibrateTSC2046() : board_ea_devkit_17884088.c , board_hitex_eva_18504350.c
- CALLBACK_Audio_Device_GetSetEndpointProperty() : AudioClassDevice.h , AudioOutput.c , AudioInput.c
- CALLBACK_Audio_Device_GetSetInterfaceProperty() : AudioInput.c
- CALLBACK_HAL_GetISOBufferAddress() : AudioOutput.c , AudioInput.c
- CALLBACK_HID_Device_CreateHIDReport() : HIDClassDevice.h , GenericHID.c , Keyboard.c , Mouse.c
- CALLBACK_HID_Device_ProcessHIDReport() : HIDClassDevice.h , GenericHID.c , Keyboard.c , Mouse.c
- CALLBACK_HIDParser_FilterHIDReportItem() : HIDParser.h , KeyboardHost.c
- CALLBACK_MS_Device_SCSICommandReceived() : MassStorageClassDevice.h , usbmsdev.c , usbmsdev.h , MassStorage_ucosiii.c , MassStorage.c
- CALLBACK_USB_GetDescriptor() : Device.h , Descriptors.c , Descriptors.h , Descriptors.c
- CALLBACK_UsbdCdc_Register_ControlInterfaceDescriptor() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInEndpointSize() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInterfaceDescriptor() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataOutEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataOutEndpointSize() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_LineCoding() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_NotificationEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdHid_IsReportChanged() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_Register_InterfaceDescriptor() : UsbRom.h , usbd_hid.h
- CALLBACK_UsbdHid_Register_ReportDescriptor() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_Register_ReportInBuffer() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_SetReport() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_SetReportChange() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_BlockCount() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_BlockSize() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_InquiryData() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_InterfaceDescriptor() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MemorySize() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCGetWriteBuf() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCRead() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCVerify() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCWrite() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdRom_Register_ConfigurationDescriptor() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_ConfigureEndpoint() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_DeviceDescriptor() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_DeviceQualifierDescriptor() : UsbRom.h , usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_StringDescriptor() : usbd.h , UsbRom.h
- CAN0_IRQHandler() : ccan.c
- CAN_AF_BYBASS_MODE : can_17xx_40xx.h
- CAN_AF_FULL_MODE : can_17xx_40xx.h
- CAN_AF_NORMAL_MODE : can_17xx_40xx.h
- CAN_AF_OFF_MODE : can_17xx_40xx.h
- CAN_BTR_BITMASK : can_001.h
- CAN_BTR_BRP : can_001.h
- CAN_BTR_SAM : can_001.h
- CAN_BTR_SJW : can_001.h
- CAN_BTR_TESG1 : can_001.h
- CAN_BTR_TESG2 : can_001.h
- CAN_BUFFER_1 : can_001.h
- CAN_BUFFER_2 : can_001.h
- CAN_BUFFER_3 : can_001.h
- CAN_BUFFER_ID : can_17xx_40xx.h
- CAN_BUFFER_LAST : can_001.h
- CAN_CMR_AT : can_001.h
- CAN_CMR_BITMASK : can_001.h
- CAN_CMR_CDO : can_001.h
- CAN_CMR_RRB : can_001.h
- CAN_CMR_SRR : can_001.h
- CAN_CMR_STB : can_001.h
- CAN_CMR_TR : can_001.h
- CAN_CTRL_NO : can.c
- CAN_error() : ccan_rom.c
- CAN_ERROR_ACK : ccand_11xx.h
- CAN_ERROR_BIT0 : ccand_11xx.h
- CAN_ERROR_BIT1 : ccand_11xx.h
- CAN_ERROR_BOFF : ccand_11xx.h
- CAN_ERROR_CRC : ccand_11xx.h
- CAN_ERROR_FORM : ccand_11xx.h
- CAN_ERROR_NONE : ccand_11xx.h
- CAN_ERROR_PASS : ccand_11xx.h
- CAN_ERROR_STUF : ccand_11xx.h
- CAN_ERROR_WARN : ccand_11xx.h
- CAN_EWL_BITMASK : can_001.h
- CAN_EWL_VAL : can_001.h
- CAN_EXT_ENTRY_CTRL_NO_MASK : can_001.h
- CAN_EXT_ENTRY_CTRL_NO_POS : can_001.h
- CAN_EXT_ENTRY_ID_MASK : can_001.h
- CAN_EXT_ENTRY_ID_POS : can_001.h
- CAN_EXT_ID_ENTRY_T : can_17xx_40xx.h
- CAN_EXT_ID_RANGE_ENTRY_T : can_17xx_40xx.h
- CAN_EXTEND_ID_USAGE : can_001.h
- CAN_GSR_BITMASK : can_001.h
- CAN_GSR_BS : can_001.h
- CAN_GSR_DOS : can_001.h
- CAN_GSR_ES : can_001.h
- CAN_GSR_RBS : can_001.h
- CAN_GSR_RS : can_001.h
- CAN_GSR_RXERR : can_001.h
- CAN_GSR_TBS : can_001.h
- CAN_GSR_TCS : can_001.h
- CAN_GSR_TS : can_001.h
- CAN_GSR_TXERR : can_001.h
- CAN_ICR_ALCBIT_VAL : can_001.h
- CAN_ICR_ALI : can_001.h
- CAN_ICR_BEI : can_001.h
- CAN_ICR_BIT_ERROR : can_001.h
- CAN_ICR_BITMASK : can_001.h
- CAN_ICR_DOI : can_001.h
- CAN_ICR_EI : can_001.h
- CAN_ICR_EPI : can_001.h
- CAN_ICR_ERR_ACK : can_001.h
- CAN_ICR_ERR_ACK_DELIMITER : can_001.h
- CAN_ICR_ERR_CRC_DELIMITER : can_001.h
- CAN_ICR_ERR_CRC_SEQ : can_001.h
- CAN_ICR_ERR_DATA_FIELD : can_001.h
- CAN_ICR_ERR_DLC : can_001.h
- CAN_ICR_ERR_EOF : can_001.h
- CAN_ICR_ERR_ID12_ID5 : can_001.h
- CAN_ICR_ERR_ID17_ID13 : can_001.h
- CAN_ICR_ERR_ID20_ID18 : can_001.h
- CAN_ICR_ERR_ID28_ID21 : can_001.h
- CAN_ICR_ERR_ID4_ID0 : can_001.h
- CAN_ICR_ERR_IDE : can_001.h
- CAN_ICR_ERR_INTERMISSION : can_001.h
- CAN_ICR_ERR_ReservedBit_0 : can_001.h
- CAN_ICR_ERR_ReservedBit_1 : can_001.h
- CAN_ICR_ERR_RTR : can_001.h
- CAN_ICR_ERR_SOF : can_001.h
- CAN_ICR_ERR_SRTR : can_001.h
- CAN_ICR_ERRBIT_VAL : can_001.h
- CAN_ICR_ERRC_VAL : can_001.h
- CAN_ICR_ERRDIR_RECEIVE : can_001.h
- CAN_ICR_FORM_ERROR : can_001.h
- CAN_ICR_IDI : can_001.h
- CAN_ICR_OTHER_ERROR : can_001.h
- CAN_ICR_RI : can_001.h
- CAN_ICR_STUFF_ERROR : can_001.h
- CAN_ICR_TI1 : can_001.h
- CAN_ICR_TI2 : can_001.h
- CAN_ICR_TI3 : can_001.h
- CAN_ICR_WUI : can_001.h
- CAN_IER_ALIE : can_001.h
- CAN_IER_BEIE : can_001.h
- CAN_IER_BITMASK : can_001.h
- CAN_IER_DOIE : can_001.h
- CAN_IER_EIE : can_001.h
- CAN_IER_EPIE : can_001.h
- CAN_IER_IDIE : can_001.h
- CAN_IER_RIE : can_001.h
- CAN_IER_TIE1 : can_001.h
- CAN_IER_TIE2 : can_001.h
- CAN_IER_TIE3 : can_001.h
- CAN_IER_WUIE : can_001.h
- CAN_IRQHandler() : can.c , ccan_rom.c
- CAN_LISTEN_ONLY_MODE : can_17xx_40xx.h
- CAN_MOD_BITMASK : can_001.h
- CAN_MOD_LOM : can_001.h
- CAN_MOD_OPERATION : can_001.h
- CAN_MOD_RM : can_001.h
- CAN_MOD_RPM : can_001.h
- CAN_MOD_SM : can_001.h
- CAN_MOD_STM : can_001.h
- CAN_MOD_TM : can_001.h
- CAN_MOD_TPM : can_001.h
- CAN_MSG_MAX_DATA_LEN : can_001.h
- CAN_MSG_T : can_17xx_40xx.h
- CAN_MSGOBJ_DAT : ccand_11xx.h
- CAN_MSGOBJ_EXT : ccand_11xx.h
- CAN_MSGOBJ_RTR : ccand_11xx.h
- CAN_MSGOBJ_STD : ccand_11xx.h
- CAN_MSR_BITMASK : can_001.h
- CAN_MSR_BS : can_001.h
- CAN_MSR_E : can_001.h
- CAN_OPERATION_MODE : can_17xx_40xx.h
- CAN_RECEIVE_PRIORITY_MODE : can_17xx_40xx.h
- CAN_REMOTE_MSG : can_001.h
- CAN_RESET_MODE : can_17xx_40xx.h
- CAN_RFS_BITMASK : can_001.h
- CAN_RFS_BP : can_001.h
- CAN_RFS_DLC : can_001.h
- CAN_RFS_FF : can_001.h
- CAN_RFS_ID_INDEX : can_001.h
- CAN_RFS_RTR : can_001.h
- CAN_RID_ID_11 : can_001.h
- CAN_RID_ID_29 : can_001.h
- CAN_RSR_BITMASK : can_001.h
- CAN_RSR_DOS : can_001.h
- CAN_RSR_RBS : can_001.h
- CAN_RSR_RS : can_001.h
- CAN_rx() : ccan_rom.c
- CAN_RX_MSG_ID : can.c
- CAN_SDOREQ_HANDLED_NOSEND : ccand_11xx.h
- CAN_SDOREQ_HANDLED_SEND : ccand_11xx.h
- CAN_SDOREQ_NOTHANDLED : ccand_11xx.h
- CAN_SDOSEG_CLOSE : ccand_11xx.h
- CAN_SDOSEG_OPEN : ccand_11xx.h
- CAN_SDOSEG_SEGMENT : ccand_11xx.h
- CAN_SEG1_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SEG2_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SELFTEST_MODE : can_17xx_40xx.h
- CAN_SJW_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SLEEP_MODE : can_17xx_40xx.h
- CAN_SR_BITMASK : can_001.h
- CAN_SR_BS : can_001.h
- CAN_SR_DOS : can_001.h
- CAN_SR_ES : can_001.h
- CAN_SR_RBS : can_001.h
- CAN_SR_RS : can_001.h
- CAN_SR_TBS : can_001.h
- CAN_SR_TCS : can_001.h
- CAN_SR_TS : can_001.h
- CAN_STD_ENTRY_CTRL_NO_MASK : can_001.h
- CAN_STD_ENTRY_CTRL_NO_POS : can_001.h
- CAN_STD_ENTRY_DISABLE_MASK : can_001.h
- CAN_STD_ENTRY_DISABLE_POS : can_001.h
- CAN_STD_ENTRY_ID_MASK : can_001.h
- CAN_STD_ENTRY_ID_POS : can_001.h
- CAN_STD_ENTRY_IE_MASK : can_001.h
- CAN_STD_ENTRY_IE_POS : can_001.h
- CAN_STD_ID_ENTRY_T : can_17xx_40xx.h
- CAN_STD_ID_RANGE_ENTRY_T : can_17xx_40xx.h
- CAN_TEST_MODE : can_17xx_40xx.h
- CAN_TFI_BITMASK : can_001.h
- CAN_TFI_DLC : can_001.h
- CAN_TFI_FF : can_001.h
- CAN_TFI_PRIO : can_001.h
- CAN_TFI_RTR : can_001.h
- CAN_TID_ID11 : can_001.h
- CAN_TID_ID29 : can_001.h
- CAN_TRANSMIT_PRIORITY_MODE : can_17xx_40xx.h
- CAN_TSR_BITMASK : can_001.h
- CAN_TSR_TBS : can_001.h
- CAN_TSR_TCS : can_001.h
- CAN_TSR_TS : can_001.h
- CAN_tx() : ccan_rom.c
- CAN_TX_MSG_EXT_ID : can.c
- CAN_TX_MSG_REMOTE_STD_ID : can.c
- CAN_TX_MSG_STD_ID : can.c
- CANAF_AFMR_ACCBP : can_001.h
- CANAF_AFMR_ACCOFF : can_001.h
- CANAF_AFMR_EFCAN : can_001.h
- CANAF_AFMR_OPERATION : can_001.h
- CANAF_ENDADDR : can_001.h
- CANAF_ENDADDR_VAL : can_001.h
- CANAF_FCAN_IC_INTPND : can_001.h
- CANAF_FCANIE : can_001.h
- CANAF_FCANIE_BITMASK : can_001.h
- CANAF_FULCAN_MSG_AF_FINISHED : can_001.h
- CANAF_FULCAN_MSG_AF_UPDATING : can_001.h
- CANAF_FULCAN_MSG_CPU_READING : can_001.h
- CANAF_FULLCAN_MSG_DLC_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_DLC_POS : can_001.h
- CANAF_FULLCAN_MSG_FF_POS : can_001.h
- CANAF_FULLCAN_MSG_ID11_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_ID11_POS : can_001.h
- CANAF_FULLCAN_MSG_LOST_POS : can_001.h
- CANAF_FULLCAN_MSG_RTR_POS : can_001.h
- CANAF_FULLCAN_MSG_SCC_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_SCC_POS : can_001.h
- CANAF_FULLCAN_MSG_SEM_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_SEM_POS : can_001.h
- CANAF_LUT_T : can_17xx_40xx.h
- CANAF_LUTERR : can_001.h
- CANAF_LUTERRAD : can_001.h
- CANAF_RAM_EFF_GRP_SEC : can_001.h
- CANAF_RAM_EFF_SEC : can_001.h
- CANAF_RAM_ENTRY_NUM : can_001.h
- CANAF_RAM_FULLCAN_SEC : can_001.h
- CANAF_RAM_SECTION : can_17xx_40xx.h
- CANAF_RAM_SECTION_NUM : can_001.h
- CANAF_RAM_SFF_GRP_SEC : can_001.h
- CANAF_RAM_SFF_SEC : can_001.h
- Capabilities : CDCClassCommon.h
- CARD_HANDLE_T : fsmci_cfg.h
- CARD_TYPE_4BIT : lpc_sdmmc.h
- CARD_TYPE_8BIT : lpc_sdmmc.h
- CARD_TYPE_HC : lpc_sdmmc.h
- CARD_TYPE_SD : lpc_sdmmc.h
- cardReset() : sdmmc_17xx_40xx.c
- CCAN_ARB : ccan_001.h
- CCAN_BASIC_TEST_MODE : ccan_001.h
- CCAN_CLRINTPND : ccan_001.h
- CCAN_CTRL : ccan_001.h
- CCAN_CTRL_CCE : ccan_001.h
- CCAN_CTRL_DAR : ccan_001.h
- CCAN_CTRL_EIE : ccan_001.h
- CCAN_CTRL_IE : ccan_001.h
- CCAN_CTRL_INIT : ccan_001.h
- CCAN_CTRL_SIE : ccan_001.h
- CCAN_CTRL_TEST : ccan_001.h
- CCAN_DATAA : ccan_001.h
- CCAN_DATAB : ccan_001.h
- CCAN_DLC : ccan_001.h
- CCAN_DLC_MASK : ccan_001.h
- CCAN_EOB : ccan_001.h
- CCAN_ERR_INT : ccan_001.h
- CCAN_ID_DIR : ccan_001.h
- CCAN_ID_EXT_MASK : ccan_001.h
- CCAN_ID_MTD : ccan_001.h
- CCAN_ID_MVAL : ccan_001.h
- CCAN_ID_STD_MASK : ccan_001.h
- CCAN_IF_Buf_transfer() : ccan_001.c
- CCAN_IF_Read : ccan_001.h
- CCAN_IF_Write : ccan_001.h
- CCAN_IFCREQ_BUSY : ccan_001.h
- CCAN_INTP : ccan_001.h
- CCAN_LOOPBACK_TEST_MODE : ccan_001.h
- CCAN_MASK : ccan_001.h
- CCAN_MASK_MDIR : ccan_001.h
- CCAN_MASK_MXTD : ccan_001.h
- CCAN_MLST : ccan_001.h
- CCAN_MODULE_INT : ccan_001.h
- CCAN_NEWD : ccan_001.h
- CCAN_NEWDAT : ccan_001.h
- CCAN_RD : ccan_001.h
- CCAN_RMTEN : ccan_001.h
- CCAN_RW : ccan_001.h
- CCAN_RX_DIR : ccan_001.h
- CCAN_RX_MODE : ccan_001.h
- CCAN_RX_MSG_ID : ccan.c
- CCAN_RXIE : ccan_001.h
- CCAN_SEG1_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_SEG2_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_SILENT_TEST_MODE : ccan_001.h
- CCAN_SJW_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_STAT_BOFF : ccan_001.h
- CCAN_STAT_EPASS : ccan_001.h
- CCAN_STAT_EWARN : ccan_001.h
- CCAN_STAT_LEC : ccan_001.h
- CCAN_STAT_RXOK : ccan_001.h
- CCAN_STAT_TXOK : ccan_001.h
- CCAN_STATUS_CHANGE_INT : ccan_001.h
- CCAN_STATUS_INT : ccan_001.h
- CCAN_TX_DIR : ccan_001.h
- CCAN_TX_MODE : ccan_001.h
- CCAN_TX_MSG_ID : ccan.c
- CCAN_TX_MSG_REMOTE_ID : ccan.c
- CCAN_TXIE : ccan_001.h
- CCAN_TXRQ : ccan_001.h
- CCAN_UMSK : ccan_001.h
- CCAN_WR : ccan_001.h
- CCEMTY_INT : HAL_LPC17xx.h
- ccu_clk_info : app_clock_apis.c
- CDC_ABSTRACT_CONTROL_MANAGEMENT : usbd_cdc.h
- CDC_ABSTRACT_CONTROL_MODEL : usbd_cdc.h
- CDC_ABSTRACT_STATE : usbd_cdc.h
- CDC_ACTIVATE_CARRIER : usbd_cdc.h
- CDC_ATM_NETWORKING : usbd_cdc.h
- CDC_ATM_NETWORKING_CONTROL_MODEL : usbd_cdc.h
- CDC_AUX_JACK_HOOK_STATE : usbd_cdc.h
- CDC_BRIDGE_TASK : VirtualSerial.c , VirtualSerial.h
- CDC_BUF_MASK : usbd_cdcuser.h
- CDC_BUF_SIZE : usbd_cdcuser.h
- CDC_CALL_MANAGEMENT : usbd_cdc.h
- CDC_CALL_STATE_CHANGE : usbd_cdc.h
- CDC_CAPI_CONTROL_MANAGEMENT : usbd_cdc.h
- CDC_CAPI_CONTROL_MODEL : usbd_cdc.h
- CDC_ClassNotifications_t : CDCClassCommon.h
- CDC_ClassRequests_t : CDCClassCommon.h
- CDC_CLEAR_COMM_FEATURE : usbd_cdc.h
- CDC_CLEAR_UNIT_PARAMETER : usbd_cdc.h
- CDC_COMMUNICATION_INTERFACE_CLASS : usbd_cdc.h
- CDC_CONNECTION_SPEED_CHANGE : usbd_cdc.h
- CDC_CONTROL_LINE_IN_BREAK : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_DCD : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_DSR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_FRAMEERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_OVERRUNERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_PARITYERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_RING : CDCClassCommon.h
- CDC_CONTROL_LINE_OUT_DTR : CDCClassCommon.h
- CDC_CONTROL_LINE_OUT_RTS : CDCClassCommon.h
- CDC_COUNTRY_SELECTION : usbd_cdc.h
- CDC_COUNTRY_SETTING : usbd_cdc.h
- CDC_CS_ENDPOINT : usbd_cdc.h
- CDC_CS_INTERFACE : usbd_cdc.h
- CDC_CSCP_ACMSubclass : CDCClassCommon.h
- CDC_CSCP_ATCommandProtocol : CDCClassCommon.h
- CDC_CSCP_CDCClass : CDCClassCommon.h
- CDC_CSCP_CDCDataClass : CDCClassCommon.h
- CDC_CSCP_NoDataProtocol : CDCClassCommon.h
- CDC_CSCP_NoDataSubclass : CDCClassCommon.h
- CDC_CSCP_NoSpecificProtocol : CDCClassCommon.h
- CDC_CSCP_NoSpecificSubclass : CDCClassCommon.h
- CDC_CSCP_VendorSpecificProtocol : CDCClassCommon.h
- CDC_DATA_INTERFACE_CLASS : usbd_cdc.h
- CDC_DATA_MULTPLEXED_STATE : usbd_cdc.h
- CDC_Descriptor_ClassSubclassProtocol_t : CDCClassCommon.h
- CDC_DescriptorSubtypes_t : CDCClassCommon.h
- CDC_Device_BytesReceived() : CDCClassDevice.h , CDCClassDevice.c
- CDC_Device_ConfigureEndpoints() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_CreateBlockingStream() : CDCClassDevice.h
- CDC_Device_CreateStream() : CDCClassDevice.h
- CDC_Device_Event_Stub() : CDCClassDevice.c
- CDC_Device_Event_Stub2() : CDCClassDevice.c
- CDC_Device_Flush() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_ProcessControlRequest() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_ReceiveByte() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendByte() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendControlLineStateChange() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendData() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendString() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_USBTask() : CDCClassDevice.c , CDCClassDevice.h
- CDC_DIAL_DIGITS : usbd_cdc.h
- CDC_DIRECT_LINE_CONTROL_MODEL : usbd_cdc.h
- CDC_DIRECT_LINE_MANAGEMENT : usbd_cdc.h
- CDC_DSUBTYPE_CSInterface_ACM : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ATM : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CallManagement : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CAPI : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CountrySelection : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_DirectLine : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Ethernet : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ExtensionUnit : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Header : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_MultiChannel : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_NetworkChannel : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ProtocolUnit : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneCall : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneOpModes : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneRinger : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Union : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_USBTerminal : CDCClassCommon.h
- CDC_DTE_PRESENT : usbd_cdc.h
- CDC_ENUMERROR_InvalidConfigDescriptor : CDCClassHost.h
- CDC_ENUMERROR_NoCompatibleInterfaceFound : CDCClassHost.h
- CDC_ENUMERROR_NoError : CDCClassHost.h
- CDC_ENUMERROR_PipeConfigurationFailed : CDCClassHost.h
- CDC_ETHERNET_NETWORKING : usbd_cdc.h
- CDC_ETHERNET_NETWORKING_CONTROL_MODEL : usbd_cdc.h
- CDC_EXTENSION_UNIT : usbd_cdc.h
- CDC_FUNCTIONAL_DESCRIPTOR : CDCClassCommon.h
- CDC_GET_ATM_DEVICE_STATISTICS : usbd_cdc.h
- CDC_GET_ATM_VC_STATISTICS : usbd_cdc.h
- CDC_GET_COMM_FEATURE : usbd_cdc.h
- CDC_GET_ENCAPSULATED_RESPONSE : usbd_cdc.h
- CDC_GET_ETHERNET_PMP_FILTER : usbd_cdc.h
- CDC_GET_ETHERNET_STATISTIC : usbd_cdc.h
- CDC_GET_LINE_CODING : usbd_cdc.h
- CDC_GET_LINE_PARMS : usbd_cdc.h
- CDC_GET_OPERATION_PARMS : usbd_cdc.h
- CDC_GET_PROFILE : usbd_cdc.h
- CDC_GET_RINGER_PARMS : usbd_cdc.h
- CDC_GET_UNIT_PARAMETER : usbd_cdc.h
- CDC_HEADER : usbd_cdc.h
- CDC_Host_BytesReceived() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_ConfigurePipes() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_CreateBlockingStream() : CDCClassHost.h
- CDC_Host_CreateStream() : CDCClassHost.h
- CDC_Host_EnumerationFailure_ErrorCodes_t : CDCClassHost.h
- CDC_Host_Event_Stub() : CDCClassHost.c
- CDC_Host_Flush() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_ReceiveByte() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendBreak() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendByte() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendControlLineStateChange() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendData() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendString() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SetLineEncoding() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_USBTask() : CDCClassHost.c , CDCClassHost.h
- CDC_IDLE_SETTING : usbd_cdc.h
- CDC_LINE_STATE_CHANGE : usbd_cdc.h
- CDC_LINEENCODING_OneAndAHalfStopBits : CDCClassCommon.h
- CDC_LINEENCODING_OneStopBit : CDCClassCommon.h
- CDC_LineEncoding_t : CDCClassCommon.h
- CDC_LINEENCODING_TwoStopBits : CDCClassCommon.h
- CDC_LineEncodingFormats_t : CDCClassCommon.h
- CDC_LineEncodingParity_t : CDCClassCommon.h
- CDC_MULTI_CHANNEL_CONTROL_MODEL : usbd_cdc.h
- CDC_MULTI_CHANNEL_MANAGEMENT : usbd_cdc.h
- CDC_NETWORK_CHANNEL : usbd_cdc.h
- CDC_NOTIF_SerialState : CDCClassCommon.h
- CDC_NOTIFICATION_EPNUM : Descriptors.h
- CDC_NOTIFICATION_EPSIZE : Descriptors.h
- CDC_NOTIFICATION_HEADER : usbd_cdc.h
- CDC_NOTIFICATION_NETWORK_CONNECTION : usbd_cdc.h
- CDC_NOTIFICATION_SERIAL_STATE : usbd_cdc.h
- CDC_PARITY_Even : CDCClassCommon.h
- CDC_PARITY_Mark : CDCClassCommon.h
- CDC_PARITY_None : CDCClassCommon.h
- CDC_PARITY_Odd : CDCClassCommon.h
- CDC_PARITY_Space : CDCClassCommon.h
- CDC_PROTOCOL_CAPI : usbd_cdc.h
- CDC_PROTOCOL_COMMON_AT_COMMANDS : usbd_cdc.h
- CDC_PROTOCOL_DESCRIBED_IN_PUFD : usbd_cdc.h
- CDC_PROTOCOL_EURO_ISDN : usbd_cdc.h
- CDC_PROTOCOL_HDLC : usbd_cdc.h
- CDC_PROTOCOL_HOST_BASED_DRIVER : usbd_cdc.h
- CDC_PROTOCOL_ISDN_BRI : usbd_cdc.h
- CDC_PROTOCOL_Q921_DATA_LINK : usbd_cdc.h
- CDC_PROTOCOL_Q921_MANAGEMENT : usbd_cdc.h
- CDC_PROTOCOL_Q921_MULTIPLEXOR : usbd_cdc.h
- CDC_PROTOCOL_TRANSPARENT : usbd_cdc.h
- CDC_PROTOCOL_UNIT : usbd_cdc.h
- CDC_PROTOCOL_V24_RATE_ADAPTATION : usbd_cdc.h
- CDC_PROTOCOL_V42 : usbd_cdc.h
- CDC_PULSE_SETUP : usbd_cdc.h
- CDC_REPORTING_CAPABILITIES : usbd_cdc.h
- CDC_REQ_GetEncapsulatedResponse : CDCClassCommon.h
- CDC_REQ_GetLineEncoding : CDCClassCommon.h
- CDC_REQ_SendBreak : CDCClassCommon.h
- CDC_REQ_SendEncapsulatedCommand : CDCClassCommon.h
- CDC_REQ_SetControlLineState : CDCClassCommon.h
- CDC_REQ_SetLineEncoding : CDCClassCommon.h
- CDC_RESPONSE_AVAILABLE : usbd_cdc.h
- CDC_RING_AUX_JACK : usbd_cdc.h
- CDC_RING_DETECT : usbd_cdc.h
- CDC_RX_EPNUM : Descriptors.h
- CDC_SEND_BREAK : usbd_cdc.h
- CDC_SEND_ENCAPSULATED_COMMAND : usbd_cdc.h
- CDC_SEND_PULSE : usbd_cdc.h
- CDC_SERIAL_STATE_BREAK : usbd_cdc.h
- CDC_SERIAL_STATE_FRAMING : usbd_cdc.h
- CDC_SERIAL_STATE_OVERRUN : usbd_cdc.h
- CDC_SERIAL_STATE_PARITY : usbd_cdc.h
- CDC_SERIAL_STATE_RING : usbd_cdc.h
- CDC_SERIAL_STATE_RX_CARRIER : usbd_cdc.h
- CDC_SERIAL_STATE_TX_CARRIER : usbd_cdc.h
- CDC_SET_ATM_DATA_FORMAT : usbd_cdc.h
- CDC_SET_ATM_DEFAULT_VC : usbd_cdc.h
- CDC_SET_AUX_LINE_STATE : usbd_cdc.h
- CDC_SET_COMM_FEATURE : usbd_cdc.h
- CDC_SET_CONTROL_LINE_STATE : usbd_cdc.h
- CDC_SET_ETHERNET_MULTICAST_FILTERS : usbd_cdc.h
- CDC_SET_ETHERNET_PACKET_FILTER : usbd_cdc.h
- CDC_SET_ETHERNET_PMP_FILTER : usbd_cdc.h
- CDC_SET_HOOK_STATE : usbd_cdc.h
- CDC_SET_LINE_CODING : usbd_cdc.h
- CDC_SET_LINE_PARMS : usbd_cdc.h
- CDC_SET_OPERATION_PARMS : usbd_cdc.h
- CDC_SET_PULSE_TIME : usbd_cdc.h
- CDC_SET_RINGER_PARMS : usbd_cdc.h
- CDC_SET_UNIT_PARAMETER : usbd_cdc.h
- CDC_TASK_SELECT : VirtualSerial.c
- CDC_TELEPHONE_CONTROL_MODEL : usbd_cdc.h
- CDC_TELEPHONE_OPERATIONAL_MODES : usbd_cdc.h
- CDC_TELEPHONE_RINGER : usbd_cdc.h
- CDC_TX_EPNUM : Descriptors.h
- CDC_TXRX_EPSIZE : Descriptors.h
- CDC_UNION : usbd_cdc.h
- CDC_USB_TERMINAL : usbd_cdc.h
- CDC_V1_10 : usbd_cdc.h
- CDCSpecification : CDCClassCommon.h
- CDFULL_INT : HAL_LPC17xx.h
- CENAF : pinint_8xx.h
- CENRL : pinint_8xx.h
- CGU_AUDIO_PLL : cguccu_18xx_43xx.h
- CGU_AUDIO_PLL_RATE : sys_config.h
- CGU_IRC_FREQ : clock_18xx_43xx.h
- CGU_PLL_FR : clock_18xx_43xx.h
- CGU_PLL_LOCKED : clock_18xx_43xx.h
- CGU_USB_PLL : cguccu_18xx_43xx.h
- CGU_USB_PLL_RATE : sys_config.h
- ch_no : gpdma_speed_test.c
- ChangeAFLUT() : can.c
- ChannelConfig : AudioClassCommon.h
- ChannelControls : AudioClassCommon.h
- ChannelHandlerArray : gpdma_17xx_40xx.c , gpdma_18xx_43xx.c
- Channels : AudioClassCommon.h
- ChannelStrIndex : AudioClassCommon.h
- channelTC : adc.c , dac.c , i2s.c , uart.c , adc.c , dac.c , i2s.c , uart.c
- channelTCErr : uart.c
- CHAR : lpc_types.h
- CharFormat : CDCClassCommon.h
- check_fs() : ff.c
- checkBadBlock() : nandflash.c
- checkMagicHeader() : dfuutil_programming_dfu_ops.c
- checkR1Response() : sdmmc_17xx_40xx.c
- Checks : DataflashManager.h
- CHECKSUM_CHECK_IP : lwipopts.h
- CHECKSUM_CHECK_TCP : lwipopts.h
- CHECKSUM_CHECK_UDP : lwipopts.h
- CHECKSUM_GEN_IP : lwipopts.h
- CHECKSUM_GEN_TCP : lwipopts.h
- CHECKSUM_GEN_UDP : lwipopts.h
- Chip_ACMP_Deinit() : acmp_8xx.c , acmp_8xx.h
- Chip_ACMP_DisableSyncCompOut() : acmp_8xx.h
- Chip_ACMP_DisableVoltLadder() : acmp_8xx.h
- Chip_ACMP_EdgeClear() : acmp_8xx.h
- Chip_ACMP_EnableSyncCompOut() : acmp_8xx.h
- Chip_ACMP_EnableVoltLadder() : acmp_8xx.h
- Chip_ACMP_GetCompStatus() : acmp_8xx.h
- Chip_ACMP_Init() : acmp_8xx.c , acmp_8xx.h
- CHIP_ACMP_NEG_INPUT_T : acmp_8xx.h
- CHIP_ACMP_POS_INPUT_T : acmp_8xx.h
- Chip_ACMP_SetEdgeSelection() : acmp_8xx.h
- Chip_ACMP_SetHysteresis() : acmp_8xx.h
- Chip_ACMP_SetNegVoltRef() : acmp_8xx.h
- Chip_ACMP_SetPosVoltRef() : acmp_8xx.h
- Chip_ACMP_SetupAMCPRefs() : acmp_8xx.h
- Chip_ACMP_SetupVoltLadder() : acmp_8xx.h
- Chip_ADC_Burst_Cmd() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Channel_Enable_Cmd() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Channel_Int_Cmd() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- CHIP_ADC_CHANNEL_T : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_DeInit() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- CHIP_ADC_EDGE_CFG_T : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_GetClk() : adc_18xx_43xx.c
- Chip_ADC_Global_Int_Cmd() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_Init() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Read_Byte() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Read_Status() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_Read_Value() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- CHIP_ADC_RESOLUTION_T : adc_11xx.h , adc_13xx.h , adc_18xx_43xx.h
- Chip_ADC_Set_Resolution() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Set_SampleRate() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Set_StartMode() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- CHIP_ADC_START_MODE_T : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- CHIP_AES_API_CMD_DECODE_CBC : aes_18xx_43xx.h
- CHIP_AES_API_CMD_DECODE_ECB : aes_18xx_43xx.h
- CHIP_AES_API_CMD_ENCODE_CBC : aes_18xx_43xx.h
- CHIP_AES_API_CMD_ENCODE_ECB : aes_18xx_43xx.h
- Chip_AES_Init() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadIV_IC() : aes_18xx_43xx.h , aes_18xx_43xx.c
- Chip_AES_LoadIV_SW() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKey() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKeyRNG() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKeySW() : aes_18xx_43xx.c , aes_18xx_43xx.h
- CHIP_AES_OP_MODE_T : aes_18xx_43xx.h
- Chip_AES_Operate() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_ProgramKey() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_SetMode() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_ATIMER_ClearIntStatus() : atimer_18xx_43xx.h
- Chip_ATIMER_DeInit() : atimer_18xx_43xx.h
- Chip_ATIMER_GetPresetValue() : atimer_18xx_43xx.h
- Chip_ATIMER_Init() : atimer_18xx_43xx.c , atimer_18xx_43xx.h
- Chip_ATIMER_IntDisable() : atimer_18xx_43xx.h
- Chip_ATIMER_IntEnable() : atimer_18xx_43xx.h
- Chip_ATIMER_SetIntStatus() : atimer_18xx_43xx.h
- Chip_ATIMER_UpdatePresetValue() : atimer_18xx_43xx.h
- CHIP_CAN_AF_MODE_T : can_17xx_40xx.h
- Chip_CAN_DeInit() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_DetermineClk() : can_17xx_40xx.c
- Chip_CAN_DetermineReset() : can_17xx_40xx.c
- Chip_CAN_FullCANIntConfig() : can_17xx_40xx.h
- Chip_CAN_FullCANReceive() : can_17xx_40xx.h
- Chip_CAN_GetClockRate() : can_17xx_40xx.c
- Chip_CAN_GetEntriesNum() : can_17xx_40xx.h
- Chip_CAN_GetFreeTxBuf() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_GetFullCANIntStatus() : can_17xx_40xx.h
- Chip_CAN_GetIntStatus() : can_17xx_40xx.h
- Chip_CAN_GetStatus() : can_17xx_40xx.h
- Chip_CAN_Init() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_InsertFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_InsertGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_InsertGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_InsertIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_InsertIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_IntDisable() : can_17xx_40xx.h
- Chip_CAN_IntEnable() : can_17xx_40xx.h
- CHIP_CAN_MODE_T : can_17xx_40xx.h
- Chip_CAN_ReadFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_ReadGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_ReadGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_ReadIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_ReadIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_Receive() : can_17xx_40xx.h
- Chip_CAN_RemoveFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_Send() : can_17xx_40xx.h
- Chip_CAN_SetAFLUT() : can_17xx_40xx.h
- Chip_CAN_SetAFMode() : can_17xx_40xx.h
- Chip_CAN_SetBitRate() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_SetMode() : can_17xx_40xx.h
- Chip_CCAN_AddReceiveID() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_ClearIntPend() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_ClearStatus() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_DeInit() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_DeleteReceiveID() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- CHIP_CCAN_DETERMINECLK : ccan_18xx_43xx.c
- Chip_CCAN_GetIntID() : ccan_18xx_43xx.h
- Chip_CCAN_GetMsgObject() : ccan_18xx_43xx.h
- Chip_CCAN_GetStatus() : ccan_18xx_43xx.h
- Chip_CCAN_Init() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_IntEnable() : ccan_18xx_43xx.h
- Chip_CCAN_Send() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_SetBitRate() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- CHIP_CCU_CLK_T : chip_clocks.h
- CHIP_CGU_BASE_CLK_T : chip_clocks.h
- CHIP_CGU_CLKIN_T : chip_clocks.h
- CHIP_CGU_IDIV_T : chip_clocks.h
- CHIP_CGU_USB_AUDIO_PLL_T : cguccu_18xx_43xx.h
- Chip_Clock_ClearPowerDown() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_Disable() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableCLKOUT() : clock_17xx_40xx.h
- Chip_Clock_DisableCrystal() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableMainPLL() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisablePeriphClock() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_DisablePLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_Enable() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableCLKOUT() : clock_17xx_40xx.h
- Chip_Clock_EnableCrystal() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableMainPLL() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableOpts() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnablePeriphClock() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_EnablePLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_FeedPLL() : clock_17xx_40xx.h
- Chip_Clock_FindBaseClock() : clock_18xx_43xx.c
- Chip_Clock_GetBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetBaseClockOpts() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetBaseClocktHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetClockInputHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetCPUClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetCPUClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetDividerDivisor() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetDividerSource() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetDivRate() : clock_18xx_43xx.c
- Chip_Clock_GetEMCClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetEMCClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetENETClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetExtClockInRate() : clock_8xx.h
- Chip_Clock_GetGPDMAClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetIntOscRate() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_GetLCDClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetMainClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetMainClockSource() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_GetMainOscRate() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_GetMainPLLHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetMainPllInClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetMainPllOutClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetMainPllSource() : clock_17xx_40xx.h
- Chip_Clock_GetPCLKDiv() : clock_17xx_40xx.h
- Chip_Clock_GetPeripheralClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetPllFreq() : clock_11xx.c , clock_13xx.c , clock_8xx.c
- Chip_Clock_GetPLLStatus() : clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetRate() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetRTCClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetRTCOscRate() : clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockSource() : clock_17xx_40xx.h
- Chip_Clock_GetSSP0ClockDiv() : clock_11xx.h , clock_13xx.h
- Chip_Clock_GetSSP1ClockDiv() : clock_13xx.h
- Chip_Clock_GetSYSCLKRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetSystemClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetSystemPllInClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetSystemPllOutClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetSystickClockDiv() : clock_13xx.h
- Chip_Clock_GetTraceClockDiv() : clock_13xx.h
- Chip_Clock_GetUARTClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_GetUSBClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetUSBClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetUSBClockSource() : clock_17xx_40xx.h
- Chip_Clock_GetUSBPllInClockRate() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.h
- Chip_Clock_GetUSBPllOutClockRate() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetWDTLFORate() : clock_11xx.c , clock_13xx.c , clock_8xx.c
- Chip_Clock_GetWDTOSCRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_IsBaseClockEnabled() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_IsCLKOUTEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsMainPLLEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsMainPLLLocked() : clock_17xx_40xx.h
- Chip_Clock_IsPeripheralClockEnabled() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_IsSystemPLLLocked() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_IsUSBPLLEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsUSBPLLLocked() : clock_13xx.h , clock_17xx_40xx.h
- Chip_Clock_MainPLLLocked() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetCLKOUTSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetCPUClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetCPUClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetDivider() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetEMCClockDiv() : clock_17xx_40xx.h
- Chip_Clock_SetLCDClockDiv() : clock_17xx_40xx.h
- Chip_Clock_SetMainClockSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetMainPllSource() : clock_17xx_40xx.h
- Chip_Clock_SetPCLKDiv() : clock_17xx_40xx.h
- Chip_Clock_SetPLLBypass() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetSPIFIClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetSPIFIClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetSSP0ClockDiv() : clock_11xx.h , clock_13xx.h
- Chip_Clock_SetSSP1ClockDiv() : clock_13xx.h
- Chip_Clock_SetSysClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetSystemPllSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetSystickClockDiv() : clock_13xx.h
- Chip_Clock_SetTraceClockDiv() : clock_13xx.h
- Chip_Clock_SetUARTClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetupMainPLLHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupMainPLLMult() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupPLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupSystemPLL() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetupUSBPLL() : clock_13xx.h
- Chip_Clock_SetUSBClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetUSBClockSource() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetUSBPllSource() : clock_13xx.c , clock_13xx.h
- Chip_Clock_SetWDTOSC() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_StartPowerDown() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_TestMainPLLMultiplier() : clock_18xx_43xx.c
- Chip_CRC_CRC16() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_CRC32() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_CRC8() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_Deinit() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_GetMode() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_GetSeed() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Init() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetMode() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetPoly() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetSeed() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Sum() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_UseDefaultConfig() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write16() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write32() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write8() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CREG_ConfigureBODaR() : creg_18xx_43xx.h
- Chip_CREG_EnableUSB0Phy() : creg_18xx_43xx.h
- Chip_CREG_OnChipFlashIsPresent() : creg_18xx_43xx.h
- Chip_CREG_SetFlashAcceleration() : creg_18xx_43xx.h
- Chip_DAC_ConfigDAConverterControl() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_DeInit() : dac_17xx_40xx.h , dac_18xx_43xx.c , dac_18xx_43xx.h
- Chip_DAC_GetIntStatus() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_Init() : dac_17xx_40xx.c , dac_17xx_40xx.h , dac_18xx_43xx.c , dac_18xx_43xx.h
- Chip_DAC_SetBias() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_SetDMATimeOut() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_UpdateValue() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DMA_GetFreeChannel() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_InitChannelCfg() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Interrupt() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_PrepareDescriptor() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_SGTransfer() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Stop() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Transfer() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_EEPROM_ClearIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DeInit() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DisableInt() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DisablePowerDown() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_EnableInt() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_EnablePowerDown() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_Erase() : eeprom_17xx_40xx.h
- Chip_EEPROM_EraseProgramPage() : eeprom_18xx_43xx.h
- Chip_EEPROM_GetIntEnable() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_GetIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_Init() : eeprom_17xx_40xx.c , eeprom_17xx_40xx.h , eeprom_18xx_43xx.c , eeprom_18xx_43xx.h
- Chip_EEPROM_Read() : eeprom_17xx_40xx.h
- Chip_EEPROM_SetAutoProg() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetCmd() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_SetReadWaitState() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetWaitState() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_WaitForIntStatus() : eeprom_18xx_43xx.h
- Chip_EEPROM_Write() : eeprom_17xx_40xx.h
- Chip_EMC_Dynamic_Enable() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Dynamic_Init() : emc_17xx_40xx.c , emc_17xx_40xx.h , emc_18xx_43xx.c , emc_18xx_43xx.h
- Chip_EMC_Enable() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Init() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_LowPowerMode() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Mirror() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_SetStaticExtendedWait() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Static_Init() : emc_17xx_40xx.c , emc_17xx_40xx.h , emc_18xx_43xx.c , emc_18xx_43xx.h
- Chip_ENET_ClearIntStatus() : enet_17xx_40xx.h
- Chip_ENET_DeInit() : enet_17xx_40xx.c , enet_17xx_40xx.h , enet_18xx_43xx.c , enet_18xx_43xx.h
- Chip_ENET_DisableInt() : enet_17xx_40xx.h
- Chip_ENET_DisableRXFilter() : enet_17xx_40xx.h
- Chip_ENET_EnableInt() : enet_17xx_40xx.h
- Chip_ENET_EnableRXFilter() : enet_17xx_40xx.h
- Chip_ENET_FindMIIDiv() : enet_17xx_40xx.c , enet_17xx_40xx.h
- Chip_ENET_GetBufferStatus() : enet_17xx_40xx.h
- Chip_ENET_GetFillDescNum() : enet_17xx_40xx.h
- Chip_ENET_GetFreeDescNum() : enet_17xx_40xx.h
- Chip_ENET_GetIntStatus() : enet_17xx_40xx.h
- Chip_ENET_GetRXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_GetRXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_GetTXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_GetTXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_IncRXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_IncTXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_Init() : enet_17xx_40xx.c , enet_17xx_40xx.h , enet_18xx_43xx.c , enet_18xx_43xx.h
- Chip_ENET_InitDescriptors() : enet_18xx_43xx.h
- Chip_ENET_InitRxDescriptors() : enet_17xx_40xx.h
- Chip_ENET_InitTxDescriptors() : enet_17xx_40xx.h
- Chip_ENET_IsMIIBusy() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_IsRxEmpty() : enet_17xx_40xx.h
- Chip_ENET_IsTxFull() : enet_17xx_40xx.h
- Chip_ENET_ReadMIIData() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_Reset() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_ResetRXLogic() : enet_17xx_40xx.h
- Chip_ENET_ResetTXLogic() : enet_17xx_40xx.h
- Chip_ENET_RXDisable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_RXEnable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_RXStart() : enet_18xx_43xx.h
- Chip_ENET_Set100Mbps() : enet_17xx_40xx.h
- Chip_ENET_Set10Mbps() : enet_17xx_40xx.h
- Chip_ENET_SetADDR() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_SetDuplex() : enet_18xx_43xx.h
- Chip_ENET_SetFullDuplex() : enet_17xx_40xx.h
- Chip_ENET_SetHalfDuplex() : enet_17xx_40xx.h
- Chip_ENET_SetSpeed() : enet_18xx_43xx.h
- Chip_ENET_SetupMII() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_StartMIIRead() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_StartMIIWrite() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXDisable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXEnable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXStart() : enet_18xx_43xx.h
- Chip_EVRT_ClrPendIntSrc() : evrt_18xx_43xx.h
- Chip_EVRT_ConfigIntSrcActiveType() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_DeInit() : evrt_18xx_43xx.h
- Chip_EVRT_Init() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_IsSourceInterrupting() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_SetUpIntSrc() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- CHIP_EVRT_SRC_ACTIVE_T : evrt_18xx_43xx.h
- CHIP_EVRT_SRC_T : evrt_18xx_43xx.h
- Chip_FIO_ClearValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FIO_ReadValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FIO_SetDir() : gpio_18xx_43xx.h
- Chip_FIO_SetValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FMC_SetFLASHAccess() : fmc_11xx.h , fmc_13xx.h , fmc_17xx_40xx.h , fmc_8xx.h
- Chip_GPDMA_ChannelCmd() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPDMA_ClearIntPending() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPDMA_DeInit() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_GPDMA_Init() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_GPDMA_IntGetStatus() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPIO_ClearValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_Init() : gpio_11xx.c , gpio_11xx.h , gpio_13xx.c , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_IntClear() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_IntCmd() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_IntGetStatus() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_ReadDirBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_ReadPortBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_ReadValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_SetDir() : gpio_11xx.c , gpio_11xx.h , gpio_13xx.c , gpio_13xx.h , gpio_18xx_43xx.c , gpio_18xx_43xx.h , gpio_8xx.c , gpio_8xx.h
- Chip_GPIO_SetValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_WriteDirBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_WritePortBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIOGP_IntClear() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntGetStatus() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntInit() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntPinAdd() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntPinRemove() : gpio_18xx_43xx.h
- Chip_I2C_DeInit() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_Disable() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_EventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_EventHandlerPolling() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_GetClockRate() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_GetMasterEventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_Init() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h , i2c_8xx.c , i2c_8xx.h
- Chip_I2C_IsMasterActive() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_IsStateChanged() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterCmdRead() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterRead() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterSend() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterStateHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterTransfer() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- CHIP_I2C_MODE_T : i2cd_8xx.h
- Chip_I2C_SetClockRate() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SetMasterEventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SlaveSetup() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SlaveStateHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2S_Config() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_DeInit() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_DisableMute() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_DMA_Cmd() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_EnableMute() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_GetLevel() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Init() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_Int_Cmd() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_ModeConfig() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Pause() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Receive() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Send() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Start() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Stop() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_IOCON_Init() : iocon_17xx_40xx.h
- CHIP_IOCON_PIN_LOC_T : iocon_11xx.h , iocon_13xx.h
- Chip_IOCON_PinLocSel() : iocon_11xx.h , iocon_13xx.h
- Chip_IOCON_PinMux() : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h
- Chip_IOCON_PinMuxSet() : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h
- Chip_IOCON_PinSetClockDivisor() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetHysteresis() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetI2CMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetInputInverted() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetOpenDrainMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetSampleMode() : iocon_8xx.c , iocon_8xx.h
- CHIP_IOCON_PIO_T : iocon_11xx.h , iocon_13xx.h
- Chip_LCD_ClearInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Config() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Disable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Enable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_LoadPalette0() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_LoadPalette1() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_SetClip() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_SetPos() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_WriteImage() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_DeInit() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_Disable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_DisableInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Enable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_EnableInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Init() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_LoadPalette() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_PowerOff() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_PowerOn() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_SetLPFrameBuffer() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_SetUPFrameBuffer() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- CHIP_LPC11CXX : sys_config.h
- CHIP_LPC11UXX : sys_config.h
- CHIP_LPC1347 : sys_config.h
- CHIP_LPC175X_6X : sys_config.h
- CHIP_LPC177X_8X : sys_config.h
- CHIP_LPC18XX : sys_config.h
- CHIP_LPC407X_8X : sys_config.h
- CHIP_LPC43XX : sys_config.h
- CHIP_LPC8XX : sys_config.h
- Chip_MRT_DeInit() : mrt_8xx.h
- Chip_MRT_GetEnabled() : mrt_8xx.h
- Chip_MRT_GetIdleChannel() : mrt_8xx.h
- Chip_MRT_GetInterval() : mrt_8xx.h
- Chip_MRT_GetIntPending() : mrt_8xx.h
- Chip_MRT_GetMode() : mrt_8xx.h
- Chip_MRT_GetTimer() : mrt_8xx.h
- Chip_MRT_Init() : mrt_8xx.h
- Chip_MRT_IntClear() : mrt_8xx.h
- Chip_MRT_IntPending() : mrt_8xx.h
- Chip_MRT_IsOneShotMode() : mrt_8xx.h
- Chip_MRT_IsRepeatMode() : mrt_8xx.h
- Chip_MRT_Running() : mrt_8xx.h
- Chip_MRT_SetEnabled() : mrt_8xx.h
- Chip_MRT_SetInterval() : mrt_8xx.h
- Chip_MRT_SetMode() : mrt_8xx.h
- CHIP_OTP_BOOT_SRC_T : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC16 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC32 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC8 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_PINS : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_SPI : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_SPIFI : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_UART0 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_UART3 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_USB0 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_USB1 : otp_18xx_43xx.h
- Chip_OTP_GenRand() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_Init() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgBootSrc() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgGPWord() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgJTAGDis() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgKey() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgUSBID() : otp_18xx_43xx.c , otp_18xx_43xx.h
- CHIP_PIN_CLKDIV_T : iocon_8xx.h
- CHIP_PIN_DIR_T : gpio_8xx.h
- CHIP_PIN_I2CMODE_T : iocon_8xx.h
- CHIP_PIN_MODE_T : iocon_8xx.h
- CHIP_PIN_SMODE_T : iocon_8xx.h
- Chip_PININT_Config() : pinint_8xx.c , pinint_8xx.h
- CHIP_PINT_CFG_T : pinint_8xx.h
- CHIP_PINx_T : iocon_8xx.h
- CHIP_PMC_PWR_STATE_T : pmc_18xx_43xx.h
- Chip_PMC_Set_PwrState() : pmc_18xx_43xx.c , pmc_18xx_43xx.h
- Chip_PMC_Sleep() : pmc_18xx_43xx.c , pmc_18xx_43xx.h
- CHIP_PMI_PIN_T : pinint_8xx.h
- Chip_PMU_GetData() : pmu_11xx.h
- CHIP_PMU_MCUPOWER_T : pmu_8xx.h
- Chip_PMU_SetMode() : pmu_11xx.h
- Chip_PMU_Sleep() : pmu_8xx.c , pmu_8xx.h
- Chip_REGFILE_Read() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_REGFILE_Write() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RGU_ClearReset() : rgu_18xx_43xx.c , rgu_18xx_43xx.h
- Chip_RGU_InReset() : rgu_18xx_43xx.c , rgu_18xx_43xx.h
- CHIP_RGU_RST_T : rgu_18xx_43xx.h
- Chip_RGU_TriggerReset() : rgu_18xx_43xx.c , rgu_18xx_43xx.h
- Chip_RIT_ClearInt() : ritimer_18xx_43xx.h
- Chip_RIT_DeInit() : ritimer_18xx_43xx.c , ritimer_18xx_43xx.h
- Chip_RIT_Disable() : ritimer_18xx_43xx.h
- Chip_RIT_Enable() : ritimer_18xx_43xx.h
- Chip_RIT_EnableCTRL() : ritimer_18xx_43xx.h
- Chip_RIT_GetCounter() : ritimer_18xx_43xx.h
- Chip_RIT_GetIntStatus() : ritimer_18xx_43xx.h
- Chip_RIT_Init() : ritimer_18xx_43xx.c , ritimer_18xx_43xx.h
- Chip_RIT_SetCOMPVAL() : ritimer_18xx_43xx.h
- Chip_RIT_SetTimerInterval() : ritimer_18xx_43xx.c , ritimer_18xx_43xx.h
- Chip_RIT_TimerDebugDisable() : ritimer_18xx_43xx.h
- Chip_RIT_TimerDebugEnable() : ritimer_18xx_43xx.h
- Chip_RTC_AlarmIntConfig() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_CalibConfig() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_CalibCounterCmd() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_ClearIntPending() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_CntIncrIntConfig() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_DeInit() : rtc_17xx_40xx.c , rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_Enable() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetFullAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetFullTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetIntPending() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetTime() : rtc_18xx_43xx.h , rtc_17xx_40xx.h
- Chip_RTC_Init() : rtc_17xx_40xx.c , rtc_17xx_40xx.h , rtc_18xx_43xx.c , rtc_18xx_43xx.h
- Chip_RTC_ResetClockTickCounter() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetFullAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetFullTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_SCT_ClearEventFlag() : sct_8xx.h
- Chip_SCT_Config() : sct_18xx_43xx.h , sct_8xx.h
- Chip_SCT_ConflictResolutionSet() : sct_18xx_43xx.h
- Chip_SCT_ControlSetClr() : sct_18xx_43xx.h
- Chip_SCT_DeInit() : sct_18xx_43xx.c , sct_18xx_43xx.h , sct_8xx.c , sct_8xx.h
- CHIP_SCT_EVENT_T : sct_8xx.h
- Chip_SCT_EventFlagClear() : sct_18xx_43xx.h
- Chip_SCT_EventIntDisable() : sct_8xx.h
- Chip_SCT_EventIntEnable() : sct_8xx.h
- Chip_SCT_Init() : sct_18xx_43xx.c , sct_18xx_43xx.h , sct_8xx.c , sct_8xx.h
- CHIP_SCT_MATCH_REG_T : sct_8xx.h
- Chip_SCT_SetCount() : sct_8xx.h
- Chip_SCT_SetCountH() : sct_8xx.h
- Chip_SCT_SetCountL() : sct_8xx.h
- Chip_SCT_SetMatchCount() : sct_8xx.h
- Chip_SCT_SetMatchReload() : sct_8xx.h
- Chip_SCU_ADC_Channel_Config() : scu_18xx_43xx.h
- Chip_SCU_ClockPinMux() : scu_18xx_43xx.h
- Chip_SCU_ClockPinMuxSet() : scu_18xx_43xx.h
- Chip_SCU_DAC_Analog_Config() : scu_18xx_43xx.h
- Chip_SCU_GPIOIntPinSel() : scu_18xx_43xx.c , scu_18xx_43xx.h
- Chip_SCU_I2C0PinConfig() : scu_18xx_43xx.h
- Chip_SCU_PinMux() : scu_18xx_43xx.h
- Chip_SCU_PinMuxSet() : scu_18xx_43xx.h
- Chip_SDC_DeInit() : sdc_17xx_40xx.c , sdc_17xx_40xx.h
- Chip_SDC_GetStatus() : sdc_17xx_40xx.h
- Chip_SDC_Init() : sdc_17xx_40xx.c , sdc_17xx_40xx.h
- CHIP_SDC_RET_CODE_T : sdc_17xx_40xx.h
- Chip_SDC_SetClock() : sdc_17xx_40xx.c , sdc_17xx_40xx.h
- Chip_SDC_SetIntMask() : sdc_17xx_40xx.h
- Chip_SDIF_CardNDetect() : sdif_18xx_43xx.h
- Chip_SDIF_CardWpOn() : sdif_18xx_43xx.h
- Chip_SDIF_DeInit() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_GetIntStatus() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_Init() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_PowerOff() : sdif_18xx_43xx.h
- Chip_SDIF_PowerOn() : sdif_18xx_43xx.h
- Chip_SDIF_SetIntMask() : sdif_18xx_43xx.h
- Chip_SDMMC_Acquire() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_FIFOIRQHandler() : sdmmc_17xx_40xx.c
- Chip_SDMMC_GetCardState() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetCardStatus() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetDeviceBlocks() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_GetDeviceSize() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_GetSDStatus() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetState() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_IRQHandler() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_ReadBlocks() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_WriteBlocks() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- CHIP_SPI_BITS_T : spi_17xx_40xx.h
- Chip_SPI_CalClkRateDivider() : spi_8xx.c , spi_8xx.h
- CHIP_SPI_CALLBACK_T : spi_17xx_40xx.h
- CHIP_SPI_CLOCK_MODE_T : spi_17xx_40xx.h
- CHIP_SPI_DATA_ORDER_T : spi_17xx_40xx.h
- Chip_SPI_DeInit() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPI_DelayConfig() : spi_8xx.h
- Chip_SPI_Disable() : spi_8xx.h
- Chip_SPI_DisableLoopBack() : spi_8xx.h
- Chip_SPI_Enable() : spi_8xx.h
- Chip_SPI_EnableLoopBack() : spi_8xx.h
- Chip_SPI_GetStatus() : spi_17xx_40xx.h , spi_8xx.h
- Chip_SPI_Init() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPI_Int_Cmd() : spi_8xx.c , spi_8xx.h
- Chip_SPI_Int_Disable() : spi_17xx_40xx.h
- Chip_SPI_Int_Enable() : spi_17xx_40xx.h
- Chip_SPI_Int_FlushData() : spi_17xx_40xx.h
- Chip_SPI_Int_RWFrames() : spi_8xx.c , spi_8xx.h
- Chip_SPI_Int_RWFrames16Bits() : spi_17xx_40xx.h
- Chip_SPI_Int_RWFrames8Bits() : spi_17xx_40xx.h
- CHIP_SPI_MODE_T : spi_17xx_40xx.h
- Chip_SPI_ReadFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPI_ReceiveFrame() : spi_8xx.h
- Chip_SPI_RWFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPI_SendFirstFrame() : spi_8xx.h
- Chip_SPI_SendFirstFrame_RxIgnore() : spi_8xx.h
- Chip_SPI_SendLastFrame() : spi_8xx.h
- Chip_SPI_SendLastFrame_RxIgnore() : spi_8xx.h
- Chip_SPI_SendMidFrame() : spi_8xx.h
- Chip_SPI_SetBitRate() : spi_17xx_40xx.h
- Chip_SPI_SetFormat() : spi_17xx_40xx.h
- Chip_SPI_SetMode() : spi_17xx_40xx.h
- Chip_SPI_WriteFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPIFI_DeInit() : spifi_17xx_40xx.h
- Chip_SPIFI_Init() : spifi_17xx_40xx.h
- CHIP_SSP_BITS_T : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- CHIP_SSP_CLOCK_MODE_T : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_DeInit() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_DetermineClk() : ssp_17xx_40xx.c
- Chip_SSP_Disable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_DisableLoopBack() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_DMA_Disable() : ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_DMA_Enable() : ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Enable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_EnableLoopBack() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- CHIP_SSP_FRAME_FORMAT_T : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- CHIP_SSP_FRAME_FORMAT_TI : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_GetClockRate() : ssp_17xx_40xx.c
- Chip_SSP_GetStatus() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Init() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_Int_Disable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Int_Enable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Int_FlushData() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_Int_RWFrames16Bits() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_Int_RWFrames8Bits() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- CHIP_SSP_MODE_T : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_ReadFrames_Blocking() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_RWFrames_Blocking() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_SetBitRate() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_SetFormat() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_SetMaster() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_WriteFrames_Blocking() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SWM_Deinit() : swm_8xx.h
- Chip_SWM_FixedPinEnable() : swm_8xx.c , swm_8xx.h
- Chip_SWM_Init() : swm_8xx.h
- Chip_SWM_IsEnabled() : swm_8xx.c , swm_8xx.h
- Chip_SWM_MovablePinAssign() : swm_8xx.c , swm_8xx.h
- CHIP_SWM_PIN_FIXED_T : swm_8xx.h
- CHIP_SWM_PIN_MOVABLE_T : swm_8xx.h
- Chip_SYSCTL_AssertPeriphReset() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- CHIP_SYSCTL_BODRINTVAL_T : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- CHIP_SYSCTL_BODRSTLVL_T : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- CHIP_SYSCTL_BOOT_MODE_REMAP_T : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- CHIP_SYSCTL_CCLKSRC_T : clock_17xx_40xx.h
- Chip_SYSCTL_ClearSystemRSTStatus() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- CHIP_SYSCTL_CLKOUTSRC_T : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- CHIP_SYSCTL_CLOCK_T : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_SYSCTL_DeassertPeriphReset() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_DisableBOD() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableBODReset() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- Chip_SYSCTL_DisableBODRPM() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableBoost() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableNMISource() : syscon_8xx.h
- Chip_SYSCTL_DisablePeriphWakeup() : syscon_8xx.h
- Chip_SYSCTL_DisablePINTWakeup() : syscon_8xx.h
- Chip_SYSCTL_DisableStartPin() : sysctl_13xx.h
- CHIP_SYSCTL_EMC_DIV_T : clock_17xx_40xx.h
- Chip_SYSCTL_EnableBOD() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableBODReset() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- Chip_SYSCTL_EnableBODRPM() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableBoost() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableNMISource() : syscon_8xx.h
- Chip_SYSCTL_EnablePeriphWakeup() : syscon_8xx.h
- Chip_SYSCTL_EnablePINTWakeuup() : syscon_8xx.h
- Chip_SYSCTL_EnableStartPin() : sysctl_13xx.h
- Chip_SYSCTL_GetClrSleepFlags() : sysctl_17xx_40xx.c , sysctl_17xx_40xx.h
- Chip_SYSCTL_GetDeepSleepPD() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_GetDeviceID() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_GetIRQLatency() : syscon_8xx.h
- Chip_SYSCTL_GetPORPIOStatus() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_GetPowerStates() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_GetStartPinStatus() : sysctl_13xx.h
- Chip_SYSCTL_GetSystemRSTStatus() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- Chip_SYSCTL_GetUSARTFRGDivider() : syscon_8xx.h
- Chip_SYSCTL_GetUSARTFRGMultiplier() : syscon_8xx.h
- Chip_SYSCTL_GetWakeup() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- CHIP_SYSCTL_MAINCLKSRC_T : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_SYSCTL_Map() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- CHIP_SYSCTL_PERIPH_RESET_T : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_PeriphReset() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.c , sysctl_17xx_40xx.h , syscon_8xx.h
- CHIP_SYSCTL_PLL_T : sysctl_17xx_40xx.h
- CHIP_SYSCTL_PLLCLKSRC_T : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_SYSCTL_PowerDown() : sysctl_11xx.c , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , syscon_8xx.h
- Chip_SYSCTL_PowerUp() : sysctl_11xx.c , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , syscon_8xx.h
- CHIP_SYSCTL_RESET_T : sysctl_17xx_40xx.h
- Chip_SYSCTL_ResetStartPin() : sysctl_13xx.h
- Chip_SYSCTL_SetBODLevels() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_SetDeepSleepPD() : sysctl_11xx.c , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , syscon_8xx.h
- Chip_SYSCTL_SetIRQLatency() : syscon_8xx.h
- Chip_SYSCTL_SetNMISource() : syscon_8xx.h
- Chip_SYSCTL_SetPinInterrupt() : syscon_8xx.h
- Chip_SYSCTL_SetStartPinFalling() : sysctl_13xx.h
- Chip_SYSCTL_SetStartPinRising() : sysctl_13xx.h
- Chip_SYSCTL_SetSYSTCKCAL() : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- Chip_SYSCTL_SetUSARTFRGDivider() : syscon_8xx.h
- Chip_SYSCTL_SetUSARTFRGMultiplier() : syscon_8xx.h
- Chip_SYSCTL_SetWakeup() : sysctl_11xx.c , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , syscon_8xx.h
- CHIP_SYSCTL_SPIFICLKSRC_T : clock_17xx_40xx.h
- CHIP_SYSCTL_USBCLKSRC_T : clock_13xx.h , clock_17xx_40xx.h
- Chip_TIMER_CaptureDisableInt() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CaptureEnableInt() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CaptureFallingEdgeDisable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CaptureFallingEdgeEnable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CapturePending() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CaptureRisingEdgeDisable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_CaptureRisingEdgeEnable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ClearCapture() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ClearMatch() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_DeInit() : timer_11xx.c , timer_11xx.h , timer_13xx.c , timer_13xx.h , timer_17xx_40xx.c , timer_17xx_40xx.h , timer_18xx_43xx.c , timer_18xx_43xx.h
- Chip_TIMER_Disable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_Enable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ExtMatchControlSet() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_Timer_GetClock() : timer_11xx.c , timer_13xx.c , timer_17xx_40xx.c , timer_18xx_43xx.c
- Chip_TIMER_Init() : timer_11xx.c , timer_11xx.h , timer_13xx.c , timer_13xx.h , timer_17xx_40xx.c , timer_17xx_40xx.h , timer_18xx_43xx.c , timer_18xx_43xx.h
- Chip_TIMER_MatchDisableInt() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_MatchEnableInt() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_MatchPending() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_PrescaleSet() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ReadCapture() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ReadCount() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ReadPrescale() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_Reset() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ResetOnMatchDisable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_ResetOnMatchEnable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_SetMatch() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_StopOnMatchDisable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_StopOnMatchEnable() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_TIMER_TIMER_SetCountClockSrc() : timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_UART_ABClearIntPending() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ABCmd() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_CheckBusy() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ClearAutoBaudReg() : uart_11xx.h , uart_13xx.h
- Chip_UART_ClearModemControl() : uart_11xx.h , uart_13xx.h
- Chip_UART_ClearRS485Flags() : uart_11xx.h , uart_13xx.h
- Chip_UART_ConfigData() : uart_11xx.h , uart_13xx.h , uart_17xx_40xx.h , uart_18xx_43xx.h , uart_8xx.h
- Chip_UART_DeInit() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h , uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_DetermineClk() : uart_17xx_40xx.c , uart_18xx_43xx.c
- Chip_UART_DisableDivisorAccess() : uart_11xx.h , uart_13xx.h
- Chip_UART_EnableDivisorAccess() : uart_11xx.h , uart_13xx.h
- Chip_UART_FIFOConfig() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_FIFOConfigStructInit() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ForceBreak() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_Get_UARTNum() : uart_17xx_40xx.c , uart_18xx_43xx.c
- Chip_UART_GetABEOStatus() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_GetClockRate() : uart_17xx_40xx.c
- Chip_UART_GetIntStatus() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h , uart_8xx.h
- Chip_UART_GetLineStatus() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_GetRS485Addr() : uart_11xx.h , uart_13xx.h
- Chip_UART_GetRS485Delay() : uart_11xx.h , uart_13xx.h
- Chip_UART_Init() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h , uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h , uart_8xx.c , uart_8xx.h
- Chip_UART_InitRingBuffer() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_IntConfig() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_IntDisable() : uart_11xx.h , uart_13xx.h
- Chip_UART_IntEnable() : uart_11xx.h , uart_13xx.h , uart_8xx.h
- Chip_UART_Interrupt_Handler() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_Interrupt_Receive() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_Interrupt_Transmit() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_IntGetStatus() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_IRQRBHandler() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_Read() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_ReadBlocking() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_ReadByte() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadIntIDReg() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadLineStatus() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadModemControl() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadModemStatus() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadRB() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_ReadScratch() : uart_11xx.h , uart_13xx.h
- Chip_UART_Receive() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ReceiveByte() : uart_17xx_40xx.h , uart_18xx_43xx.h , uart_8xx.c , uart_8xx.h
- Chip_UART_RXIntHandlerRB() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_Send() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h , uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_SendBlocking() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_SendByte() : uart_11xx.h , uart_13xx.h , uart_17xx_40xx.h , uart_18xx_43xx.h , uart_8xx.c , uart_8xx.h
- Chip_UART_SendRB() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_SetAutoBaudReg() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetBaud() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h , uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_SetBaudFDR() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetBaudRate() : uart_8xx.c , uart_8xx.h
- Chip_UART_SetDivisorLatches() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetModemControl() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetRS485Addr() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetRS485Delay() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetRS485Flags() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetScratch() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetupFIFOS() : uart_11xx.h , uart_13xx.h
- Chip_UART_TxCmd() : uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_TXDisable() : uart_11xx.h , uart_13xx.h
- Chip_UART_TXEnable() : uart_11xx.h , uart_13xx.h
- Chip_UART_TXIntHandlerRB() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- CHIP_WDTLFO_OSC_T : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_WKT_ClearIntStatus() : wkt_8xx.h
- CHIP_WKT_CLKSRC_T : wkt_8xx.h
- Chip_WKT_Start() : wkt_8xx.c , wkt_8xx.h
- Chip_WKT_Stop() : wkt_8xx.h
- Chip_WWDT_ClearStatusFlag() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_DeInit() : wwdt_11xx.c , wwdt_11xx.h , wwdt_13xx.c , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_Feed() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_GetCurrentCount() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_GetStatus() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_Init() : wwdt_11xx.c , wwdt_11xx.h , wwdt_13xx.c , wwdt_13xx.h , wwdt_17xx_40xx.c , wwdt_17xx_40xx.h , wwdt_18xx_43xx.c , wwdt_18xx_43xx.h , wwdt_8xx.c , wwdt_8xx.h
- Chip_WWDT_SetOption() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_SetTimeOut() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_SetWarning() : wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_SetWindow() : wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_Start() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_UnsetOption() : wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- chk_chr() : ff.c
- chk_mounted() : ff.c
- CHKTAG : eeprom.c , nandflash.c , norflash.c , eeprom.c
- CHKTAG_SIZE : eeprom.c , nandflash.c , norflash.c , eeprom.c
- Class : StdDescriptors.h
- CLCDC_LCDCTRL_ENABLE : lcd_001.h
- CLCDC_LCDCTRL_PWR : lcd_001.h
- CLK0_DELAY : sysinit_ea_devkit_17884088.c , sysinit_hitex_eva_18504350.c , sysinit_keil_mcb_18574357.c
- CLK_APB0_SSP0 : chip_clocks.h
- CLK_APB0_UART0 : chip_clocks.h
- CLK_APB0_UART1 : chip_clocks.h
- CLK_APB1_BUS : chip_clocks.h
- CLK_APB1_CAN1 : chip_clocks.h
- CLK_APB1_I2C0 : chip_clocks.h
- CLK_APB1_I2S : chip_clocks.h
- CLK_APB1_MOTOCON : chip_clocks.h
- CLK_APB2_SDIO : chip_clocks.h
- CLK_APB2_SSP1 : chip_clocks.h
- CLK_APB2_UART2 : chip_clocks.h
- CLK_APB2_UART3 : chip_clocks.h
- CLK_APB3_ADC0 : chip_clocks.h
- CLK_APB3_ADC1 : chip_clocks.h
- CLK_APB3_BUS : chip_clocks.h
- CLK_APB3_CAN0 : chip_clocks.h
- CLK_APB3_DAC : chip_clocks.h
- CLK_APB3_I2C1 : chip_clocks.h
- CLK_APLL : chip_clocks.h
- CLK_BASE_APB1 : chip_clocks.h
- CLK_BASE_APB3 : chip_clocks.h
- CLK_BASE_APLL : chip_clocks.h
- CLK_BASE_CGU_OUT0 : chip_clocks.h
- CLK_BASE_CGU_OUT1 : chip_clocks.h
- CLK_BASE_LAST : chip_clocks.h
- CLK_BASE_LCD : chip_clocks.h
- CLK_BASE_MX : chip_clocks.h
- CLK_BASE_NONE : chip_clocks.h
- CLK_BASE_OUT : chip_clocks.h
- CLK_BASE_PHY_RX : chip_clocks.h
- CLK_BASE_PHY_TX : chip_clocks.h
- CLK_BASE_RESERVED1 : chip_clocks.h
- CLK_BASE_RESERVED2 : chip_clocks.h
- CLK_BASE_RESERVED3 : chip_clocks.h
- CLK_BASE_RESERVED4 : chip_clocks.h
- CLK_BASE_RESERVED5 : chip_clocks.h
- CLK_BASE_RESERVED6 : chip_clocks.h
- CLK_BASE_RESERVED7 : chip_clocks.h
- CLK_BASE_SAFE : chip_clocks.h
- CLK_BASE_SDIO : chip_clocks.h
- CLK_BASE_SPIFI : chip_clocks.h
- CLK_BASE_SSP0 : chip_clocks.h
- CLK_BASE_SSP1 : chip_clocks.h
- CLK_BASE_UART0 : chip_clocks.h
- CLK_BASE_UART1 : chip_clocks.h
- CLK_BASE_UART2 : chip_clocks.h
- CLK_BASE_UART3 : chip_clocks.h
- CLK_BASE_USB0 : chip_clocks.h
- CLK_BASE_USB1 : chip_clocks.h
- CLK_CCU1_LAST : chip_clocks.h
- CLK_CCU2_LAST : chip_clocks.h
- CLK_CCU2_START : chip_clocks.h
- CLK_IDIV_A : chip_clocks.h
- CLK_IDIV_B : chip_clocks.h
- CLK_IDIV_C : chip_clocks.h
- CLK_IDIV_D : chip_clocks.h
- CLK_IDIV_E : chip_clocks.h
- CLK_IDIV_LAST : chip_clocks.h
- CLK_MX_BUS : chip_clocks.h
- CLK_MX_CREG : chip_clocks.h
- CLK_MX_DMA : chip_clocks.h
- CLK_MX_EEPROM : chip_clocks.h
- CLK_MX_EMC : chip_clocks.h
- CLK_MX_EMC_DIV : chip_clocks.h
- CLK_MX_ETHERNET : chip_clocks.h
- CLK_MX_FLASHA : chip_clocks.h
- CLK_MX_FLASHB : chip_clocks.h
- CLK_MX_GPIO : chip_clocks.h
- CLK_MX_LCD : chip_clocks.h
- CLK_MX_MXCORE : chip_clocks.h
- CLK_MX_QEI : chip_clocks.h
- CLK_MX_RITIMER : chip_clocks.h
- CLK_MX_SCT : chip_clocks.h
- CLK_MX_SCU : chip_clocks.h
- CLK_MX_SDIO : chip_clocks.h
- CLK_MX_SPIFI : chip_clocks.h
- CLK_MX_SSP0 : chip_clocks.h
- CLK_MX_SSP1 : chip_clocks.h
- CLK_MX_TIMER0 : chip_clocks.h
- CLK_MX_TIMER1 : chip_clocks.h
- CLK_MX_TIMER2 : chip_clocks.h
- CLK_MX_TIMER3 : chip_clocks.h
- CLK_MX_UART0 : chip_clocks.h
- CLK_MX_UART1 : chip_clocks.h
- CLK_MX_UART2 : chip_clocks.h
- CLK_MX_UART3 : chip_clocks.h
- CLK_MX_USB0 : chip_clocks.h
- CLK_MX_USB1 : chip_clocks.h
- CLK_MX_WWDT : chip_clocks.h
- CLK_RESERVED1 : chip_clocks.h
- CLK_RESERVED2 : chip_clocks.h
- CLK_RESERVED3 : chip_clocks.h
- CLK_RESERVED3A : chip_clocks.h
- CLK_RESERVED4 : chip_clocks.h
- CLK_RESERVED5 : chip_clocks.h
- CLK_RESERVED7 : chip_clocks.h
- CLK_RESERVED8 : chip_clocks.h
- CLK_SPIFI : chip_clocks.h
- CLK_USB0 : chip_clocks.h
- CLK_USB1 : chip_clocks.h
- CLKIN : swm_8xx.h
- CLKIN_32K : chip_clocks.h
- CLKIN_AUDIOPLL : chip_clocks.h
- CLKIN_CLKIN : chip_clocks.h
- CLKIN_CRYSTAL : chip_clocks.h
- CLKIN_ENET_RX : chip_clocks.h
- CLKIN_ENET_TX : chip_clocks.h
- CLKIN_IDIVA : chip_clocks.h
- CLKIN_IDIVB : chip_clocks.h
- CLKIN_IDIVC : chip_clocks.h
- CLKIN_IDIVD : chip_clocks.h
- CLKIN_IDIVE : chip_clocks.h
- clkin_info : app_clock_apis.c
- CLKIN_IRC : chip_clocks.h
- CLKIN_MAINPLL : chip_clocks.h
- CLKIN_RESERVED1 : chip_clocks.h
- CLKIN_RESERVED2 : chip_clocks.h
- CLKIN_RESERVED3 : chip_clocks.h
- CLKIN_USBPLL : chip_clocks.h
- CLKINPUT_PD : chip_clocks.h
- clksEnabled : i2s_18xx_43xx.c
- CLR_BUF_PO : HAL_LPC17xx.h
- clust2sect() : ff.c
- CMD : sdmmc_18xx_43xx.h
- CMD13_RCA : lpc_sdmmc.h
- CMD3_RCA : lpc_sdmmc.h
- CMD55_RCA : lpc_sdmmc.h
- CMD7_RCA : lpc_sdmmc.h
- CMD8_CHECKPATTERN : lpc_sdmmc.h
- CMD8_DEF_PATTERN : lpc_sdmmc.h
- CMD8_VOLTAGESUPPLIED_27_36 : lpc_sdmmc.h
- CMD9_RCA : lpc_sdmmc.h
- CMD_ALL_SEND_CID : sdmmc_18xx_43xx.h
- CMD_BIT_APP : sdmmc_18xx_43xx.h
- CMD_BIT_AUTO_STOP : sdmmc_18xx_43xx.h
- CMD_BIT_BUSY : sdmmc_18xx_43xx.h
- CMD_BIT_DATA : sdmmc_18xx_43xx.h
- CMD_BIT_INIT : sdmmc_18xx_43xx.h
- CMD_BIT_LS : sdmmc_18xx_43xx.h
- CMD_BIT_STREAM : sdmmc_18xx_43xx.h
- CMD_BIT_WRITE : sdmmc_18xx_43xx.h
- CMD_CFG_DEV : HAL_LPC17xx.h
- CMD_CLR_BUF : HAL_LPC17xx.h
- CMD_DESELECT_CARD : sdmmc_18xx_43xx.h
- CMD_GET_DEV_STAT : HAL_LPC17xx.h
- CMD_GET_ERR_CODE : HAL_LPC17xx.h
- CMD_IDLE : sdmmc_18xx_43xx.h
- CMD_MASK_CMD : sdmmc_18xx_43xx.h
- CMD_MASK_RESP : sdmmc_18xx_43xx.h
- CMD_MMC_OP_COND : sdmmc_18xx_43xx.h
- CMD_MMC_SET_RCA : sdmmc_18xx_43xx.h
- CMD_RD_ERR_STAT : HAL_LPC17xx.h
- CMD_RD_FRAME : HAL_LPC17xx.h
- CMD_RD_TEST : HAL_LPC17xx.h
- CMD_READ_MULTIPLE : sdmmc_18xx_43xx.h
- CMD_READ_SINGLE : sdmmc_18xx_43xx.h
- CMD_RESP : sdmmc_18xx_43xx.h
- CMD_RESP_R0 : sdmmc_18xx_43xx.h
- CMD_RESP_R1 : sdmmc_18xx_43xx.h
- CMD_RESP_R2 : sdmmc_18xx_43xx.h
- CMD_RESP_R3 : sdmmc_18xx_43xx.h
- CMD_SD_OP_COND : sdmmc_18xx_43xx.h
- CMD_SD_SEND_IF_COND : sdmmc_18xx_43xx.h
- CMD_SD_SEND_RCA : sdmmc_18xx_43xx.h
- CMD_SD_SET_WIDTH : sdmmc_18xx_43xx.h
- CMD_SEL_EP : HAL_LPC17xx.h
- CMD_SEL_EP_CLRI : HAL_LPC17xx.h
- CMD_SELECT_CARD : sdmmc_18xx_43xx.h
- CMD_SEND_CSD : sdmmc_18xx_43xx.h
- CMD_SEND_EXT_CSD : sdmmc_18xx_43xx.h
- CMD_SEND_STATUS : sdmmc_18xx_43xx.h
- CMD_SET_ADDR : HAL_LPC17xx.h
- CMD_SET_BLOCKLEN : sdmmc_18xx_43xx.h
- CMD_SET_DEV_STAT : HAL_LPC17xx.h
- CMD_SET_EP_STAT : HAL_LPC17xx.h
- CMD_SET_MODE : HAL_LPC17xx.h
- CMD_SHIFT_CMD : sdmmc_18xx_43xx.h
- CMD_STOP : sdmmc_18xx_43xx.h
- CMD_SUCCESS : flash_001.h
- CMD_TIMEOUT : sdmmc_17xx_40xx.c
- CMD_VALID_BUF : HAL_LPC17xx.h
- CMD_WRITE_MULTIPLE : sdmmc_18xx_43xx.h
- CMD_WRITE_SINGLE : sdmmc_18xx_43xx.h
- CmdQue : MassStorageClassCommon.h
- CMDRESP_NONE_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R1_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R1b_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R2_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R3_HC_CCS : lpc_sdmmc.h
- CMDRESP_R3_INIT_COMPLETE : lpc_sdmmc.h
- CMDRESP_R3_OCR_VAL : lpc_sdmmc.h
- CMDRESP_R3_S18A : lpc_sdmmc.h
- CMDRESP_R3_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R6_CARD_STATUS : lpc_sdmmc.h
- CMDRESP_R6_RCA_VAL : lpc_sdmmc.h
- CMDRESP_R6_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R7_CHECK_PATTERN : lpc_sdmmc.h
- CMDRESP_R7_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R7_VOLTAGE_ACCEPTED : lpc_sdmmc.h
- CmdSpecificInformation : MassStorageClassCommon.h
- CMP_CTRL_BITMASK : cmp_001.h
- CMP_CTRL_EXT_RESET_CMPRESET : cmp_001.h
- CMP_CTRL_EXT_RESET_INTERNAL : cmp_001.h
- CMP_CTRL_PD_IREF : cmp_001.h
- CMP_CTRL_PD_IREF_BITMASK : cmp_001.h
- CMP_CTRL_PD_VBG : cmp_001.h
- CMP_CTRL_PD_VBG_BITMASK : cmp_001.h
- CMP_CTRL_ROSC_BITMASK : cmp_001.h
- CMP_CTRL_ROSCCTL_CMP0 : cmp_001.h
- CMP_CTRL_ROSCCTL_CMP1 : cmp_001.h
- CMP_CTRL_T0CAP2_0LEVEL : cmp_001.h
- CMP_CTRL_T0CAP2_1LEVEL : cmp_001.h
- CMP_CTRL_T0CAP3_0EDGE : cmp_001.h
- CMP_CTRL_T0CAP3_1EDGE : cmp_001.h
- CMP_CTRL_T1CAP2_0LEVEL : cmp_001.h
- CMP_CTRL_T1CAP2_1EDGE : cmp_001.h
- CMP_CTRL_T1CAP3_0EDGE : cmp_001.h
- CMP_CTRL_T1CAP3_1LEVEL : cmp_001.h
- CMP_CTRL_TIMERCAPTURE_BITMASK : cmp_001.h
- CMP_CTRLx_BITMASK : cmp_001.h
- CMP_CTRLx_EN : cmp_001.h
- CMP_CTRLx_EN_BITMASK : cmp_001.h
- CMP_CTRLx_HYS : cmp_001.h
- CMP_CTRLx_HYS_BITMASK : cmp_001.h
- CMP_CTRLx_INTCTRL_BITMASK : cmp_001.h
- CMP_CTRLx_INTEDGE : cmp_001.h
- CMP_CTRLx_INTEDGE_BITMASK : cmp_001.h
- CMP_CTRLx_INTFLAG : cmp_001.h
- CMP_CTRLx_INTPOL_INV : cmp_001.h
- CMP_CTRLx_INTPOL_NORMAL : cmp_001.h
- CMP_CTRLx_INTTYPE_EDGE : cmp_001.h
- CMP_CTRLx_INTTYPE_LEVEL : cmp_001.h
- CMP_CTRLx_OE : cmp_001.h
- CMP_CTRLx_STAT : cmp_001.h
- CMP_CTRLx_SYNC : cmp_001.h
- CMP_CTRLx_VLADEN : cmp_001.h
- CMP_CTRLx_VLADEN_BITMASK : cmp_001.h
- CMP_CTRLx_VLADREF_VDDA : cmp_001.h
- CMP_CTRLx_VLADREF_VREFCMP : cmp_001.h
- CMP_CTRLx_VM : cmp_001.h
- CMP_CTRLx_VM_BITMASK : cmp_001.h
- CMP_CTRLx_VP : cmp_001.h
- CMP_CTRLx_VP_BITMASK : cmp_001.h
- CMP_CTRLx_VSEL : cmp_001.h
- CMP_CTRLx_VSEL_BITMASK : cmp_001.h
- CMP_ENCTRL_DIS_IN_DS_PWD : cmp_001.h
- CMP_ENCTRL_DIS_IN_PWD : cmp_001.h
- CMP_ENCTRL_DISABLE : cmp_001.h
- CMP_ENCTRL_ENABLE : cmp_001.h
- CMP_HYS_10MV : cmp_001.h
- CMP_HYS_15MV : cmp_001.h
- CMP_HYS_5MV : cmp_001.h
- CMP_HYS_NONE : cmp_001.h
- CMP_ID : cmp.c
- CMP_INPUT_CMP_OTHER_IN0 : cmp_001.h
- CMP_INPUT_CMPx_IN0 : cmp_001.h
- CMP_INPUT_CMPx_IN1 : cmp_001.h
- CMP_INPUT_CMPx_IN2 : cmp_001.h
- CMP_INPUT_CMPx_IN3 : cmp_001.h
- CMP_INPUT_INTERNAL_09VBG : cmp_001.h
- CMP_INPUT_VREF_DIV : cmp_001.h
- CMP_INTEDGE_BOTH : cmp_001.h
- CMP_INTEDGE_FALLING : cmp_001.h
- CMP_INTEDGE_RISING : cmp_001.h
- CMP_IRQHandler() : acmp.c
- CMP_NUM : cmp_001.h
- COLOR_CONVERSION : LCDConf.c
- COLOR_T : lpc_colors.h
- COLORS_8_565_MODE : lpc_colors.h
- COLORS_DEF : lpc_colors.h
- COLUMN_ADDR : lpc_nandflash_k9f1g.c
- command : dfuutil_programming_iflash_algorithm.c
- Command : MIDIClassCommon.h
- COMPARE_ERROR : flash_001.h
- COMPILE_TIME_ASSERT : error.h
- con_get_input() : i2c.c
- Con_GetInput() : i2s.c
- con_print_data() : i2c.c
- ConditionCode : OHCI.h
- CONF_DVICE : HAL_LPC17xx.h
- CONFIG_CPU_CLOCK_HZ : cpu_bsp_lpc43xx_m0.c
- CONFIG_SCT_nEV : sct_001.h
- CONFIG_SCT_nOU : sct_001.h
- CONFIG_SCT_nRG : sct_001.h
- configASSERT : lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- ConfigAttributes : StdDescriptors.h
- configCHECK_FOR_STACK_OVERFLOW : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- ConfigComparatorPtr_t : ConfigDescriptor.h
- configCPU_CLOCK_HZ : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configGENERATE_RUN_TIME_STATS : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configIDLE_SHOULD_YIELD : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configKERNEL_INTERRUPT_PRIORITY : FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configLIBRARY_LOWEST_INTERRUPT_PRIORITY : lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configLIBRARY_MAX_SYSCALL_INTERRUPT_PRIORITY : FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_CO_ROUTINE_PRIORITIES : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_PRIORITIES : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_SYSCALL_INTERRUPT_PRIORITY : lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_TASK_NAME_LEN : FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMINIMAL_STACK_SIZE : lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configPRIO_BITS : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configQUEUE_REGISTRY_SIZE : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- ConfigStruct : spi.c
- configTICK_RATE_HZ : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_QUEUE_LENGTH : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_TASK_PRIORITY : lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_TASK_STACK_DEPTH : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTOTAL_HEAP_SIZE : lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTSC2046Pins() : board_ea_devkit_17884088.c
- ConfigurationDescriptor : Descriptors.c
- ConfigurationNumber : StdDescriptors.h
- ConfigurationStrIndex : StdDescriptors.h
- configUSE_16_BIT_TICKS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_ALTERNATIVE_API : FreeRTOSConfig.h
- configUSE_APPLICATION_TASK_TAG : lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_CO_ROUTINES : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_COUNTING_SEMAPHORES : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_CUSTOM_TICK : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_IDLE_HOOK : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_MALLOC_FAILED_HOOK : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_MUTEXES : FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_PREEMPTION : lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_RECURSIVE_MUTEXES : FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_TICK_HOOK : FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_TICKLESS_IDLE : FreeRTOSConfig.h
- configUSE_TIMERS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h
- configUSE_TRACE_FACILITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h
- ContiguousBufferLength : RNDISClassHost.c
- CONTROL_BULK_SERVICE_RATIO : OHCI.h
- CONTROL_LIST_HEAD : OHCI.h
- CONTROL_REQTYPE_DIRECTION : StdRequestType.h
- CONTROL_REQTYPE_RECIPIENT : StdRequestType.h
- CONTROL_REQTYPE_TYPE : StdRequestType.h
- CONTROL_TRANSFER : HCD.h
- ControlEndpointFlag : EHCI.h
- ControlSize : AudioClassCommon.h
- COORD_GET_NUM : board_ea_devkit_17884088.c , board_hitex_eva_18504350.c
- COUNT_ERROR : flash_001.h
- counter : dualcore_emwin.c
- CountryCode : HIDClassCommon.h
- COUNTUP_TO : sct_001.h
- COUNTUP_TO_LIMIT_THEN_CLEAR_TO_ZERO : sct_001.h
- CPU_ADDR : cpu.h
- CPU_ALIGN : cpu.h
- CPU_BIT_BAND_PERIPH_BASE : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_PERIPH_REG_HI : cpu_c_m0.c , cpu_c.c , cpu_c_m0.c
- CPU_BIT_BAND_PERIPH_REG_LO : cpu_c_m0.c , cpu_c.c , cpu_c_m0.c
- CPU_BIT_BAND_SRAM_BASE : cpu_c.c , cpu_c_m0.c , cpu_c.c , cpu_c_m0.c , cpu_c.c , cpu_c_m0.c
- CPU_BIT_BAND_SRAM_REG_HI : cpu_c.c , cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_SRAM_REG_LO : cpu_c_m0.c , cpu_c.c , cpu_c_m0.c , cpu_c.c
- CPU_BitBandClr() : cpu.h , cpu_c_m0.c , cpu_c.c , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c
- CPU_BitBandSet() : cpu_c.c , cpu_c_m0.c , cpu_c.c , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c
- CPU_BOOLEAN : cpu.h
- CPU_BSP_MODULE : cpu_bsp.c
- CPU_CFG_ADDR_SIZE : cpu.h
- CPU_CFG_CRITICAL_METHOD : cpu.h
- CPU_CFG_DATA_SIZE : cpu.h
- CPU_CFG_ENDIAN_TYPE : cpu.h
- CPU_CFG_INT_DIS_MEAS_EN : cpu_cfg.h
- CPU_CFG_INT_DIS_MEAS_OVRHD_NBR : cpu_cfg.h
- CPU_CFG_LEAD_ZEROS_ASM_PRESENT : cpu_cfg.h , cpu.h
- CPU_CFG_NAME_EN : cpu_cfg.h
- CPU_CFG_NAME_SIZE : cpu_cfg.h
- CPU_CFG_STK_GROWTH : cpu.h
- CPU_CFG_TS_32_EN : cpu_cfg.h
- CPU_CFG_TS_64_EN : cpu_cfg.h
- CPU_CFG_TS_EN : cpu_core.h
- CPU_CFG_TS_TMR_EN : cpu_core.h
- CPU_CFG_TS_TMR_SIZE : cpu_cfg.h
- CPU_CHAR : cpu.h
- CPU_CntLeadZeros() : cpu.h , cpu_core.h , os_cpu_c_m0.c , cpu.h , cpu_core.c , cpu.h
- CPU_CntLeadZerosTbl : cpu_core.c
- CPU_CORE_EXT : cpu_core.h
- CPU_CORE_MODULE : cpu_core.c
- CPU_CORE_VERSION : cpu_core.h
- CPU_CRITICAL_ENTER : cpu.h
- CPU_CRITICAL_EXIT : cpu.h
- CPU_CRITICAL_METHOD_INT_DIS_EN : cpu_def.h
- CPU_CRITICAL_METHOD_NONE : cpu_def.h
- CPU_CRITICAL_METHOD_STATUS_LOCAL : cpu_def.h
- CPU_CRITICAL_METHOD_STATUS_STK : cpu_def.h
- CPU_DATA : cpu.h
- CPU_ENDIAN_TYPE_BIG : cpu_def.h
- CPU_ENDIAN_TYPE_LITTLE : cpu_def.h
- CPU_ENDIAN_TYPE_NONE : cpu_def.h
- CPU_ERR : cpu_core.h
- CPU_ERR_NAME_SIZE : cpu_core.h
- CPU_ERR_NONE : cpu_core.h
- CPU_ERR_NULL_PTR : cpu_core.h
- CPU_ERR_TS_FREQ_INVALID : cpu_core.h
- CPU_FNCT_PTR : cpu.h
- CPU_FNCT_VOID : cpu.h
- CPU_FP32 : cpu.h
- CPU_FP64 : cpu.h
- CPU_Init() : cpu_core.h , cpu_core.c
- CPU_INT08S : cpu.h
- CPU_INT08U : cpu.h
- CPU_INT16S : cpu.h
- CPU_INT16U : cpu.h
- CPU_INT32S : cpu.h
- CPU_INT32U : cpu.h
- CPU_INT64S : cpu.h
- CPU_INT64U : cpu.h
- CPU_INT_BUSFAULT : cpu.h
- CPU_INT_DBGMON : cpu.h
- CPU_INT_DIS : cpu.h
- CPU_INT_EN : cpu.h
- CPU_INT_EXT0 : cpu.h
- CPU_INT_HFAULT : cpu.h
- CPU_INT_MEM : cpu.h
- CPU_INT_NMI : cpu.h
- CPU_INT_PENDSV : cpu.h
- CPU_INT_RESET : cpu.h
- CPU_INT_RSVD_07 : cpu.h
- CPU_INT_RSVD_08 : cpu.h
- CPU_INT_RSVD_09 : cpu.h
- CPU_INT_RSVD_10 : cpu.h
- CPU_INT_RSVD_13 : cpu.h
- CPU_INT_SRC_POS_MAX : cpu_c_m0.c , cpu_c.c , cpu_c_m0.c
- CPU_INT_STK_PTR : cpu.h
- CPU_INT_SVCALL : cpu.h
- CPU_INT_SYSTICK : cpu.h
- CPU_INT_USAGEFAULT : cpu.h
- CPU_IntDis() : cpu.h
- CPU_IntEn() : cpu.h
- CPU_IntSrcDis() : cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h
- CPU_IntSrcEn() : cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c
- CPU_IntSrcPendClr() : cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c
- CPU_IntSrcPrioGet() : cpu_c_m0.c , cpu.h , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c
- CPU_IntSrcPrioSet() : cpu_c_m0.c , cpu.h , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h
- CPU_MSK_NVIC_ICSR_VECT_ACTIVE : cpu.h
- CPU_Name : cpu_core.h
- CPU_NameClr() : cpu_core.h , cpu_core.c
- CPU_NameGet() : cpu_core.h , cpu_core.c
- CPU_NameInit() : cpu_core.c
- CPU_NameSet() : cpu_core.c , cpu_core.h
- CPU_REG08 : cpu.h
- CPU_REG16 : cpu.h
- CPU_REG32 : cpu.h
- CPU_REG64 : cpu.h
- CPU_REG_DBG_CTRL : cpu.h
- CPU_REG_DBG_DATA : cpu.h
- CPU_REG_DBG_INT : cpu.h
- CPU_REG_DBG_SELECT : cpu.h
- CPU_REG_MPU_CTRL : cpu.h
- CPU_REG_MPU_REG_ATTR : cpu.h
- CPU_REG_MPU_REG_BASE : cpu.h
- CPU_REG_MPU_REG_NBR : cpu.h
- CPU_REG_MPU_TYPE : cpu.h
- CPU_REG_NVIC_ACTIVE : cpu.h
- CPU_REG_NVIC_AFR0 : cpu.h
- CPU_REG_NVIC_AFSR : cpu.h
- CPU_REG_NVIC_AIRCR : cpu.h
- CPU_REG_NVIC_AIRCR_ENDIANNESS : cpu.h
- CPU_REG_NVIC_AIRCR_SYSRESETREQ : cpu.h
- CPU_REG_NVIC_AIRCR_VECTCLRACTIVE : cpu.h
- CPU_REG_NVIC_AIRCR_VECTRESET : cpu.h
- CPU_REG_NVIC_BFAR : cpu.h
- CPU_REG_NVIC_CCR : cpu.h
- CPU_REG_NVIC_CCR_BFHFNMIGN : cpu.h
- CPU_REG_NVIC_CCR_DIV_0_TRP : cpu.h
- CPU_REG_NVIC_CCR_NONBASETHRDENA : cpu.h
- CPU_REG_NVIC_CCR_STKALIGN : cpu.h
- CPU_REG_NVIC_CCR_UNALIGN_TRP : cpu.h
- CPU_REG_NVIC_CCR_USERSETMPEND : cpu.h
- CPU_REG_NVIC_CFSR : cpu.h
- CPU_REG_NVIC_CFSR_BFARVALID : cpu.h
- CPU_REG_NVIC_CFSR_DACCVIOL : cpu.h
- CPU_REG_NVIC_CFSR_DIVBYZERO : cpu.h
- CPU_REG_NVIC_CFSR_IACCVIOL : cpu.h
- CPU_REG_NVIC_CFSR_IBUSERR : cpu.h
- CPU_REG_NVIC_CFSR_IMPRECISERR : cpu.h
- CPU_REG_NVIC_CFSR_INVPC : cpu.h
- CPU_REG_NVIC_CFSR_INVSTATE : cpu.h
- CPU_REG_NVIC_CFSR_MMARVALID : cpu.h
- CPU_REG_NVIC_CFSR_MSTKERR : cpu.h
- CPU_REG_NVIC_CFSR_MUNSTKERR : cpu.h
- CPU_REG_NVIC_CFSR_NOCP : cpu.h
- CPU_REG_NVIC_CFSR_PRECISERR : cpu.h
- CPU_REG_NVIC_CFSR_STKERR : cpu.h
- CPU_REG_NVIC_CFSR_UNALIGNED : cpu.h
- CPU_REG_NVIC_CFSR_UNDEFINSTR : cpu.h
- CPU_REG_NVIC_CFSR_UNSTKERR : cpu.h
- CPU_REG_NVIC_CLREN : cpu.h
- CPU_REG_NVIC_CLRPEND : cpu.h
- CPU_REG_NVIC_CPUID : cpu.h
- CPU_REG_NVIC_DFR0 : cpu.h
- CPU_REG_NVIC_DFSR : cpu.h
- CPU_REG_NVIC_DFSR_BKPT : cpu.h
- CPU_REG_NVIC_DFSR_DWTTRAP : cpu.h
- CPU_REG_NVIC_DFSR_EXTERNAL : cpu.h
- CPU_REG_NVIC_DFSR_HALTED : cpu.h
- CPU_REG_NVIC_DFSR_VCATCH : cpu.h
- CPU_REG_NVIC_HFSR : cpu.h
- CPU_REG_NVIC_HFSR_DEBUGEVT : cpu.h
- CPU_REG_NVIC_HFSR_FORCED : cpu.h
- CPU_REG_NVIC_HFSR_VECTTBL : cpu.h
- CPU_REG_NVIC_ICSR : cpu.h
- CPU_REG_NVIC_ICSR_ISRPENDING : cpu.h
- CPU_REG_NVIC_ICSR_ISRPREEMPT : cpu.h
- CPU_REG_NVIC_ICSR_NMIPENDSET : cpu.h
- CPU_REG_NVIC_ICSR_PENDSTCLR : cpu.h
- CPU_REG_NVIC_ICSR_PENDSTSET : cpu.h
- CPU_REG_NVIC_ICSR_PENDSVCLR : cpu.h
- CPU_REG_NVIC_ICSR_PENDSVSET : cpu.h
- CPU_REG_NVIC_ICSR_RETTOBASE : cpu.h
- CPU_REG_NVIC_ISAFR0 : cpu.h
- CPU_REG_NVIC_ISAFR1 : cpu.h
- CPU_REG_NVIC_ISAFR2 : cpu.h
- CPU_REG_NVIC_ISAFR3 : cpu.h
- CPU_REG_NVIC_ISAFR4 : cpu.h
- CPU_REG_NVIC_MMFAR : cpu.h
- CPU_REG_NVIC_MMFR0 : cpu.h
- CPU_REG_NVIC_MMFR1 : cpu.h
- CPU_REG_NVIC_MMFR2 : cpu.h
- CPU_REG_NVIC_MMFR3 : cpu.h
- CPU_REG_NVIC_NVIC : cpu.h
- CPU_REG_NVIC_PFR0 : cpu.h
- CPU_REG_NVIC_PFR1 : cpu.h
- CPU_REG_NVIC_PRIO : cpu.h
- CPU_REG_NVIC_SCR : cpu.h
- CPU_REG_NVIC_SCR_SEVONPEND : cpu.h
- CPU_REG_NVIC_SCR_SLEEPDEEP : cpu.h
- CPU_REG_NVIC_SCR_SLEEPONEXIT : cpu.h
- CPU_REG_NVIC_SETEN : cpu.h
- CPU_REG_NVIC_SETPEND : cpu.h
- CPU_REG_NVIC_SHCSR : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_MONITORACT : cpu.h
- CPU_REG_NVIC_SHCSR_PENDSVACT : cpu.h
- CPU_REG_NVIC_SHCSR_SVCALLACT : cpu.h
- CPU_REG_NVIC_SHCSR_SVCALLPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_SYSTICKACT : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHPRI1 : cpu.h
- CPU_REG_NVIC_SHPRI2 : cpu.h
- CPU_REG_NVIC_SHPRI3 : cpu.h
- CPU_REG_NVIC_ST_CAL : cpu.h
- CPU_REG_NVIC_ST_CAL_NOREF : cpu.h
- CPU_REG_NVIC_ST_CAL_SKEW : cpu.h
- CPU_REG_NVIC_ST_CTRL : cpu.h
- CPU_REG_NVIC_ST_CTRL_CLKSOURCE : cpu.h
- CPU_REG_NVIC_ST_CTRL_COUNTFLAG : cpu.h
- CPU_REG_NVIC_ST_CTRL_ENABLE : cpu.h
- CPU_REG_NVIC_ST_CTRL_TICKINT : cpu.h
- CPU_REG_NVIC_ST_CURRENT : cpu.h
- CPU_REG_NVIC_ST_RELOAD : cpu.h
- CPU_REG_NVIC_SW_TRIG : cpu.h
- CPU_REG_NVIC_VTOR : cpu.h
- CPU_REG_NVIC_VTOR_TBLBASE : cpu.h
- CPU_RevBits() : cpu.h
- CPU_SIZE_T : cpu.h
- CPU_SR : cpu.h
- CPU_SR_ALLOC : cpu.h
- CPU_SR_Restore() : cpu.h
- CPU_SR_Save() : cpu.h
- CPU_STK : cpu.h
- CPU_STK_GROWTH_HI_TO_LO : cpu_def.h
- CPU_STK_GROWTH_LO_TO_HI : cpu_def.h
- CPU_STK_GROWTH_NONE : cpu_def.h
- CPU_STK_SIZE : cpu.h
- CPU_SW_Exception() : cpu_core.c , cpu_core.h
- CPU_SW_EXCEPTION : cpu_core.h
- CPU_TIME_MEAS_NBR_MAX : cpu_core.h
- CPU_TIME_MEAS_NBR_MIN : cpu_core.h
- CPU_TO_BE16 : Endianness.h
- cpu_to_be16 : Endianness.h
- CPU_TO_BE32 : Endianness.h
- cpu_to_be32 : Endianness.h
- CPU_TO_LE16 : Endianness.h
- cpu_to_le16 : Endianness.h
- CPU_TO_LE32 : Endianness.h
- cpu_to_le32 : Endianness.h
- CPU_TS : cpu_core.h
- CPU_TS32 : cpu_core.h
- CPU_TS32_to_uSec() : cpu_core.h
- CPU_TS64 : cpu_core.h
- CPU_TS64_to_uSec() : cpu_core.h
- CPU_TS_Get32() : cpu_core.c , cpu_core.h
- CPU_TS_Get64() : cpu_core.h , cpu_core.c
- CPU_TS_Init() : cpu_core.c
- CPU_TS_TMR : cpu_core.h
- CPU_TS_TMR_FREQ : cpu_core.h
- CPU_TS_TmrFreq_Hz : cpu_core.h
- CPU_TS_TmrFreqGet() : cpu_core.c , cpu_core.h
- CPU_TS_TmrFreqSet() : cpu_core.h , cpu_core.c
- CPU_TS_TmrInit() : cpu_bsp.c , cpu_bsp_lpc43xx_m0.c , cpu_core.h
- CPU_TS_TmrRd() : cpu_bsp.c , cpu_core.h , cpu_bsp_lpc43xx_m0.c
- CPU_TS_Update() : cpu_core.c , cpu_core.h
- CPU_TYPE_CREATE : cpu_core.h
- CPU_VOID : cpu.h
- CPU_WaitForExcept() : cpu.h
- CPU_WaitForInt() : cpu.h
- CPU_WORD_SIZE_08 : cpu_def.h
- CPU_WORD_SIZE_16 : cpu_def.h
- CPU_WORD_SIZE_32 : cpu_def.h
- CPU_WORD_SIZE_64 : cpu_def.h
- CPUCLOCKFRQINKHZ : dfuutil_programming_iflash_algorithm.c
- CRC_MODE_POLY_BITMASK : crc_001.h
- CRC_MODE_POLY_CCITT : crc_001.h
- CRC_MODE_POLY_CRC16 : crc_001.h
- CRC_MODE_POLY_CRC32 : crc_001.h
- CRC_MODE_SUM_BIT_RVS : crc_001.h
- CRC_MODE_SUM_BITMASK : crc_001.h
- CRC_MODE_SUM_CMPL : crc_001.h
- CRC_MODE_WRDATA_BIT_RVS : crc_001.h
- CRC_MODE_WRDATA_BITMASK : crc_001.h
- CRC_MODE_WRDATA_CMPL : crc_001.h
- CRC_POLY_CCITT : crc_001.h
- CRC_POLY_CRC16 : crc_001.h
- CRC_POLY_CRC32 : crc_001.h
- CRC_POLY_LAST : crc_001.h
- CRC_POLY_T : crc_8xx.h , crc_17xx_40xx.h
- CRC_SEED_CCITT : crc_001.h
- CRC_SEED_CRC16 : crc_001.h
- CRC_SEED_CRC32 : crc_001.h
- create_chain() : ff.c
- CREATE_LINKMAP : ff.h
- create_name() : ff.c
- CreateDiskImage() : fatutil.h , fatutil.c
- createExtIDEntry() : can_001.c
- createStdIDEntry() : can_001.c
- createUnUsedSTDEntry() : can_001.c
- CRYSTAL_32K_FREQ_IN : sys_config.h
- CRYSTAL_MAIN_FREQ_IN : sys_config.h
- CSW_CMD_FAILED : usbd_msc.h
- CSW_CMD_PASSED : usbd_msc.h
- CSW_PHASE_ERROR : usbd_msc.h
- CT_BLOCK : diskio.h
- CT_MMC : diskio.h
- CT_SD1 : diskio.h
- CT_SD2 : diskio.h
- CT_SDC : diskio.h
- CTRL_EJECT : diskio.h
- CTRL_ERASE_SECTOR : diskio.h
- CTRL_FORMAT : diskio.h
- CTRL_LOCK : diskio.h
- CTRL_POWER : diskio.h
- CTRL_RD_EN : HAL_LPC17xx.h
- CTRL_SYNC : diskio.h
- CTRL_WR_EN : HAL_LPC17xx.h
- CTS : usart_002.h
- CTS_DELTA : usart_002.h
- CTS_DELTA_INT : usart_002.h
- currCmdAddr : dfuutil_programming_dfu_ops.c
- currCmdSize : dfuutil_programming_dfu_ops.c
- CurrentAudioSampleFrequency : AudioOutput.c , AudioInput.c , AudioOutput.c
- CurrentBufferPointer : OHCI.h
- CurrentQtd : EHCI.h
- currStatus : dfuutil_programming_dfu_ops.c
- Cursor : Cursor.h
- CURSOR_H_OFS : Cursor.h
- CURSOR_H_SIZE : Cursor.h
- CURSOR_V_OFS : Cursor.h
- CURSOR_V_SIZE : Cursor.h