| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
Chip_I2S_Audio_Format_T Struct Reference
CHIP: LPC17xx/40xx I2S driver | CHIP: LPC18xx/43xx I2S driver

## Detailed Description

I2S Audio Format Structure.

Definition at line 50 of file i2s_17xx_40xx.h.

`#include "i2s_17xx_40xx.h"`

## Data Fields
uint32_t | SampleRate
uint8_t | ChannelNumber
uint8_t | WordWidth

## Field Documentation

uint8_t ChannelNumber

Channel Number - 1 is mono, 2 is stereo

Definition at line 52 of file i2s_17xx_40xx.h.

uint32_t SampleRate

Sample Rate

Definition at line 51 of file i2s_17xx_40xx.h.

uint8_t WordWidth

Word Width - 8, 16 or 32 bits

Definition at line 53 of file i2s_17xx_40xx.h.

The documentation for this struct was generated from the following files:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_chip/chip_17xx_40xx/i2s_17xx_40xx.h
- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_chip/chip_18xx_43xx/i2s_18xx_43xx.h