| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Keyboard Device
USB examples

## Detailed Description

Example description
This example implements a HID device which is used for keyboard configuration.

When the example is run and the board is connected to a PC with a USB cable it will enumerate on the PC as a HID Keyboard device. You should see the device appear in the "Device Manager" under "Keyboards". If you right click on HID Keyboard Device->Properties a window will appear called "HID Keyboard Device Properties". If you select the "Details" tab you will see a "Properties" drop down, click on it and select "Hardware Ids". You should see the below entries for Vendor Id and Product Id.

HID\VID_1FC9&PID_2042&REV_0001
HID\VID_1FC9&PID_2042

This information should match the data in the "Device Descriptor Structure" in the "Descriptors.c" file in the Example_KeyboardDevice project directory.

To demostrate the keyboard open an editing application such as Notepad or MS Word. Moving the joystick (SW2) on the Xpresso base board will output characters onto the editing application.

Special connection requirements
Need to connect with base board for using buttons and joystick

Build procedures:
LPC11xx example quickstart for Code Red Xpresso
LPC11xx example quickstart for Keil uVision4
LPC11xx example quickstart for IAR EWARM

Supported boards and board setup:
NXP Xpresso LPC11U14 board
NXP Xpresso LPC11C24 board

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Main definitions
| ROM stack support