| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - d -

- DAC_BIAS_EN : dac_001.h
- DAC_CCNT_VALUE : dac_001.h
- DAC_CNT_ENA : dac_001.h
- DAC_DACCTRL_MASK : dac_001.h
- DAC_DBLBUF_ENA : dac_001.h
- DAC_DMA_ENA : dac_001.h
- DAC_TIMEOUT : dac.c
- DAC_VALUE : dac_001.h
- DARKGRAY : lpc_colors.h
- DAT_CLR_BUF : HAL_LPC17xx.h
- DAT_GET_DEV_STAT : HAL_LPC17xx.h
- DAT_GET_ERR_CODE : HAL_LPC17xx.h
- DAT_RD_ERR_STAT : HAL_LPC17xx.h
- DAT_RD_FRAME : HAL_LPC17xx.h
- DAT_RD_TEST : HAL_LPC17xx.h
- DAT_SEL_EP : HAL_LPC17xx.h
- DAT_SEL_EP_CLRI : HAL_LPC17xx.h
- DAT_WR_BYTE : HAL_LPC17xx.h
- DATA_RAM_BLOCK_SIZE : DataRam.h
- DATA_READ : SCSI.h
- DATA_SIZE : dac.c
- DATA_TIMEOUT : sdmmc_17xx_40xx.c
- DATA_TIMER_VALUE_R : sdmmc_17xx_40xx.c
- DATA_TIMER_VALUE_W : sdmmc_17xx_40xx.c
- DATA_WRITE : SCSI.h
- DATA_X : board_keil_mcb_18574357.h
- DATA_XYZ : board_keil_mcb_18574357.h
- DATA_Y : board_keil_mcb_18574357.h
- DATA_Z : board_keil_mcb_18574357.h
- DATASECTORS : fatutil.h
- DATE_DAY : fatutil.h
- DATE_MONTH : fatutil.h
- DATE_YEAR : fatutil.h
- DDE : ff.c
- DEBUG_ENABLE : sys_config.h
- DEBUG_UART : sys_config.h
- DEBUGIN : board_api.h
- DEBUGINIT : board_api.h
- DEBUGOUT : board_api.h
- debugstr : app_sdmmc_meas.c , sdmmc.c
- DEBUGSTR : board_api.h
- DEF_ABS : lib_def.h
- DEF_ACTIVE : lib_def.h
- DEF_BIT : lib_def.h
- DEF_BIT_00 : lib_def.h
- DEF_BIT_01 : lib_def.h
- DEF_BIT_02 : lib_def.h
- DEF_BIT_03 : lib_def.h
- DEF_BIT_04 : lib_def.h
- DEF_BIT_05 : lib_def.h
- DEF_BIT_06 : lib_def.h
- DEF_BIT_07 : lib_def.h
- DEF_BIT_08 : lib_def.h
- DEF_BIT_09 : lib_def.h
- DEF_BIT_10 : lib_def.h
- DEF_BIT_11 : lib_def.h
- DEF_BIT_12 : lib_def.h
- DEF_BIT_13 : lib_def.h
- DEF_BIT_14 : lib_def.h
- DEF_BIT_15 : lib_def.h
- DEF_BIT_16 : lib_def.h
- DEF_BIT_17 : lib_def.h
- DEF_BIT_18 : lib_def.h
- DEF_BIT_19 : lib_def.h
- DEF_BIT_20 : lib_def.h
- DEF_BIT_21 : lib_def.h
- DEF_BIT_22 : lib_def.h
- DEF_BIT_23 : lib_def.h
- DEF_BIT_24 : lib_def.h
- DEF_BIT_25 : lib_def.h
- DEF_BIT_26 : lib_def.h
- DEF_BIT_27 : lib_def.h
- DEF_BIT_28 : lib_def.h
- DEF_BIT_29 : lib_def.h
- DEF_BIT_30 : lib_def.h
- DEF_BIT_31 : lib_def.h
- DEF_BIT_32 : lib_def.h
- DEF_BIT_33 : lib_def.h
- DEF_BIT_34 : lib_def.h
- DEF_BIT_35 : lib_def.h
- DEF_BIT_36 : lib_def.h
- DEF_BIT_37 : lib_def.h
- DEF_BIT_38 : lib_def.h
- DEF_BIT_39 : lib_def.h
- DEF_BIT_40 : lib_def.h
- DEF_BIT_41 : lib_def.h
- DEF_BIT_42 : lib_def.h
- DEF_BIT_43 : lib_def.h
- DEF_BIT_44 : lib_def.h
- DEF_BIT_45 : lib_def.h
- DEF_BIT_46 : lib_def.h
- DEF_BIT_47 : lib_def.h
- DEF_BIT_48 : lib_def.h
- DEF_BIT_49 : lib_def.h
- DEF_BIT_50 : lib_def.h
- DEF_BIT_51 : lib_def.h
- DEF_BIT_52 : lib_def.h
- DEF_BIT_53 : lib_def.h
- DEF_BIT_54 : lib_def.h
- DEF_BIT_55 : lib_def.h
- DEF_BIT_56 : lib_def.h
- DEF_BIT_57 : lib_def.h
- DEF_BIT_58 : lib_def.h
- DEF_BIT_59 : lib_def.h
- DEF_BIT_60 : lib_def.h
- DEF_BIT_61 : lib_def.h
- DEF_BIT_62 : lib_def.h
- DEF_BIT_63 : lib_def.h
- DEF_BIT_CLR : lib_def.h
- DEF_BIT_FIELD : lib_def.h
- DEF_BIT_IS_CLR : lib_def.h
- DEF_BIT_IS_CLR_ANY : lib_def.h
- DEF_BIT_IS_SET : lib_def.h
- DEF_BIT_IS_SET_ANY : lib_def.h
- DEF_BIT_MASK : lib_def.h
- DEF_BIT_NONE : lib_def.h
- DEF_BIT_SET : lib_def.h
- DEF_CHK_VAL : lib_def.h
- DEF_CHK_VAL_MAX : lib_def.h
- DEF_CHK_VAL_MIN : lib_def.h
- DEF_CLR : lib_def.h
- DEF_DISABLED : lib_def.h
- DEF_ENABLED : lib_def.h
- DEF_FAIL : lib_def.h
- DEF_FALSE : lib_def.h
- DEF_INACTIVE : lib_def.h
- DEF_INT_08_MASK : lib_def.h
- DEF_INT_08_NBR_BITS : lib_def.h
- DEF_INT_08S_MAX_VAL : lib_def.h
- DEF_INT_08S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_08S_MIN_VAL : lib_def.h
- DEF_INT_08S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_08S_NBR_DIG_MAX : lib_def.h
- DEF_INT_08S_NBR_DIG_MIN : lib_def.h
- DEF_INT_08U_MAX_VAL : lib_def.h
- DEF_INT_08U_MIN_VAL : lib_def.h
- DEF_INT_08U_NBR_DIG_MAX : lib_def.h
- DEF_INT_08U_NBR_DIG_MIN : lib_def.h
- DEF_INT_16_MASK : lib_def.h
- DEF_INT_16_NBR_BITS : lib_def.h
- DEF_INT_16S_MAX_VAL : lib_def.h
- DEF_INT_16S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_16S_MIN_VAL : lib_def.h
- DEF_INT_16S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_16S_NBR_DIG_MAX : lib_def.h
- DEF_INT_16S_NBR_DIG_MIN : lib_def.h
- DEF_INT_16U_MAX_VAL : lib_def.h
- DEF_INT_16U_MIN_VAL : lib_def.h
- DEF_INT_16U_NBR_DIG_MAX : lib_def.h
- DEF_INT_16U_NBR_DIG_MIN : lib_def.h
- DEF_INT_32_MASK : lib_def.h
- DEF_INT_32_NBR_BITS : lib_def.h
- DEF_INT_32S_MAX_VAL : lib_def.h
- DEF_INT_32S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_32S_MIN_VAL : lib_def.h
- DEF_INT_32S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_32S_NBR_DIG_MAX : lib_def.h
- DEF_INT_32S_NBR_DIG_MIN : lib_def.h
- DEF_INT_32U_MAX_VAL : lib_def.h
- DEF_INT_32U_MIN_VAL : lib_def.h
- DEF_INT_32U_NBR_DIG_MAX : lib_def.h
- DEF_INT_32U_NBR_DIG_MIN : lib_def.h
- DEF_INT_64_MASK : lib_def.h
- DEF_INT_64_NBR_BITS : lib_def.h
- DEF_INT_64S_MAX_VAL : lib_def.h
- DEF_INT_64S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_64S_MIN_VAL : lib_def.h
- DEF_INT_64S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_64S_NBR_DIG_MAX : lib_def.h
- DEF_INT_64S_NBR_DIG_MIN : lib_def.h
- DEF_INT_64U_MAX_VAL : lib_def.h
- DEF_INT_64U_MIN_VAL : lib_def.h
- DEF_INT_64U_NBR_DIG_MAX : lib_def.h
- DEF_INT_64U_NBR_DIG_MIN : lib_def.h
- DEF_INT_CPU_NBR_BITS : lib_def.h
- DEF_INVALID : lib_def.h
- DEF_MAX : lib_def.h
- DEF_MIN : lib_def.h
- DEF_NAMEBUF : ff.c
- DEF_NBR_BASE_BIN : lib_def.h
- DEF_NBR_BASE_DEC : lib_def.h
- DEF_NBR_BASE_HEX : lib_def.h
- DEF_NBR_BASE_OCT : lib_def.h
- DEF_NIBBLE_MASK : lib_def.h
- DEF_NIBBLE_NBR_BITS : lib_def.h
- DEF_NO : lib_def.h
- DEF_OCTET_MASK : lib_def.h
- DEF_OCTET_NBR_BITS : lib_def.h
- DEF_OFF : lib_def.h
- DEF_OK : lib_def.h
- DEF_ON : lib_def.h
- DEF_SET : lib_def.h
- DEF_TIME_NBR_DAY_PER_WK : lib_def.h
- DEF_TIME_NBR_DAY_PER_YR : lib_def.h
- DEF_TIME_NBR_DAY_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_HR_PER_DAY : lib_def.h
- DEF_TIME_NBR_HR_PER_WK : lib_def.h
- DEF_TIME_NBR_HR_PER_YR : lib_def.h
- DEF_TIME_NBR_HR_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_MIN_PER_DAY : lib_def.h
- DEF_TIME_NBR_MIN_PER_HR : lib_def.h
- DEF_TIME_NBR_MIN_PER_WK : lib_def.h
- DEF_TIME_NBR_MIN_PER_YR : lib_def.h
- DEF_TIME_NBR_MIN_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_mS_PER_SEC : lib_def.h
- DEF_TIME_NBR_nS_PER_SEC : lib_def.h
- DEF_TIME_NBR_SEC_PER_DAY : lib_def.h
- DEF_TIME_NBR_SEC_PER_HR : lib_def.h
- DEF_TIME_NBR_SEC_PER_MIN : lib_def.h
- DEF_TIME_NBR_SEC_PER_WK : lib_def.h
- DEF_TIME_NBR_SEC_PER_YR : lib_def.h
- DEF_TIME_NBR_SEC_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_uS_PER_SEC : lib_def.h
- DEF_TRUE : lib_def.h
- DEF_VALID : lib_def.h
- DEF_YES : lib_def.h
- DEFAULT_ACCEPTMBOX_SIZE : lwipopts.h
- DEFAULT_I2C : i2c.c
- DEFAULT_TCP_RECVMBOX_SIZE : lwipopts.h
- DEFAULT_THREAD_PRIO : lwipopts.h
- DEFAULT_THREAD_STACKSIZE : lwipopts.h
- DEFAULT_UDP_RECVMBOX_SIZE : lwipopts.h
- DELTA_RXBRK : usart_002.h
- DELTA_RXBRK_INT : usart_002.h
- DESCRIPTOR_CAST : ConfigDescriptor.h
- DESCRIPTOR_PCAST : ConfigDescriptor.h
- DESCRIPTOR_SIZE : ConfigDescriptor.h
- DESCRIPTOR_TYPE : ConfigDescriptor.h
- DEV_ADDR_MASK : HAL_LPC17xx.h
- DEV_CON : HAL_LPC17xx.h
- DEV_CON_CH : HAL_LPC17xx.h
- DEV_EN : HAL_LPC17xx.h
- DEV_RST : HAL_LPC17xx.h
- DEV_STAT_INT : Endpoint_LPC11Uxx.h , HAL_LPC17xx.h
- DEV_SUS : HAL_LPC17xx.h
- DEV_SUS_CH : HAL_LPC17xx.h
- DEVICE_TYPE_BLOCK : SCSI.h
- DEVICE_TYPE_CDROM : SCSI.h
- DFU_BUFF_PROG_SIZE : dfuutil_programming_iflash_algorithm.c , dfuutil_programming_spiflash_algorithm.c , dfuutil_programming_any_algorithm.c
- DFU_EP0_DATA : usbd_dfu.h
- DFU_EP0_NONE : usbd_dfu.h
- DFU_EP0_STALL : usbd_dfu.h
- DFU_EP0_UNHANDLED : usbd_dfu.h
- DFU_EP0_ZLP : usbd_dfu.h
- DFU_FUNC_DESC_SIZE : usbd_dfu.h
- DFU_GET_STATUS_SIZE : usbd_dfu.h
- DFU_STATUS_errADDRESS : usbd_dfu.h
- DFU_STATUS_errCHECK_ERASED : usbd_dfu.h
- DFU_STATUS_errERASE : usbd_dfu.h
- DFU_STATUS_errFILE : usbd_dfu.h
- DFU_STATUS_errFIRMWARE : usbd_dfu.h
- DFU_STATUS_errNOTDONE : usbd_dfu.h
- DFU_STATUS_errPOR : usbd_dfu.h
- DFU_STATUS_errPROG : usbd_dfu.h
- DFU_STATUS_errSTALLEDPKT : usbd_dfu.h
- DFU_STATUS_errTARGET : usbd_dfu.h
- DFU_STATUS_errUNKNOWN : usbd_dfu.h
- DFU_STATUS_errUSBR : usbd_dfu.h
- DFU_STATUS_errVENDOR : usbd_dfu.h
- DFU_STATUS_errVERIFY : usbd_dfu.h
- DFU_STATUS_errWRITE : usbd_dfu.h
- DFU_STATUS_OK : usbd_dfu.h
- DFUPROG_VALIDVAL : dfuutil_programming_api.h
- DHCP_DEBUG : lwipopts.h
- DIR_Attr : ff.c
- DIR_CrtDate : ff.c
- DIR_CrtTime : ff.c
- DIR_CrtTimeTenth : ff.c
- DIR_FileSize : ff.c
- DIR_FstClusHI : ff.c
- DIR_FstClusLO : ff.c
- DIR_LstAccDate : ff.c
- DIR_Name : ff.c
- DIR_NTres : ff.c
- DIR_WrtDate : ff.c
- DIR_WrtTime : ff.c
- DIRECTORYSECTORCNT : fatutil.h
- DISABLE_WDT_TIMEOUT : watchdog.c
- DISK_READ_ONLY : MassStorage.h , usbmsdev.h
- DISKSIZE : fatutil.h
- DISPLAY_DRIVER : LCDConf.c
- DISPLAY_HEIGHT : swim_color_bars.c
- DISPLAY_ORIENTATION : LCDConf.c
- DISPLAY_WIDTH : swim_color_bars.c
- DMA_BM_AAL : enet_001.h
- DMA_BM_ATDS : enet_001.h
- DMA_BM_DA : enet_001.h
- DMA_BM_DSL : enet_001.h
- DMA_BM_FB : enet_001.h
- DMA_BM_MB : enet_001.h
- DMA_BM_PBL : enet_001.h
- DMA_BM_PBL8X : enet_001.h
- DMA_BM_PR : enet_001.h
- DMA_BM_RPBL : enet_001.h
- DMA_BM_SWR : enet_001.h
- DMA_BM_TXPR : enet_001.h
- DMA_BM_USP : enet_001.h
- DMA_CONTROLLER : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- DMA_DESCRIPTOR_COUNT : gpdma_speed_test.c
- DMA_IE_AIE : enet_001.h
- DMA_IE_ERE : enet_001.h
- DMA_IE_ETE : enet_001.h
- DMA_IE_FBE : enet_001.h
- DMA_IE_NIE : enet_001.h
- DMA_IE_OVE : enet_001.h
- DMA_IE_RIE : enet_001.h
- DMA_IE_RSE : enet_001.h
- DMA_IE_RUE : enet_001.h
- DMA_IE_RWE : enet_001.h
- DMA_IE_TIE : enet_001.h
- DMA_IE_TJE : enet_001.h
- DMA_IE_TSE : enet_001.h
- DMA_IE_TUE : enet_001.h
- DMA_IE_UNE : enet_001.h
- DMA_MFRM_FMA : enet_001.h
- DMA_MFRM_FMCMSK : enet_001.h
- DMA_MFRM_OC : enet_001.h
- DMA_MFRM_OF : enet_001.h
- DMA_OM_DFF : enet_001.h
- DMA_OM_DT : enet_001.h
- DMA_OM_FEF : enet_001.h
- DMA_OM_FTF : enet_001.h
- DMA_OM_FUF : enet_001.h
- DMA_OM_OSF : enet_001.h
- DMA_OM_RSF : enet_001.h
- DMA_OM_RTC : enet_001.h
- DMA_OM_SR : enet_001.h
- DMA_OM_ST : enet_001.h
- DMA_OM_TSF : enet_001.h
- DMA_OM_TTC : enet_001.h
- DMA_ST_AIE : enet_001.h
- DMA_ST_ALL : enet_001.h
- DMA_ST_ERI : enet_001.h
- DMA_ST_ETI : enet_001.h
- DMA_ST_FBI : enet_001.h
- DMA_ST_NIS : enet_001.h
- DMA_ST_OVF : enet_001.h
- DMA_ST_RI : enet_001.h
- DMA_ST_RPS : enet_001.h
- DMA_ST_RU : enet_001.h
- DMA_ST_RWT : enet_001.h
- DMA_ST_TI : enet_001.h
- DMA_ST_TJT : enet_001.h
- DMA_ST_TPS : enet_001.h
- DMA_ST_TU : enet_001.h
- DMA_ST_UNF : enet_001.h
- DMA_TIMEOUT : uart.c
- DP8_100BASE_T4 : lpc_phy_dp83848.c
- DP8_100BASE_TX_FD : lpc_phy_dp83848.c
- DP8_100BASE_TX_HD : lpc_phy_dp83848.c
- DP8_10BASE_T_FD : lpc_phy_dp83848.c
- DP8_10BASE_T_HD : lpc_phy_dp83848.c
- DP8_ANADV_REG : lpc_phy_dp83848.c
- DP8_ANEEXP_REG : lpc_phy_dp83848.c
- DP8_ANLPA_REG : lpc_phy_dp83848.c
- DP8_AUTONEG : lpc_phy_dp83848.c
- DP8_AUTONEG_ABILITY : lpc_phy_dp83848.c
- DP8_AUTONEG_COMP : lpc_phy_dp83848.c
- DP8_BMCR_REG : lpc_phy_dp83848.c
- DP8_BMSR_REG : lpc_phy_dp83848.c
- DP8_COLLISION_TEST : lpc_phy_dp83848.c
- DP8_DUPLEX_MODE : lpc_phy_dp83848.c
- DP8_EXTEND_CAPAB : lpc_phy_dp83848.c
- DP8_FULLDUPLEX : lpc_phy_dp83848.c
- DP8_ISOLATE : lpc_phy_dp83848.c
- DP8_JABBER_DETECT : lpc_phy_dp83848.c
- DP8_LINK_STATUS : lpc_phy_dp83848.c
- DP8_LOOPBACK : lpc_phy_dp83848.c
- DP8_MF_PREAMB_SUPPR : lpc_phy_dp83848.c
- DP8_PHY_INT_CTL_REG : lpc_phy_dp83848.c
- DP8_PHY_RBR_REG : lpc_phy_dp83848.c
- DP8_PHY_STAT_REG : lpc_phy_dp83848.c
- DP8_PHY_STS_REG : lpc_phy_dp83848.c
- DP8_PHYID1_OUI : lpc_phy_dp83848.c
- DP8_PHYID2_OUI : lpc_phy_dp83848.c
- DP8_POWER_DOWN : lpc_phy_dp83848.c
- DP8_RBR_RMII_MODE : lpc_phy_dp83848.c
- DP8_REMOTEFAULT : lpc_phy_dp83848.c
- DP8_RESET : lpc_phy_dp83848.c
- DP8_RESTART_AUTONEG : lpc_phy_dp83848.c
- DP8_RMT_FAULT : lpc_phy_dp83848.c
- DP8_SPEED10MBPS : lpc_phy_dp83848.c
- DP8_SPEED_SELECT : lpc_phy_dp83848.c
- DP8_VALID_LINK : lpc_phy_dp83848.c
- DRAM_BASE_ADDRESS : memtest.c
- DRAM_SIZE : memtest.c
- DRIVER_MODE_DMA : uartd_8xx.h
- DRIVER_MODE_INTERRUPT : uartd_8xx.h
- DRIVER_MODE_POLLING : uartd_8xx.h
- DST_PER_CONTROLLER : gpdma_18xx_43xx.h , gpdma_17xx_40xx.h