| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions
board_ngx_xplorer_18304330.h File Reference
`#include "chip.h"`
`#include "board_api.h"`
`#include "lpc_phy.h"`
`#include "uda1380.h"`

Go to the source code of this file.

## Macros
#define | BOARD_NGX_XPLORER_18304330
#define | I2CDEV_UDA1380_ADDR (0x34 >> 1)
#define | UDA1380_I2C_BUS I2C0
#define | LEDS_LED1 0x01
#define | LEDS_LED2 0x02
#define | LEDS_LED3 0x04
#define | LEDS_LED4 0x08
#define | LEDS_NO_LEDS 0x00
#define | BUTTONS_BUTTON1 0x01
#define | JOY_UP 0x01
#define | JOY_DOWN 0x02
#define | JOY_LEFT 0x04
#define | JOY_RIGHT 0x08
#define | JOY_PRESS 0x10
#define | NO_BUTTON_PRESSED 0x00
#define | BUTTONS_BUTTON1_GPIO_PORT_NUM 0
#define | BUTTONS_BUTTON1_GPIO_BIT_NUM 7
#define | LED1_GPIO_PORT_NUM 1
#define | LED1_GPIO_BIT_NUM 11
#define | LED2_GPIO_PORT_NUM 1
#define | LED2_GPIO_BIT_NUM 12

## Functions
void | Board_I2C_Init (I2C_ID_T id)
| Sets up board specific I2C interface.
STATIC INLINE void | Board_I2C_EnableFastPlus (I2C_ID_T id)
| Sets up I2C Fast Plus mode.
STATIC INLINE void | Board_I2C_DisableFastPlus (I2C_ID_T id)
| Disable I2C Fast Plus mode and enables default mode.
void | Board_GPIO_Int_Init (void)
| Initializes board specific GPIO Interrupt.
void | Board_SSP_Init (LPC_SSP_T *pSSP)
| Initialize pin muxing for SSP interface.
void | Board_ENET_GetMacADDR (uint8_t *mcaddr)
| Returns the MAC address assigned to this board.
void | Board_SDMMC_Init (void)
| Initialize pin muxing for SDMMC interface.
void | Board_Buttons_Init (void)
| Initialize button(s) interface on board.
void | Board_Joystick_Init (void)
| Initialize joystick interface on board.
uint8_t | Joystick_GetStatus (void)
| Returns joystick states on board.
uint32_t | Buttons_GetStatus (void)
| Returns button(s) state on board.
void | Board_Audio_Init (LPC_I2S_T *pI2S, int micIn)
| Initialize I2S interface for the board and UDA1380.
void | Serial_CreateStream (void *Stream)
| FIXME.
void | Board_UART_Init (LPC_USART_T *pUART)
| Initialize pin muxing for a UART.