| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
rtc_18xx_43xx.h File Reference

Go to the source code of this file.

## Functions
void | Chip_RTC_Init (LPC_RTC_T *pRTC)
| Initialize the RTC peripheral.
STATIC INLINE void | Chip_RTC_DeInit (LPC_RTC_T *pRTC)
| De-initialize the RTC peripheral.
STATIC INLINE void | Chip_RTC_ResetClockTickCounter (LPC_RTC_T *pRTC)
| Reset clock tick counter in the RTC peripheral.
STATIC INLINE void | Chip_RTC_Enable (LPC_RTC_T *pRTC, FunctionalState NewState)
| Start/Stop RTC peripheral.
STATIC INLINE void | Chip_RTC_CntIncrIntConfig (LPC_RTC_T *pRTC, uint32_t cntrMask, FunctionalState NewState)
| Enable/Disable Counter increment interrupt for a time type in the RTC peripheral.
STATIC INLINE void | Chip_RTC_AlarmIntConfig (LPC_RTC_T *pRTC, uint32_t alarmMask, FunctionalState NewState)
| Enable/Disable Alarm interrupt for a time type in the RTC peripheral.
STATIC INLINE void | Chip_RTC_SetTime (LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t TimeValue)
| Set current time value for a time type in the RTC peripheral.
STATIC INLINE uint32_t | Chip_RTC_GetTime (LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
| Get current time value for a type time type.
STATIC INLINE void | Chip_RTC_SetFullTime (LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Set full time in the RTC peripheral.
STATIC INLINE void | Chip_RTC_GetFullTime (LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Get full time from the RTC peripheral.
STATIC INLINE void | Chip_RTC_SetAlarmTime (LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t ALValue)
| Set alarm time value for a time type.
STATIC INLINE uint32_t | Chip_RTC_GetAlarmTime (LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
| Get alarm time value for a time type.
STATIC INLINE void | Chip_RTC_SetFullAlarmTime (LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Set full alarm time in the RTC peripheral.
STATIC INLINE void | Chip_RTC_GetFullAlarmTime (LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Get full alarm time in the RTC peripheral.
STATIC INLINE void | Chip_REGFILE_Write (LPC_REGFILE_T *pRegFile, uint8_t index, uint32_t Value)
| Write value to General purpose registers.
STATIC INLINE uint32_t | Chip_REGFILE_Read (LPC_REGFILE_T *pRegFile, uint8_t index)
| Read value from General purpose registers.
STATIC INLINE void | Chip_RTC_CalibCounterCmd (LPC_RTC_T *pRTC, FunctionalState NewState)
| Enable/Disable calibration counter in the RTC peripheral.
STATIC INLINE void | Chip_RTC_CalibConfig (LPC_RTC_T *pRTC, uint32_t CalibValue, uint8_t CalibDir)
| Configures Calibration in the RTC peripheral.
STATIC INLINE void | Chip_RTC_ClearIntPending (LPC_RTC_T *pRTC, uint32_t IntType)
| Clear specified Location interrupt pending in the RTC peripheral.
STATIC INLINE IntStatus | Chip_RTC_GetIntPending (LPC_RTC_T *pRTC, uint32_t IntType)
| Check whether if specified location interrupt in the RTC peripheral is set or not.