| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions | Variables
BOARD: PHY status and control driver for the DP83848
BOARD: Board specific PHY drivers

## Detailed Description

Various functions for controlling and monitoring the status of the DP83848 PHY.

## Macros
#define | DP8_BMCR_REG 0x0
| DP83848 PHY register offsets.
#define | DP8_BMSR_REG 0x1
#define | DP8_ANADV_REG 0x4
#define | DP8_ANLPA_REG 0x5
#define | DP8_ANEEXP_REG 0x6
#define | DP8_PHY_STAT_REG 0x10
#define | DP8_PHY_INT_CTL_REG 0x11
#define | DP8_PHY_RBR_REG 0x17
#define | DP8_PHY_STS_REG 0x19
#define | DP8_RESET (1 << 15)
#define | DP8_LOOPBACK (1 << 14)
#define | DP8_SPEED_SELECT (1 << 13)
#define | DP8_AUTONEG (1 << 12)
#define | DP8_POWER_DOWN (1 << 11)
#define | DP8_ISOLATE (1 << 10)
#define | DP8_RESTART_AUTONEG (1 << 9)
#define | DP8_DUPLEX_MODE (1 << 8)
#define | DP8_COLLISION_TEST (1 << 7)
#define | DP8_100BASE_T4 (1 << 15)
#define | DP8_100BASE_TX_FD (1 << 14)
#define | DP8_100BASE_TX_HD (1 << 13)
#define | DP8_10BASE_T_FD (1 << 12)
#define | DP8_10BASE_T_HD (1 << 11)
#define | DP8_MF_PREAMB_SUPPR (1 << 6)
#define | DP8_AUTONEG_COMP (1 << 5)
#define | DP8_RMT_FAULT (1 << 4)
#define | DP8_AUTONEG_ABILITY (1 << 3)
#define | DP8_LINK_STATUS (1 << 2)
#define | DP8_JABBER_DETECT (1 << 1)
#define | DP8_EXTEND_CAPAB (1 << 0)
#define | DP8_RBR_RMII_MODE (1 << 5)
#define | DP8_REMOTEFAULT (1 << 6)
#define | DP8_FULLDUPLEX (1 << 2)
#define | DP8_SPEED10MBPS (1 << 1)
#define | DP8_VALID_LINK (1 << 0)
#define | DP8_PHYID1_OUI 0x2000
#define | DP8_PHYID2_OUI 0x5c90

## Functions
static Status | lpc_mii_write (uint8_t reg, uint16_t data)
static Status | lpc_mii_read (uint8_t reg, uint16_t *data)
static void | lpc_update_phy_sts (uint16_t linksts)
uint32_t | lpc_phy_init (bool rmii, p_msDelay_func_t pDelayMsFunc)
| Initialize the PHY.
uint32_t | lpcPHYStsPoll (void)
| Phy status update state machine.

## Variables
static uint32_t | physts
static uint32_t | olddphysts
static int32_t | phyustate
static p_msDelay_func_t | pDelayMs

## Macro Definition Documentation

#define DP8_100BASE_T4 (1 << 15)

T4 mode

Definition at line 65 of file lpc_phy_dp83848.c.

#define DP8_100BASE_TX_FD (1 << 14)

100MBps full duplex

Definition at line 66 of file lpc_phy_dp83848.c.

#define DP8_100BASE_TX_HD (1 << 13)

100MBps half duplex

Definition at line 67 of file lpc_phy_dp83848.c.

#define DP8_10BASE_T_FD (1 << 12)

100Bps full duplex

Definition at line 68 of file lpc_phy_dp83848.c.

#define DP8_10BASE_T_HD (1 << 11)

10MBps half duplex

Definition at line 69 of file lpc_phy_dp83848.c.

#define DP8_ANADV_REG 0x4

Auto_Neg Advt Reg

Definition at line 45 of file lpc_phy_dp83848.c.

#define DP8_ANEEXP_REG 0x6

Auto-neg Expansion Reg

Definition at line 47 of file lpc_phy_dp83848.c.

#define DP8_ANLPA_REG 0x5

Auto_neg Link Partner Ability Reg

Definition at line 46 of file lpc_phy_dp83848.c.

#define DP8_AUTONEG (1 << 12)

1=Enable auto-negotiation

Definition at line 57 of file lpc_phy_dp83848.c.

#define DP8_AUTONEG_ABILITY (1 << 3)

Auto-negotation supported

Definition at line 73 of file lpc_phy_dp83848.c.

#define DP8_AUTONEG_COMP (1 << 5)

Auto-negotation complete

Definition at line 71 of file lpc_phy_dp83848.c.

#define DP8_BMCR_REG 0x0

DP83848 PHY register offsets.

Basic Mode Control Register

Definition at line 43 of file lpc_phy_dp83848.c.

#define DP8_BMSR_REG 0x1

Basic Mode Status Reg

Definition at line 44 of file lpc_phy_dp83848.c.

#define DP8_COLLISION_TEST (1 << 7)

1=Perform collsion test

Definition at line 62 of file lpc_phy_dp83848.c.

#define DP8_DUPLEX_MODE (1 << 8)

1=Full duplex mode

Definition at line 61 of file lpc_phy_dp83848.c.

#define DP8_EXTEND_CAPAB (1 << 0)

Supports extended capabilities

Definition at line 76 of file lpc_phy_dp83848.c.

#define DP8_FULLDUPLEX (1 << 2)

1=full duplex

Definition at line 83 of file lpc_phy_dp83848.c.

#define DP8_ISOLATE (1 << 10)

1=Isolate PHY

Definition at line 59 of file lpc_phy_dp83848.c.

#define DP8_JABBER_DETECT (1 << 1)

Jabber detect

Definition at line 75 of file lpc_phy_dp83848.c.

#define DP8_LINK_STATUS (1 << 2)

1=Link active

Definition at line 74 of file lpc_phy_dp83848.c.

#define DP8_LOOPBACK (1 << 14)

1=loopback Enabled

Definition at line 55 of file lpc_phy_dp83848.c.

#define DP8_MF_PREAMB_SUPPR (1 << 6)

Preamble suppress

Definition at line 70 of file lpc_phy_dp83848.c.

#define DP8_PHY_INT_CTL_REG 0x11

PHY Interrupt Control Register

Definition at line 49 of file lpc_phy_dp83848.c.

#define DP8_PHY_RBR_REG 0x17

PHY RMII and Bypass Register

Definition at line 50 of file lpc_phy_dp83848.c.

#define DP8_PHY_STAT_REG 0x10

PHY Status Register

Definition at line 48 of file lpc_phy_dp83848.c.

#define DP8_PHY_STS_REG 0x19

PHY Status Register

Definition at line 51 of file lpc_phy_dp83848.c.

#define DP8_PHYID1_OUI 0x2000

Expected PHY ID1

Definition at line 88 of file lpc_phy_dp83848.c.

#define DP8_PHYID2_OUI 0x5c90

Expected PHY ID2

Definition at line 89 of file lpc_phy_dp83848.c.

#define DP8_POWER_DOWN (1 << 11)

1=Power down PHY

Definition at line 58 of file lpc_phy_dp83848.c.

#define DP8_RBR_RMII_MODE (1 << 5)

Use RMII mode

Definition at line 79 of file lpc_phy_dp83848.c.

#define DP8_REMOTEFAULT (1 << 6)

Remote fault

Definition at line 82 of file lpc_phy_dp83848.c.

#define DP8_RESET (1 << 15)

1= S/W Reset

Definition at line 54 of file lpc_phy_dp83848.c.

#define DP8_RESTART_AUTONEG (1 << 9)

1=Restart auto-negoatiation

Definition at line 60 of file lpc_phy_dp83848.c.

#define DP8_RMT_FAULT (1 << 4)

Fault

Definition at line 72 of file lpc_phy_dp83848.c.

#define DP8_SPEED10MBPS (1 << 1)

1=10MBps speed

Definition at line 84 of file lpc_phy_dp83848.c.

#define DP8_SPEED_SELECT (1 << 13)

1=Select 100MBps

Definition at line 56 of file lpc_phy_dp83848.c.

#define DP8_VALID_LINK (1 << 0)

1=Link active

Definition at line 85 of file lpc_phy_dp83848.c.

## Function Documentation

static Status lpc_mii_read | ( | uint8_t | reg,
|  | uint16_t * | data
| ) |  |
| static

Definition at line 127 of file lpc_phy_dp83848.c.

static Status lpc_mii_write | ( | uint8_t | reg,
|  | uint16_t | data
| ) |  |
| static

Definition at line 102 of file lpc_phy_dp83848.c.

uint32_t lpc_phy_init | ( | bool | rmii,
|  | p_msDelay_func_t | pDelayMsFunc
| ) |  |

Initialize the PHY.

Parameters

  rmii | : Initializes PHY for RMII mode if true, MII if false
  pDelayMsFunc | : Delay function (in mS) used for this driver

Returns
  PHY_LINK_ERROR or 0 on success

Note
  This function initializes the PHY. It will block until complete. It will not wait for the PHY to detect a connected cable and remain busy. Use lpcPHYStsPoll to detect cable insertion.

Definition at line 187 of file lpc_phy_dp83848.c.

static void lpc_update_phy_sts | ( | uint16_t | linksts | ) |
| static

Definition at line 152 of file lpc_phy_dp83848.c.

uint32_t lpcPHYStsPoll | ( | void |  | ) |

Phy status update state machine.

Returns
  An Or'ed value of PHY_LINK_* statuses

Note
  This function can be called at any rate and will poll the the PHY status. Multiple calls may be needed to determine PHY status.

Definition at line 253 of file lpc_phy_dp83848.c.

## Variable Documentation

uint32_t olddphysts
| static

Definition at line 92 of file lpc_phy_dp83848.c.

p_msDelay_func_t pDelayMs
| static

Definition at line 98 of file lpc_phy_dp83848.c.

uint32_t physts
| static

Definition at line 92 of file lpc_phy_dp83848.c.

int32_t phyustate
| static

Definition at line 95 of file lpc_phy_dp83848.c.