| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_ENET_001_ENHRXDESC_T Struct Reference
IP: Ethernet register block and driver

## Detailed Description

Structure of a enhanced receive descriptor (with timestamp)

Definition at line 443 of file enet_001.h.

`#include "enet_001.h"`

## Data Fields
__IO uint32_t | STATUS
__IO uint32_t | CTRL
__IO uint32_t | B1ADD
__IO uint32_t | B2ADD
__IO uint32_t | EXTSTAT
__IO uint32_t | RDES5
__IO uint32_t | RTSL
__IO uint32_t | RTSH

## Field Documentation

__IO uint32_t B1ADD

Buffer 1 address

Definition at line 446 of file enet_001.h.

__IO uint32_t B2ADD

Buffer 2 or next descriptor address

Definition at line 447 of file enet_001.h.

__IO uint32_t CTRL

Buffer 1/2 byte counts

Definition at line 445 of file enet_001.h.

__IO uint32_t EXTSTAT

Extended Status

Definition at line 448 of file enet_001.h.

__IO uint32_t RDES5

Reserved

Definition at line 449 of file enet_001.h.

__IO uint32_t RTSH

Timestamp value high

Definition at line 451 of file enet_001.h.

__IO uint32_t RTSL

Timestamp value low

Definition at line 450 of file enet_001.h.

__IO uint32_t STATUS

RDES status word

Definition at line 444 of file enet_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/enet_001.h