| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions
LPC18xx/43xx Simple blinky example
Peripheral examples

## Detailed Description

Example description
The Blinky example is known as the "Hello, World!" of embedded programming. This example will flash an LED on your board at a periodic rate and output the timer information on the UART port.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Macros
#define | TICKRATE_HZ 10

## Functions
void | TIMER1_IRQHandler (void)
| Handle interrupt from 32-bit timer.
int | main (void)
| main routine for blinky example

## Macro Definition Documentation

#define TICKRATE_HZ 10

Definition at line 67 of file blinky.c.

## Function Documentation

int main | ( | void |  | ) |

main routine for blinky example

Main program body.

Returns
  Function should not exit.

Definition at line 100 of file blinky.c.

void TIMER1_IRQHandler | ( | void |  | ) |

Handle interrupt from 32-bit timer.

Returns
  Nothing

Definition at line 85 of file blinky.c.