| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
lpc_sdmmc.h
Go to the documentation of this file.
1 /*
2 * @brief Common definitions used in SD/MMC cards
3 * @note
4 * Copyright(C) NXP Semiconductors, 2012
5 * All rights reserved.
6 *
7 * @par
8 * Software that is described herein is for illustrative purposes only
9 * which provides customers with programming information regarding the
10 * LPC products. This software is supplied "AS IS" without any warranties of
11 * any kind, and NXP Semiconductors and its licensor disclaim any and
12 * all warranties, express or implied, including all implied warranties of
13 * merchantability, fitness for a particular purpose and non-infringement of
14 * intellectual property rights. NXP Semiconductors assumes no responsibility
15 * or liability for the use of the software, conveys no license or rights under any
16 * patent, copyright, mask work right, or any other intellectual property rights in
17 * or to any products. NXP Semiconductors reserves the right to make changes
18 * in the software without notification. NXP Semiconductors also makes no
19 * representation or warranty that such application will be suitable for the
20 * specified use without further testing or modification.
21 *
22 * @par
23 * Permission to use, copy, modify, and distribute this software and its
24 * documentation is hereby granted, under NXP Semiconductors' and its
25 * licensor's relevant copyrights in the software, without fee, provided that it
26 * is used in conjunction with NXP Semiconductors microcontrollers. This
27 * copyright, permission, and disclaimer notice must appear in all copies of
28 * this code.
29 */
30
31 #ifndef __LPC_SDMMC_H
32 #define __LPC_SDMMC_H
33
34 #ifdef __cplusplus
35 extern "C" {
36 #endif
37
47 #define SDC_OCR_20_21 (((uint32_t) 1) << 8)
48
49 #define SDC_OCR_21_22 (((uint32_t) 1) << 9)
50
51 #define SDC_OCR_22_23 (((uint32_t) 1) << 10)
52
53 #define SDC_OCR_23_24 (((uint32_t) 1) << 11)
54
55 #define SDC_OCR_24_25 (((uint32_t) 1) << 12)
56
57 #define SDC_OCR_25_26 (((uint32_t) 1) << 13)
58
59 #define SDC_OCR_26_27 (((uint32_t) 1) << 14)
60
61 #define SDC_OCR_27_28 (((uint32_t) 1) << 15)
62
63 #define SDC_OCR_28_29 (((uint32_t) 1) << 16)
64
65 #define SDC_OCR_29_30 (((uint32_t) 1) << 17)
66
67 #define SDC_OCR_30_31 (((uint32_t) 1) << 18)
68
69 #define SDC_OCR_31_32 (((uint32_t) 1) << 19)
70
71 #define SDC_OCR_32_33 (((uint32_t) 1) << 20)
72
73 #define SDC_OCR_33_34 (((uint32_t) 1) << 21)
74
75 #define SDC_OCR_34_35 (((uint32_t) 1) << 22)
76
77 #define SDC_OCR_35_36 (((uint32_t) 1) << 23)
78
79 #define SDC_OCR_27_36 ((uint32_t) 0x00FF8000)
80
81 #define SDC_OCR_HC_CCS (((uint32_t) 1) << 30)
82
83 #define SDC_OCR_IDLE (((uint32_t) 1) << 31)
84 #define SDC_OCR_BUSY (((uint32_t) 0) << 31)
85
86 /* SD/MMC commands - this matrix shows the command, response types, and
87 supported card type for that command.
88 Command Number Resp SD MMC
89 ----------------------- ------ ----- --- ---
90 Reset (go idle) CMD0 NA x x
91 Send op condition CMD1 R3 x
92 All send CID CMD2 R2 x x
93 Send relative address CMD3 R1 x
94 Send relative address CMD3 R6 x
95 Program DSR CMD4 NA x
96 Select/deselect card CMD7 R1b x
97 Select/deselect card CMD7 R1 x
98 Send CSD CMD9 R2 x x
99 Send CID CMD10 R2 x x
100 Read data until stop CMD11 R1 x x
101 Stop transmission CMD12 R1/b x x
102 Send status CMD13 R1 x x
103 Go inactive state CMD15 NA x x
104 Set block length CMD16 R1 x x
105 Read single block CMD17 R1 x x
106 Read multiple blocks CMD18 R1 x x
107 Write data until stop CMD20 R1 x
108 Setblock count CMD23 R1 x
109 Write single block CMD24 R1 x x
110 Write multiple blocks CMD25 R1 x x
111 Program CID CMD26 R1 x
112 Program CSD CMD27 R1 x x
113 Set write protection CMD28 R1b x x
114 Clear write protection CMD29 R1b x x
115 Send write protection CMD30 R1 x x
116 Erase block start CMD32 R1 x
117 Erase block end CMD33 R1 x
118 Erase block start CMD35 R1 x
119 Erase block end CMD36 R1 x
120 Erase blocks CMD38 R1b x
121 Fast IO CMD39 R4 x
122 Go IRQ state CMD40 R5 x
123 Lock/unlock CMD42 R1b x
124 Application command CMD55 R1 x
125 General command CMD56 R1b x
126
127 *** SD card application commands - these must be preceded with ***
128 *** MMC CMD55 application specific command first ***
129 Set bus width ACMD6 R1 x
130 Send SD status ACMD13 R1 x
131 Send number WR blocks ACMD22 R1 x
132 Set WR block erase cnt ACMD23 R1 x
133 Send op condition ACMD41 R3 x
134 Set clear card detect ACMD42 R1 x
135 Send CSR ACMD51 R1 x */
136
141 typedef enum {
142 SD_SET_BUS_WIDTH,
143 SD_SEND_STATUS,
144 SD_SEND_WR_BLOCKS,
145 SD_SET_ERASE_COUNT,
146 SD_SENDOP_COND,
147 SD_CLEAR_CARD_DET,
148 SD_SEND_SCR,
149 SD_INVALID_APP_CMD
150 } SD_APP_CMD_T;
151
155 typedef enum {
156 SDMMC_RESPONSE_R1,
157 SDMMC_RESPONSE_R1B,
158 SDMMC_RESPONSE_R2,
159 SDMMC_RESPONSE_R3,
160 SDMMC_RESPONSE_R4,
161 SDMMC_RESPONSE_R5,
162 SDMMC_RESPONSE_R6,
163 SDMMC_RESPONSE_NONE
164 } SDMMC_RESPONSE_T;
165
169 typedef enum {
170 SDMMC_IDLE_ST = 0,
171 SDMMC_READY_ST,
172 SDMMC_IDENT_ST,
173 SDMMC_STBY_ST,
174 SDMMC_TRAN_ST,
175 SDMMC_DATA_ST,
176 SDMMC_RCV_ST,
177 SDMMC_PRG_ST,
178 SDMMC_DIS_ST
179 } SDMMC_STATE_T;
180
181 /* Function prototype for event setup function */
182 typedef void (*SDMMC_EVSETUP_FUNC_T)(void *);
183
184 /* Function prototype for wait for event function */
185 typedef uint32_t (*SDMMC_EVWAIT_FUNC_T)(void);
186
187 /* Function prototype for milliSecond delay function */
188 typedef void (*SDMMC_MSDELAY_FUNC_T)(uint32_t);
189
193 typedef struct {
194 uint32_t response[4];
195 uint32_t cid[4];
196 uint32_t csd[4];
197 uint32_t ext_csd[512 / 4];
198 uint32_t card_type;
199 uint16_t rca;
200 uint32_t speed;
201 uint32_t block_len;
202 uint32_t device_size;
203 uint32_t blocknr;
204 uint32_t clk_rate;
205 SDMMC_EVSETUP_FUNC_T evsetup_cb;
206 SDMMC_EVWAIT_FUNC_T waitfunc_cb;
207 SDMMC_MSDELAY_FUNC_T msdelay_func;
208 } SDMMC_CARD_T;
209
214 /* class 1 */
215 #define MMC_GO_IDLE_STATE 0 /* bc */
216 #define MMC_SEND_OP_COND 1 /* bcr [31:0] OCR R3 */
217 #define MMC_ALL_SEND_CID 2 /* bcr R2 */
218 #define MMC_SET_RELATIVE_ADDR 3 /* ac [31:16] RCA R1 */
219 #define MMC_SET_DSR 4 /* bc [31:16] RCA */
220 #define MMC_SELECT_CARD 7 /* ac [31:16] RCA R1 */
221 #define MMC_SEND_EXT_CSD 8 /* bc R1 */
222 #define MMC_SEND_CSD 9 /* ac [31:16] RCA R2 */
223 #define MMC_SEND_CID 10 /* ac [31:16] RCA R2 */
224 #define MMC_STOP_TRANSMISSION 12 /* ac R1b */
225 #define MMC_SEND_STATUS 13 /* ac [31:16] RCA R1 */
226 #define MMC_GO_INACTIVE_STATE 15 /* ac [31:16] RCA */
227
228 /* class 2 */
229 #define MMC_SET_BLOCKLEN 16 /* ac [31:0] block len R1 */
230 #define MMC_READ_SINGLE_BLOCK 17 /* adtc [31:0] data addr R1 */
231 #define MMC_READ_MULTIPLE_BLOCK 18 /* adtc [31:0] data addr R1 */
232
233 /* class 3 */
234 #define MMC_WRITE_DAT_UNTIL_STOP 20 /* adtc [31:0] data addr R1 */
235
236 /* class 4 */
237 #define MMC_SET_BLOCK_COUNT 23 /* adtc [31:0] data addr R1 */
238 #define MMC_WRITE_BLOCK 24 /* adtc [31:0] data addr R1 */
239 #define MMC_WRITE_MULTIPLE_BLOCK 25 /* adtc R1 */
240 #define MMC_PROGRAM_CID 26 /* adtc R1 */
241 #define MMC_PROGRAM_CSD 27 /* adtc R1 */
242
243 /* class 6 */
244 #define MMC_SET_WRITE_PROT 28 /* ac [31:0] data addr R1b */
245 #define MMC_CLR_WRITE_PROT 29 /* ac [31:0] data addr R1b */
246 #define MMC_SEND_WRITE_PROT 30 /* adtc [31:0] wpdata addr R1 */
247
248 /* class 5 */
249 #define MMC_ERASE_GROUP_START 35 /* ac [31:0] data addr R1 */
250 #define MMC_ERASE_GROUP_END 36 /* ac [31:0] data addr R1 */
251 #define MMC_ERASE 37 /* ac R1b */
252 #define SD_ERASE_WR_BLK_START 32 /* ac [31:0] data addr R1 */
253 #define SD_ERASE_WR_BLK_END 33 /* ac [31:0] data addr R1 */
254 #define SD_ERASE 38 /* ac R1b */
255
256 /* class 9 */
257 #define MMC_FAST_IO 39 /* ac <Complex> R4 */
258 #define MMC_GO_IRQ_STATE 40 /* bcr R5 */
259
260 /* class 7 */
261 #define MMC_LOCK_UNLOCK 42 /* adtc R1b */
262
263 /* class 8 */
264 #define MMC_APP_CMD 55 /* ac [31:16] RCA R1 */
265 #define MMC_GEN_CMD 56 /* adtc [0] RD/WR R1b */
266
267 /* SD commands type argument response */
268 /* class 8 */
269 /* This is basically the same command as for MMC with some quirks. */
270 #define SD_SEND_RELATIVE_ADDR 3 /* ac R6 */
271 #define SD_CMD8 8 /* bcr [31:0] OCR R3 */
272
273 /* Application commands */
274 #define SD_APP_SET_BUS_WIDTH 6 /* ac [1:0] bus width R1 */
275 #define SD_APP_OP_COND 41 /* bcr [31:0] OCR R1 (R4) */
276 #define SD_APP_SEND_SCR 51 /* adtc R1 */
277
293 #define R1_OUT_OF_RANGE (1UL << 31) /* er, c */
294 #define R1_ADDRESS_ERROR (1 << 30) /* erx, c */
295 #define R1_BLOCK_LEN_ERROR (1 << 29) /* er, c */
296 #define R1_ERASE_SEQ_ERROR (1 << 28) /* er, c */
297 #define R1_ERASE_PARAM (1 << 27) /* ex, c */
298 #define R1_WP_VIOLATION (1 << 26) /* erx, c */
299 #define R1_CARD_IS_LOCKED (1 << 25) /* sx, a */
300 #define R1_LOCK_UNLOCK_FAILED (1 << 24) /* erx, c */
301 #define R1_COM_CRC_ERROR (1 << 23) /* er, b */
302 #define R1_ILLEGAL_COMMAND (1 << 22) /* er, b */
303 #define R1_CARD_ECC_FAILED (1 << 21) /* ex, c */
304 #define R1_CC_ERROR (1 << 20) /* erx, c */
305 #define R1_ERROR (1 << 19) /* erx, c */
306 #define R1_UNDERRUN (1 << 18) /* ex, c */
307 #define R1_OVERRUN (1 << 17) /* ex, c */
308 #define R1_CID_CSD_OVERWRITE (1 << 16) /* erx, c, CID/CSD overwrite */
309 #define R1_WP_ERASE_SKIP (1 << 15) /* sx, c */
310 #define R1_CARD_ECC_DISABLED (1 << 14) /* sx, a */
311 #define R1_ERASE_RESET (1 << 13) /* sr, c */
312 #define R1_STATUS(x) (x & 0xFFFFE000)
313 #define R1_CURRENT_STATE(x) ((x & 0x00001E00) >> 9) /* sx, b (4 bits) */
314 #define R1_READY_FOR_DATA (1 << 8) /* sx, a */
315 #define R1_APP_CMD (1 << 5) /* sr, c */
316
320 #define OCR_ALL_READY (1UL << 31) /* Card Power up status bit */
321 #define OCR_HC_CCS (1 << 30) /* High capacity card */
322 #define OCR_VOLTAGE_RANGE_MSK (0x00FF8000)
323
324 #define SD_SEND_IF_ARG 0x000001AA
325 #define SD_SEND_IF_ECHO_MSK 0x000000FF
326 #define SD_SEND_IF_RESP 0x000000AA
327
331 #define CMDRESP_R3_OCR_VAL(n) (((uint32_t) n) & 0xFFFFFF)
332 #define CMDRESP_R3_S18A (((uint32_t) 1 ) << 24)
333 #define CMDRESP_R3_HC_CCS (((uint32_t) 1 ) << 30)
334 #define CMDRESP_R3_INIT_COMPLETE (((uint32_t) 1 ) << 31)
335
339 #define CMDRESP_R6_RCA_VAL(n) (((uint32_t) (n >> 16)) & 0xFFFF)
340 #define CMDRESP_R6_CARD_STATUS(n) (((uint32_t) (n & 0x1FFF)) | \
341 ((n & (1 << 13)) ? (1 << 19) : 0) | \
342 ((n & (1 << 14)) ? (1 << 22) : 0) | \
343 ((n & (1 << 15)) ? (1 << 23) : 0))
344
349 #define CMDRESP_R7_CHECK_PATTERN(n) (((uint32_t) n ) & 0xFF)
350
351 #define CMDRESP_R7_VOLTAGE_ACCEPTED (((uint32_t) 1 ) << 8)
352
357 #define CMD3_RCA(n) (((uint32_t) (n & 0xFFFF) ) << 16)
358
363 #define CMD7_RCA(n) (((uint32_t) (n & 0xFFFF) ) << 16)
364
369 #define CMD8_CHECKPATTERN(n) (((uint32_t) (n & 0xFF) ) << 0)
370
371 #define CMD8_DEF_PATTERN (0xAA)
372
373 #define CMD8_VOLTAGESUPPLIED_27_36 (((uint32_t) 1 ) << 8)
374
378 #define CMD9_RCA(n) (((uint32_t) (n & 0xFFFF) ) << 16)
379
383 #define CMD13_RCA(n) (((uint32_t) (n & 0xFFFF) ) << 16)
384
388 #define CMD55_RCA(n) (((uint32_t) (n & 0xFFFF) ) << 16)
389
393 #define ACMD41_OCR(n) (((uint32_t) n) & 0xFFFFFF)
394 #define ACMD41_S18R (((uint32_t) 1 ) << 24)
395 #define ACMD41_XPC (((uint32_t) 1 ) << 28)
396 #define ACMD41_HCS (((uint32_t) 1 ) << 30)
397
401 #define ACMD6_BUS_WIDTH(n) ((uint32_t) n & 0x03)
402 #define ACMD6_BUS_WIDTH_1 (0)
403 #define ACMD6_BUS_WIDTH_4 (2)
404
407 #define CARD_TYPE_SD (1 << 0)
408 #define CARD_TYPE_4BIT (1 << 1)
409 #define CARD_TYPE_8BIT (1 << 2)
410 #define CARD_TYPE_HC (OCR_HC_CCS)
415 #define MMC_SECTOR_SIZE 512
416
417 #ifdef __cplusplus
418 }
419 #endif
420
425 #endif /* __LPC_SDMMC_H */