| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
emc_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx EMC driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __EMC_17XX_40XX_H_
33 #define __EMC_17XX_40XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
50 #define EMC_ADDRESS_DYCS0 (0xA0000000)
51 #define EMC_ADDRESS_DYCS1 (0xB0000000)
52 #define EMC_ADDRESS_DYCS2 (0xC0000000)
53 #define EMC_ADDRESS_DYCS3 (0xD0000000)
54
58 #define EMC_ADDRESS_CS0 (0x80000000)
59 #define EMC_ADDRESS_CS1 (0x90000000)
60 #define EMC_ADDRESS_CS2 (0x98000000)
61 #define EMC_ADDRESS_CS3 (0x9C000000)
62
68 void Chip_EMC_Dynamic_Init(IP_EMC_DYN_CONFIG_T *Dynamic_Config);
69
75 void Chip_EMC_Static_Init(IP_EMC_STATIC_CONFIG_T *Static_Config);
76
82 STATIC INLINE void Chip_EMC_Dynamic_Enable(uint8_t Enable)
83 {
84 IP_EMC_Dynamic_Enable(LPC_EMC, Enable);
85 }
86
92 STATIC INLINE void Chip_EMC_Mirror(uint8_t Enable)
93 {
94 IP_EMC_Mirror(LPC_EMC, Enable);
95 }
96
102 STATIC INLINE void Chip_EMC_Enable(uint8_t Enable)
103 {
104 IP_EMC_Enable(LPC_EMC, Enable);
105 }
106
114 STATIC INLINE void Chip_EMC_LowPowerMode(uint8_t Enable)
115 {
116 IP_EMC_LowPowerMode(LPC_EMC, Enable);
117 }
118
126 STATIC INLINE void Chip_EMC_Init(uint32_t Enable, uint32_t ClockRatio, uint32_t EndianMode)
127 {
128 IP_EMC_Init(LPC_EMC, Enable, ClockRatio, EndianMode);
129 }
130
136 STATIC INLINE void Chip_EMC_SetStaticExtendedWait(uint32_t Wait16Clks)
137 {
138 IP_EMC_SetStaticExtendedWait(LPC_EMC, Wait16Clks);
139 }
140
145 #ifdef __cplusplus
146 }
147 #endif
148
149 #endif /* __EMC_17XX_40XX_H_ */