| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Mouse Device
USB examples

## Detailed Description

Example description
This example implements a HID device which is used for mouse configuration.

When the example is run and the board is connected to a PC with a USB cable it will enumerate on the PC as a HID mouse device and the joystick (SW2) on the EA Baseboard will generate mouse movement on your PC.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Main definitions
| ROM stack support