| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
LPC18xx/43xx State Configurable Timer Blinky example
Misc examples

## Detailed Description

Example description
This example implements the Blinky example using State Configurable Timer module. The FSM is built by using FZM tool. The FZM tool can be downloded from :
SCT Tools

Special connection requirements

- Hitex LPC1850EVA-A4-2 and LPC4350EVA-A4-2 boards
  Make sure that the jumper JP34 is in 2-3 position for SCTIN_1
- Keil MCB1857 and MCB4357 boards

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
void | SCT_PinsConfigure (void)
void | SCT_IRQHandler (void)
| SCT interrupt handler.
int | main (void)
| Main entry point.

## Function Documentation

int main | ( | void |  | ) |

Main entry point.

Main program body.

Returns
  Nothing

Definition at line 142 of file sct_blinky.c.

void SCT_IRQHandler | ( | void |  | ) |

SCT interrupt handler.

Returns
  Nothing

Definition at line 135 of file sct_blinky.c.

void SCT_PinsConfigure | ( | void |  | ) |

Definition at line 83 of file sct_blinky.c.