| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
BOARD: LPC1850 Hitex EVA board builds options
LPC1850 and LPC4350 Hitex EVA board support functions

## Detailed Description

This board has options that configure its operation at build-time.

For more information on driver options see
LPCOpen platform design approach and goals

## Macro Definition Documentation

#define CGU_AUDIO_PLL_RATE (0)

Definition at line 66 of file sys_config.h.

#define CGU_USB_PLL_RATE (480000000)

Definition at line 67 of file sys_config.h.

#define CHIP_LPC18XX

Definition at line 38 of file sys_config.h.

#define CRYSTAL_32K_FREQ_IN 32768

Definition at line 57 of file sys_config.h.

#define CRYSTAL_MAIN_FREQ_IN 12000000

Definition at line 54 of file sys_config.h.

#define DEBUG_ENABLE

Definition at line 44 of file sys_config.h.

#define DEBUG_UART LPC_USART0

Definition at line 51 of file sys_config.h.

#define EXTERNAL_CLKIN_FREQ_IN 0

Definition at line 60 of file sys_config.h.

#define MAX_CLOCK_FREQ (180000000)

Definition at line 63 of file sys_config.h.