| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
i2s_17xx_40xx.c File Reference
`#include "chip.h"`

Go to the source code of this file.

## Functions
void | Chip_I2S_Init (LPC_I2S_T *pI2S)
| Initialize for I2S.
void | Chip_I2S_DeInit (LPC_I2S_T *pI2S)
| Shutdown I2S.
Status | Chip_I2S_Config (LPC_I2S_T *pI2S, uint8_t TRMode, Chip_I2S_Audio_Format_T *audio_format)
| Configure I2S for Audio Format input.
void | Chip_I2S_Int_Cmd (LPC_I2S_T *pI2S, uint8_t TRMode, FunctionalState NewState, uint8_t FIFO_Depth)
| Enable/Disable Interrupt with a specific FIFO depth.
void | Chip_I2S_DMA_Cmd (LPC_I2S_T *pI2S, uint8_t TRMode, uint8_t DMANum, FunctionalState NewState, uint8_t FIFO_Depth)
| Enable/Disable DMA with a specific FIFO depth.