| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Miscellaneous LPCOpen device benchmarks

LWIP benchmarks using LPCOpen examples
LWIP benchmarks on LPC devices

SD card benchmarks using LPCOpen examples for LPC18xx/43xx device family
LPC18xx/43xx benchmarks were made using the 'app_sdmmc_meas' example included in the LPC18xx/43xx example area of the LPCopen platform. The tests were performed with code running from IRAM or FLASH and use a Transcend 32GB SDHC class 4 card (not exactly the fastest card).

Hitex LPC1850/LPC4350 boards
Hitex LPC1850/LPC4350 boards running from SPI FLASH (approximate speed)

    READ: Ave Time: 1911 usecs Ave Speed : 4286 KB/sec
    WRITE:Ave Time: 4023 usecs Ave Speed : 2036 KB/sec

Hitex LPC1850/LPC4350 boards running from IRAM (approximate speed)

    READ: Ave Time: 114400 usecs Ave Speed : 9165 KB/sec
    WRITE:Ave Time: 116198 usecs Ave Speed : 9024 KB/sec

SD card benchmarks using LPCOpen examples for LPC17xx/40xx device family
LPC17xx/40xx benchmarks were made using the 'app_sdmmc_meas' example included in the LPC17xx/40xx example area of the LPCopen platform. The tests were performed with code running from IRAM or FLASH and use a Transcend 32GB SDHC class 4 card (not exactly the fastest card).

Embedded Artists LPC1788/4088 boards
Not available yet.