| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Enumerations | Functions
rtc_001.h File Reference
`#include "sys_config.h"`
`#include "cmsis.h"`

Go to the source code of this file.

## Data Structures
struct | IP_RTC_001_T
| Real Time Clock register block structure. More...
struct | IP_RTC_TIME_T

## Macros
#define | RTC_ILR_BITMASK ((0x00000003))
| ILR register definitions.
#define | RTC_IRL_RTCCIF ((1 << 0))
#define | RTC_IRL_RTCALF ((1 << 1))
#define | RTC_CCR_BITMASK ((0x00000013))
| CCR register definitions.
#define | RTC_CCR_CLKEN ((1 << 0))
#define | RTC_CCR_CTCRST ((1 << 1))
#define | RTC_CCR_CCALEN ((1 << 4))
#define | RTC_AMR_CIIR_IMSEC ((1 << 0))
| CIIR and AMR register definitions.
#define | RTC_AMR_CIIR_IMMIN ((1 << 1))
#define | RTC_AMR_CIIR_IMHOUR ((1 << 2))
#define | RTC_AMR_CIIR_IMDOM ((1 << 3))
#define | RTC_AMR_CIIR_IMDOW ((1 << 4))
#define | RTC_AMR_CIIR_IMDOY ((1 << 5))
#define | RTC_AMR_CIIR_IMMON ((1 << 6))
#define | RTC_AMR_CIIR_IMYEAR ((1 << 7))
#define | RTC_AMR_CIIR_BITMASK ((0xFF))
#define | RTC_AUX_RTC_OSCF ((1 << 4))
| RTC_AUX register definitions.
#define | RTC_AUXEN_RTC_OSCFEN ((1 << 4))
| RTC_AUXEN register definitions.
#define | RTC_CTIME0_SECONDS_MASK ((0x3F))
| Consolidated Time Register 0 definitions.
#define | RTC_CTIME0_MINUTES_MASK ((0x3F00))
#define | RTC_CTIME0_HOURS_MASK ((0x1F0000))
#define | RTC_CTIME0_DOW_MASK ((0x7000000))
#define | RTC_CTIME1_DOM_MASK ((0x1F))
| Consolidated Time Register 1 definitions.
#define | RTC_CTIME1_MONTH_MASK ((0xF00))
#define | RTC_CTIME1_YEAR_MASK ((0xFFF0000))
#define | RTC_CTIME2_DOY_MASK ((0xFFF))
| Consolidated Time Register 2 definitions.
#define | RTC_SEC_MASK (0x0000003F)
| Time Counter Group and Alarm register group.
#define | RTC_MIN_MASK (0x0000003F)
#define | RTC_HOUR_MASK (0x0000001F)
#define | RTC_DOM_MASK (0x0000001F)
#define | RTC_DOW_MASK (0x00000007)
#define | RTC_DOY_MASK (0x000001FF)
#define | RTC_MONTH_MASK (0x0000000F)
#define | RTC_YEAR_MASK (0x00000FFF)
#define | RTC_SECOND_MAX 59
#define | RTC_MINUTE_MAX 59
#define | RTC_HOUR_MAX 23
#define | RTC_MONTH_MIN 1
#define | RTC_MONTH_MAX 12
#define | RTC_DAYOFMONTH_MIN 1
#define | RTC_DAYOFMONTH_MAX 31
#define | RTC_DAYOFWEEK_MAX 6
#define | RTC_DAYOFYEAR_MIN 1
#define | RTC_DAYOFYEAR_MAX 366
#define | RTC_YEAR_MAX 4095
#define | RTC_CALIBRATION_CALVAL_MASK ((0x1FFFF))
| Calibration register.
#define | RTC_CALIBRATION_LIBDIR ((1 << 17))
#define | RTC_CALIBRATION_MAX ((0x20000))
#define | RTC_CALIB_DIR_FORWARD ((uint8_t) (0))
#define | RTC_CALIB_DIR_BACKWARD ((uint8_t) (1))

## Enumerations
enum | IP_RTC_TIMEINDEX_T { RTC_TIMETYPE_SECOND, RTC_TIMETYPE_MINUTE, RTC_TIMETYPE_HOUR, RTC_TIMETYPE_DAYOFMONTH, RTC_TIMETYPE_DAYOFWEEK, RTC_TIMETYPE_DAYOFYEAR, RTC_TIMETYPE_MONTH, RTC_TIMETYPE_YEAR, RTC_TIMETYPE_LAST }
| RTC time type option. More...
enum | IP_RTC_INT_OPT_T { RTC_INT_COUNTER_INCREASE = RTC_IRL_RTCCIF, RTC_INT_ALARM = RTC_IRL_RTCALF }
| RTC enumeration. More...

## Functions
void | IP_RTC_Init (IP_RTC_001_T *pRTC)
| Initialize the RTC peripheral.
STATIC INLINE void | IP_RTC_DeInit (IP_RTC_001_T *pRTC)
| De-initialize the RTC peripheral.
void | IP_RTC_ResetClockTickCounter (IP_RTC_001_T *pRTC)
| Reset clock tick counter in the RTC peripheral.
void | IP_RTC_Enable (IP_RTC_001_T *pRTC, FunctionalState NewState)
| Start/Stop RTC peripheral.
void | IP_RTC_CntIncrIntConfig (IP_RTC_001_T *pRTC, uint32_t cntrMask, FunctionalState NewState)
| Enable/Disable Counter increment interrupt for a time type in the RTC peripheral.
void | IP_RTC_AlarmIntConfig (IP_RTC_001_T *pRTC, uint32_t alarmMask, FunctionalState NewState)
| Enable/Disable Alarm interrupt for a time type in the RTC peripheral.
void | IP_RTC_SetTime (IP_RTC_001_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t TimeValue)
| Set current time value for a time type in the RTC peripheral.
uint32_t | IP_RTC_GetTime (IP_RTC_001_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
| Get current time value for a type time type.
void | IP_RTC_SetFullTime (IP_RTC_001_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Set full time in the RTC peripheral.
void | IP_RTC_GetFullTime (IP_RTC_001_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Get full time from the RTC peripheral.
void | IP_RTC_SetAlarmTime (IP_RTC_001_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t ALValue)
| Set alarm time value for a time type.
uint32_t | IP_RTC_GetAlarmTime (IP_RTC_001_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
| Get alarm time value for a time type.
void | IP_RTC_SetFullAlarmTime (IP_RTC_001_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Set full alarm time in the RTC peripheral.
void | IP_RTC_GetFullAlarmTime (IP_RTC_001_T *pRTC, IP_RTC_TIME_T *pFullTime)
| Get full alarm time in the RTC peripheral.
void | IP_RTC_CalibCounterCmd (IP_RTC_001_T *pRTC, FunctionalState NewState)
| Enable/Disable calibration counter in the RTC peripheral.
void | IP_RTC_CalibConfig (IP_RTC_001_T *pRTC, uint32_t CalibValue, uint8_t CalibDir)
| Configures Calibration in the RTC peripheral.
STATIC INLINE void | IP_RTC_ClearIntPending (IP_RTC_001_T *pRTC, uint32_t IntType)
| Clear specified Location interrupt pending in the RTC peripheral.
STATIC INLINE IntStatus | IP_RTC_GetIntPending (IP_RTC_001_T *pRTC, uint32_t IntType)
| Check whether if specified location interrupt in the RTC peripheral is set or not.