| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - m -

- M0_IMAGE_ADDR : main.c
- M0_Image_Magic : cr_startup_lpc43xx_m0.c
- M0_IMAGE_OFFSET : lpc43xx_dualcore_config.h
- M0Image_Boot() : dualcore_common.h
- M0SCB_SEVONPEND : pmu_8xx.c
- M0SCB_SLEEPDEEP : pmu_8xx.c
- M0SCB_SLEEPONEXIT : pmu_8xx.c
- MAC_Address_t : RNDISClassCommon.h
- MAC_ADRH_MO : enet_001.h
- MAC_CFG_ACS : enet_001.h
- MAC_CFG_BL : enet_001.h
- MAC_CFG_DCRS : enet_001.h
- MAC_CFG_DF : enet_001.h
- MAC_CFG_DM : enet_001.h
- MAC_CFG_DO : enet_001.h
- MAC_CFG_DR : enet_001.h
- MAC_CFG_FES : enet_001.h
- MAC_CFG_IFG : enet_001.h
- MAC_CFG_IPC : enet_001.h
- MAC_CFG_JD : enet_001.h
- MAC_CFG_JE : enet_001.h
- MAC_CFG_LM : enet_001.h
- MAC_CFG_LUD : enet_001.h
- MAC_CFG_PS : enet_001.h
- MAC_CFG_RE : enet_001.h
- MAC_CFG_TE : enet_001.h
- MAC_CFG_WD : enet_001.h
- MAC_FC_DZPQ : enet_001.h
- MAC_FC_FCB : enet_001.h
- MAC_FC_PLT : enet_001.h
- MAC_FC_PT : enet_001.h
- MAC_FC_RFE : enet_001.h
- MAC_FC_TFE : enet_001.h
- MAC_FC_UP : enet_001.h
- MAC_FF_DAIF : enet_001.h
- MAC_FF_DBF : enet_001.h
- MAC_FF_PCF : enet_001.h
- MAC_FF_PM : enet_001.h
- MAC_FF_PR : enet_001.h
- MAC_FF_RA : enet_001.h
- MAC_FF_SAF : enet_001.h
- MAC_FF_SAIF : enet_001.h
- MAC_IM_PMT : enet_001.h
- MAC_MIIA_CR : enet_001.h
- MAC_MIIA_GB : enet_001.h
- MAC_MIIA_GR : enet_001.h
- MAC_MIIA_PA : enet_001.h
- MAC_MIIA_W : enet_001.h
- MAC_MIID_GDMSK : enet_001.h
- MAC_PMT_GU : enet_001.h
- MAC_PMT_MPE : enet_001.h
- MAC_PMT_MPR : enet_001.h
- MAC_PMT_PD : enet_001.h
- MAC_PMT_WFE : enet_001.h
- MAC_PMT_WFFRPR : enet_001.h
- MAC_PMT_WFR : enet_001.h
- MAC_TS_TSADDR : enet_001.h
- MAC_TS_TSCFUP : enet_001.h
- MAC_TS_TSCLKT : enet_001.h
- MAC_TS_TSCTRL : enet_001.h
- MAC_TS_TSENA : enet_001.h
- MAC_TS_TSENAL : enet_001.h
- MAC_TS_TSENMA : enet_001.h
- MAC_TS_TSEVNT : enet_001.h
- MAC_TS_TSINIT : enet_001.h
- MAC_TS_TSIPENA : enet_001.h
- MAC_TS_TSIPV4E : enet_001.h
- MAC_TS_TSIPV6E : enet_001.h
- MAC_TS_TSMSTR : enet_001.h
- MAC_TS_TSTRIG : enet_001.h
- MAC_TS_TSUPDT : enet_001.h
- MAC_TS_TSVER2 : enet_001.h
- MAC_VT_ETC : enet_001.h
- MAC_VT_VL : enet_001.h
- MACROE : Common.h
- MACROS : Common.h
- main() : swim_color_bars.c , ucos_iii_blinky.c , freertos_blinky.c , AudioOutput.c , lwip_tcpecho_freertos.c , lwip_tcpecho_sa.c , main.c , nandflash.c , norflash.c , adc.c , blinky.c , can.c , cmp.c , crc.c , dac.c , eeprom.c , enet.c , i2c.c , i2s.c , lcd.c , memtest.c , ritimer.c , rtc.c , rtc_ev.c , sdmmc.c , spi.c , ssp.c , uart.c , watchdog.c , swim_color_bars.c , ucos_iii_blinky.c , freertos_blinky.c , cr_freertos_startup_lpc11xx.c , adc.c , blinky.c , bod.c , ccan_rom.c , clkout.c , i2c.c , ssp.c , uart.c , watchdog.c , cr_startup_lpc11xx.c , freertos_blinky.c , acmp.c , blinky.c , bod.c , clkout.c , crc.c , i2c.c , mrt.c , sct.c , spi.c , uart.c , uart_rom.c , wkt.c , wwdt.c , dfuutil_programming_dfu_ops.c , AudioInput.c , AudioOutputHost.c , main.c , GenericHID.c , Keyboard.c , main.c , KeyboardHost.c , MassStorage.c , main.c , MassStorageHost.c , Mouse.c , freertos_blinky.c , VirtualSerial.c , AudioOutput.c , freertos_blinky.c , cr_freertos_startup_lpc13xx.c , lwip_tcpecho_freertos.c , adc.c , blinky.c , lwip_tcpecho_sa.c , bod.c , clkout.c , webserver.c , eeprom.c , i2c.c , app_clock_apis.c , ritimer.c , ssp.c , gpdma_speed_test.c , uart.c , watchdog.c , app_otp_funcs.c , cr_startup_lpc13xx.c , app_pmc_states.c , app_sdmmc_meas.c , main.c , sct_blinky.c , sct_simple_match.c , sct_trafficlight.c , adc.c , atimer.c , blinky.c , ccan.c , dac.c , eeprom.c , enet.c , i2c.c , i2s.c , lcd.c , memtest.c , ritimer.c , rtc.c , sdmmc.c , ssp.c , uart.c , watchdog.c
- main_tasks() : main.c
- MainTask() : main.c , TOUCH_Sample.c
- MajorVersion : RNDISClassCommon.h
- MakeString() : eeprom.c , nandflash.c , norflash.c , eeprom.c
- ManufacturerStrIndex : StdDescriptors.h
- ManufacturerString : Descriptors.c
- ManufacturerStringPtr : Descriptors.c
- MASS_STORAGE_IN_EPNUM : Descriptors.h
- MASS_STORAGE_IO_EPSIZE : Descriptors.h
- MASS_STORAGE_OUT_EPNUM : Descriptors.h
- MassStorage_GetAddressInImage() : ramdisk.c , ramdisk.h , DataRam.c , DataRam.h
- MASTER_RECEIVE : i2cd_8xx.h
- MASTER_SEND : i2cd_8xx.h
- MasterInterfaceNumber : CDCClassCommon.h
- Math_Init() : lib_math.c , lib_math.h
- Math_Rand() : lib_math.c , lib_math.h
- Math_RandSeed() : lib_math.c , lib_math.h
- Math_RandSeedCur : lib_math.c
- Math_RandSetSeed() : lib_math.c , lib_math.h
- MAX : lpc_types.h , Common.h
- MAX_CLOCK_FREQ : sys_config.h , clock_18xx_43xx.h
- MAX_ED : OHCI.h
- MAX_GTD : OHCI.h
- MAX_ITD : OHCI.h
- MAX_OBJECT : ccan_18xx_43xx.c
- MAX_STATIC_ED : OHCI.h
- MaxPackageSize : EHCI.h , OHCI.h
- MaxPacketsPerTransfer : RNDISClassCommon.h
- MaxPowerConsumption : StdDescriptors.h
- MaxTransferSize : RNDISClassCommon.h
- MBR_Table : ff.c
- MCB4300_LCD : board_keil_mcb_18574357.c , board_keil_mcb_18574357.h
- MCB_17XX_AUDIO_LINE_IN_SELECT : board_nxp_xpresso_1769.h
- MCB_17XX_AUDIO_MIC_SELECT : board_nxp_xpresso_1769.h
- MCI_BMOD_DE : sdmmc_001.h
- MCI_BMOD_DSL : sdmmc_001.h
- MCI_BMOD_FB : sdmmc_001.h
- MCI_BMOD_PBL1 : sdmmc_001.h
- MCI_BMOD_PBL128 : sdmmc_001.h
- MCI_BMOD_PBL16 : sdmmc_001.h
- MCI_BMOD_PBL256 : sdmmc_001.h
- MCI_BMOD_PBL32 : sdmmc_001.h
- MCI_BMOD_PBL4 : sdmmc_001.h
- MCI_BMOD_PBL64 : sdmmc_001.h
- MCI_BMOD_PBL8 : sdmmc_001.h
- MCI_BMOD_SWR : sdmmc_001.h
- MCI_CLK_SOURCE : sdmmc_001.h
- MCI_CLKEN_ENABLE : sdmmc_001.h
- MCI_CLKEN_LOW_PWR : sdmmc_001.h
- MCI_CLKSRC_CLKDIV0 : sdmmc_001.h
- MCI_CLKSRC_CLKDIV1 : sdmmc_001.h
- MCI_CLKSRC_CLKDIV2 : sdmmc_001.h
- MCI_CLKSRC_CLKDIV3 : sdmmc_001.h
- MCI_CLOCK_DIVIDER : sdmmc_001.h
- MCI_CMD_BOOT_MODE : sdmmc_001.h
- MCI_CMD_CCS_EXP : sdmmc_001.h
- MCI_CMD_CEATA_RD : sdmmc_001.h
- MCI_CMD_DAT_EXP : sdmmc_001.h
- MCI_CMD_DAT_WR : sdmmc_001.h
- MCI_CMD_DISABLE_BOOT : sdmmc_001.h
- MCI_CMD_ENABLE_BOOT : sdmmc_001.h
- MCI_CMD_EXPECT_BOOT_ACK : sdmmc_001.h
- MCI_CMD_INDX : sdmmc_001.h
- MCI_CMD_INIT : sdmmc_001.h
- MCI_CMD_PRV_DAT_WAIT : sdmmc_001.h
- MCI_CMD_RESP_CRC : sdmmc_001.h
- MCI_CMD_RESP_EXP : sdmmc_001.h
- MCI_CMD_RESP_LONG : sdmmc_001.h
- MCI_CMD_SEND_STOP : sdmmc_001.h
- MCI_CMD_START : sdmmc_001.h
- MCI_CMD_STOP : sdmmc_001.h
- MCI_CMD_STRM_MODE : sdmmc_001.h
- MCI_CMD_UPD_CLK : sdmmc_001.h
- MCI_CMD_VOLT_SWITCH : sdmmc_001.h
- MCI_CTRL_ABRT_READ_DATA : sdmmc_001.h
- MCI_CTRL_CARDV_MASK : sdmmc_001.h
- MCI_CTRL_CEATA_INT_EN : sdmmc_001.h
- MCI_CTRL_DMA_RESET : sdmmc_001.h
- MCI_CTRL_FIFO_RESET : sdmmc_001.h
- MCI_CTRL_INT_ENABLE : sdmmc_001.h
- MCI_CTRL_READ_WAIT : sdmmc_001.h
- MCI_CTRL_RESET : sdmmc_001.h
- MCI_CTRL_SEND_AS_CCSD : sdmmc_001.h
- MCI_CTRL_SEND_CCSD : sdmmc_001.h
- MCI_CTRL_SEND_IRQ_RESP : sdmmc_001.h
- MCI_CTRL_USE_INT_DMAC : sdmmc_001.h
- MCI_CTYPE_4BIT : sdmmc_001.h
- MCI_CTYPE_8BIT : sdmmc_001.h
- MCI_DMADES0_CES : sdmmc_001.h
- MCI_DMADES0_CH : sdmmc_001.h
- MCI_DMADES0_DIC : sdmmc_001.h
- MCI_DMADES0_ER : sdmmc_001.h
- MCI_DMADES0_FS : sdmmc_001.h
- MCI_DMADES0_LD : sdmmc_001.h
- MCI_DMADES0_OWN : sdmmc_001.h
- MCI_DMADES1_BS1 : sdmmc_001.h
- MCI_DMADES1_BS2 : sdmmc_001.h
- MCI_DMADES1_MAXTR : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_1 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_128 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_16 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_256 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_32 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_4 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_64 : sdmmc_001.h
- MCI_FIFOTH_DMA_MTS_8 : sdmmc_001.h
- MCI_FIFOTH_RX_WM : sdmmc_001.h
- MCI_FIFOTH_TX_WM : sdmmc_001.h
- MCI_INT_ACD : sdmmc_001.h
- MCI_INT_CD : sdmmc_001.h
- MCI_INT_CMD_DONE : sdmmc_001.h
- MCI_INT_DATA_OVER : sdmmc_001.h
- MCI_INT_DCRC : sdmmc_001.h
- MCI_INT_DTO : sdmmc_001.h
- MCI_INT_EBE : sdmmc_001.h
- MCI_INT_FRUN : sdmmc_001.h
- MCI_INT_HLE : sdmmc_001.h
- MCI_INT_HTO : sdmmc_001.h
- MCI_INT_RCRC : sdmmc_001.h
- MCI_INT_RESP_ERR : sdmmc_001.h
- MCI_INT_RTO : sdmmc_001.h
- MCI_INT_RXDR : sdmmc_001.h
- MCI_INT_SBE : sdmmc_001.h
- MCI_INT_SDIO : sdmmc_001.h
- MCI_INT_TXDR : sdmmc_001.h
- MCI_IRQ_CB_FUNC_T : sdmmc_001.h
- MCI_POWER_ENABLE : sdmmc_001.h
- MCI_STS_GET_FCNT : sdmmc_001.h
- MCI_TMOUT_DATA : sdmmc_001.h
- MCI_TMOUT_DATA_MSK : sdmmc_001.h
- MCI_TMOUT_RESP : sdmmc_001.h
- MCI_TMOUT_RESP_MSK : sdmmc_001.h
- MD_ADMODE : iocon_11xx.h , iocon_13xx.h
- MD_ANA_DIS : iocon_17xx_40xx.h
- MD_ANA_ENA : iocon_17xx_40xx.h
- MD_BUK : iocon_11xx.h , iocon_13xx.h , scu_18xx_43xx.h
- MD_DAC_DIS : iocon_17xx_40xx.h
- MD_DAC_ENA : iocon_17xx_40xx.h
- MD_DIGMODE : iocon_11xx.h , iocon_13xx.h
- MD_DISFIL : iocon_11xx.h , iocon_13xx.h
- MD_EHD0 : scu_18xx_43xx.h
- MD_EHD1 : scu_18xx_43xx.h
- MD_EHS : scu_18xx_43xx.h
- MD_ENFIL : iocon_11xx.h , iocon_13xx.h
- MD_EZI : scu_18xx_43xx.h
- MD_FAST_SLEW_RATE : iocon_17xx_40xx.h
- MD_FASTI2C : iocon_11xx.h , iocon_13xx.h
- MD_FILT_DIS : iocon_17xx_40xx.h
- MD_FILT_ENA : iocon_17xx_40xx.h
- MD_HD_DIS : iocon_17xx_40xx.h
- MD_HD_ENA : iocon_17xx_40xx.h
- MD_HS_DIS : iocon_17xx_40xx.h
- MD_HS_ENA : iocon_17xx_40xx.h
- MD_HYS : iocon_11xx.h , iocon_13xx.h
- MD_HYS_DIS : iocon_17xx_40xx.h
- MD_HYS_ENA : iocon_17xx_40xx.h
- MD_IINV_DIS : iocon_17xx_40xx.h
- MD_IINV_ENA : iocon_17xx_40xx.h
- MD_INV : iocon_11xx.h , iocon_13xx.h
- MD_OD_DIS : iocon_17xx_40xx.h
- MD_OD_ENA : iocon_17xx_40xx.h
- MD_OPENDRAIN : iocon_11xx.h , iocon_13xx.h
- MD_PDN : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h , scu_18xx_43xx.h
- MD_PLN : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h , scu_18xx_43xx.h
- MD_PLN_FAST : scu_18xx_43xx.h
- MD_PUP : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h , scu_18xx_43xx.h
- MD_RPT : iocon_17xx_40xx.h
- MD_SFI2C : iocon_11xx.h , iocon_13xx.h
- MD_STD_SLEW_RATE : iocon_17xx_40xx.h
- MD_STDI2C : iocon_11xx.h , iocon_13xx.h
- MD_ZI : scu_18xx_43xx.h
- Medium : RNDISClassCommon.h
- MEM_ALIGNMENT : lwipopts.h
- Mem_Clr() : lib_mem.h , lib_mem.c
- Mem_Cmp() : lib_mem.c , lib_mem.h
- mem_cmp() : ff.c
- Mem_Copy() : lib_mem.h
- mem_cpy() : ff.c
- Mem_Heap : lib_mem.c
- Mem_HeapAlloc() : lib_mem.c
- Mem_Init() : lib_mem.c , lib_mem.h
- Mem_IsInitialized : USBController.c
- MEM_LIBC_MALLOC : lwipopts.h
- MEM_POOL_IX : lib_mem.h
- MEM_POOL_IX_MAX : lib_mem.h
- MEM_POOL_IX_MIN : lib_mem.h
- MEM_POOL_IX_NONE : lib_mem.h
- Mem_PoolBlkFree() : lib_mem.c
- Mem_PoolBlkGet() : lib_mem.c
- Mem_PoolBlkIsValidAddr() : lib_mem.c
- Mem_PoolClr() : lib_mem.c
- Mem_PoolCreate() : lib_mem.c
- Mem_PoolHeap : lib_mem.c
- Mem_PoolSegAlloc() : lib_mem.c
- Mem_PoolSegCalcTotSize() : lib_mem.c
- Mem_PoolTbl : lib_mem.c
- mem_ptr_t : cc.h
- mem_set() : ff.c
- Mem_Set() : lib_mem.c , lib_mem.h
- MEM_SIZE : lwipopts.h
- mem_stack : MassStorage_ucosiii.c
- mem_tcb : MassStorage_ucosiii.c
- mem_test_address() : mem_tests.c , mem_tests.h
- mem_test_invaddress() : mem_tests.h , mem_tests.c
- mem_test_pattern() : mem_tests.c , mem_tests.h
- mem_test_pattern_seed() : mem_tests.c , mem_tests.h
- mem_test_walking0() : mem_tests.c , mem_tests.h
- mem_test_walking1() : mem_tests.h , mem_tests.c
- MEM_VAL_COPY_08 : lib_mem.h
- MEM_VAL_COPY_16 : lib_mem.h
- MEM_VAL_COPY_32 : lib_mem.h
- MEM_VAL_COPY_GET_INT08U : lib_mem.h
- MEM_VAL_COPY_GET_INT08U_BIG : lib_mem.h
- MEM_VAL_COPY_GET_INT08U_LITTLE : lib_mem.h
- MEM_VAL_COPY_GET_INT16U : lib_mem.h
- MEM_VAL_COPY_GET_INT16U_BIG : lib_mem.h
- MEM_VAL_COPY_GET_INT16U_LITTLE : lib_mem.h
- MEM_VAL_COPY_GET_INT32U : lib_mem.h
- MEM_VAL_COPY_GET_INT32U_BIG : lib_mem.h
- MEM_VAL_COPY_GET_INT32U_LITTLE : lib_mem.h
- MEM_VAL_COPY_GET_INTU : lib_mem.h
- MEM_VAL_COPY_GET_INTU_BIG : lib_mem.h
- MEM_VAL_COPY_GET_INTU_LITTLE : lib_mem.h
- MEM_VAL_COPY_SET_INT08U : lib_mem.h
- MEM_VAL_COPY_SET_INT08U_BIG : lib_mem.h
- MEM_VAL_COPY_SET_INT08U_LITTLE : lib_mem.h
- MEM_VAL_COPY_SET_INT16U : lib_mem.h
- MEM_VAL_COPY_SET_INT16U_BIG : lib_mem.h
- MEM_VAL_COPY_SET_INT16U_LITTLE : lib_mem.h
- MEM_VAL_COPY_SET_INT32U : lib_mem.h
- MEM_VAL_COPY_SET_INT32U_BIG : lib_mem.h
- MEM_VAL_COPY_SET_INT32U_LITTLE : lib_mem.h
- MEM_VAL_COPY_SET_INTU : lib_mem.h
- MEM_VAL_COPY_SET_INTU_BIG : lib_mem.h
- MEM_VAL_COPY_SET_INTU_LITTLE : lib_mem.h
- MEM_VAL_GET_INT08U : lib_mem.h
- MEM_VAL_GET_INT08U_BIG : lib_mem.h
- MEM_VAL_GET_INT08U_LITTLE : lib_mem.h
- MEM_VAL_GET_INT16U : lib_mem.h
- MEM_VAL_GET_INT16U_BIG : lib_mem.h
- MEM_VAL_GET_INT16U_LITTLE : lib_mem.h
- MEM_VAL_GET_INT32U : lib_mem.h
- MEM_VAL_GET_INT32U_BIG : lib_mem.h
- MEM_VAL_GET_INT32U_LITTLE : lib_mem.h
- MEM_VAL_SET_INT08U : lib_mem.h
- MEM_VAL_SET_INT08U_BIG : lib_mem.h
- MEM_VAL_SET_INT08U_LITTLE : lib_mem.h
- MEM_VAL_SET_INT16U : lib_mem.h
- MEM_VAL_SET_INT16U_BIG : lib_mem.h
- MEM_VAL_SET_INT16U_LITTLE : lib_mem.h
- MEM_VAL_SET_INT32U : lib_mem.h
- MEM_VAL_SET_INT32U_BIG : lib_mem.h
- MEM_VAL_SET_INT32U_LITTLE : lib_mem.h
- MemManage_Handler() : cr_startup_lpc18xx43xx.c , cr_freertos_startup_lpc18xx43xx.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc17xx40xx.c , cr_startup_lpc17xx40xx.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c
- MEMP_MEM_MALLOC : lwipopts.h
- MEMP_NUM_SYS_TIMEOUT : lwipopts.h
- MEMSPACE_EEPROM : DeviceStandardReq.h
- MEMSPACE_FLASH : DeviceStandardReq.h
- MEMSPACE_RAM : DeviceStandardReq.h
- menu : app_clock_apis.c , app_pmc_states.c
- menu1 : app_pmc_states.c
- menu2 : app_pmc_states.c
- menu3 : app_pmc_states.c
- MessageLength : RNDISClassCommon.h
- MessageType : RNDISClassCommon.h
- MIC_IN_ADC_CHANNEL : AudioInput.h , AudioOutputHost.h
- MIC_IN_ADC_MUX_MASK : AudioInput.h , AudioOutputHost.h
- MICRIUM_SOURCE : os_msg.c , os_mutex.c , os_flag.c , os_app_hooks.c , os_prio.c , os_q.c , os_tls.c , os_cfg_app.c , os_dbg.c , os_int.c , os_pend_multi.c , os_stat.c , os_tmr.c , os_core.c , os_mem.c , os_task.c , os_tls.c , os_time.c , os_var.c , os_sem.c , os_tick.c
- Microphone_Audio_Interface : AudioInput.c
- MIDI_CHANNEL : MIDIClassCommon.h
- MIDI_COMMAND_NOTE_OFF : MIDIClassCommon.h
- MIDI_COMMAND_NOTE_ON : MIDIClassCommon.h
- MIDI_Device_ConfigureEndpoints() : MIDIClassDevice.c , MIDIClassDevice.h
- MIDI_Device_Flush() : MIDIClassDevice.c , MIDIClassDevice.h
- MIDI_Device_ProcessControlRequest() : MIDIClassDevice.h
- MIDI_Device_ReceiveEventPacket() : MIDIClassDevice.c , MIDIClassDevice.h
- MIDI_Device_SendEventPacket() : MIDIClassDevice.h , MIDIClassDevice.c
- MIDI_Device_USBTask() : MIDIClassDevice.h , MIDIClassDevice.c
- MIDI_ENUMERROR_InvalidConfigDescriptor : MIDIClassHost.h
- MIDI_ENUMERROR_NoCompatibleInterfaceFound : MIDIClassHost.h
- MIDI_ENUMERROR_NoError : MIDIClassHost.h
- MIDI_ENUMERROR_PipeConfigurationFailed : MIDIClassHost.h
- MIDI_EventPacket_t : MIDIClassCommon.h
- MIDI_Host_ConfigurePipes() : MIDIClassHost.c , MIDIClassHost.h
- MIDI_Host_EnumerationFailure_ErrorCodes_t : MIDIClassHost.h
- MIDI_Host_Flush() : MIDIClassHost.h , MIDIClassHost.c
- MIDI_Host_ReceiveEventPacket() : MIDIClassHost.c , MIDIClassHost.h
- MIDI_Host_SendEventPacket() : MIDIClassHost.h , MIDIClassHost.c
- MIDI_Host_USBTask() : MIDIClassHost.h , MIDIClassHost.c
- MIDI_JACKTYPE_Embedded : MIDIClassCommon.h
- MIDI_JACKTYPE_External : MIDIClassCommon.h
- MIDI_JackTypes_t : MIDIClassCommon.h
- MIDI_STANDARD_VELOCITY : MIDIClassCommon.h
- MIN : Common.h , lpc_types.h
- MIN_FAT16 : ff.c
- MIN_FAT32 : ff.c
- MINBLUE : lpc_colors.h
- MINGREEN : lpc_colors.h
- MinorVersion : RNDISClassCommon.h
- MINRED : lpc_colors.h
- MissedUframe : EHCI.h
- MMC : diskio.c
- MMC_ALL_SEND_CID : lpc_sdmmc.h
- MMC_APP_CMD : lpc_sdmmc.h
- MMC_CLR_WRITE_PROT : lpc_sdmmc.h
- MMC_ERASE : lpc_sdmmc.h
- MMC_ERASE_GROUP_END : lpc_sdmmc.h
- MMC_ERASE_GROUP_START : lpc_sdmmc.h
- MMC_FAST_IO : lpc_sdmmc.h
- MMC_GEN_CMD : lpc_sdmmc.h
- MMC_GET_CID : diskio.h
- MMC_GET_CSD : diskio.h
- MMC_GET_OCR : diskio.h
- MMC_GET_SDSTAT : diskio.h
- MMC_GET_TYPE : diskio.h
- MMC_GO_IDLE_STATE : lpc_sdmmc.h
- MMC_GO_INACTIVE_STATE : lpc_sdmmc.h
- MMC_GO_IRQ_STATE : lpc_sdmmc.h
- MMC_HIGH_BUS_MAX_CLOCK : sdif_18xx_43xx.h
- MMC_LOCK_UNLOCK : lpc_sdmmc.h
- MMC_LOW_BUS_MAX_CLOCK : sdif_18xx_43xx.h
- MMC_MAX_CLOCK : sdif_18xx_43xx.h
- MMC_PROGRAM_CID : lpc_sdmmc.h
- MMC_PROGRAM_CSD : lpc_sdmmc.h
- MMC_READ_MULTIPLE_BLOCK : lpc_sdmmc.h
- MMC_READ_SINGLE_BLOCK : lpc_sdmmc.h
- MMC_SECTOR_SIZE : lpc_sdmmc.h
- MMC_SELECT_CARD : lpc_sdmmc.h
- MMC_SEND_CID : lpc_sdmmc.h
- MMC_SEND_CSD : lpc_sdmmc.h
- MMC_SEND_EXT_CSD : lpc_sdmmc.h
- MMC_SEND_OP_COND : lpc_sdmmc.h
- MMC_SEND_STATUS : lpc_sdmmc.h
- MMC_SEND_WRITE_PROT : lpc_sdmmc.h
- MMC_SET_BLOCK_COUNT : lpc_sdmmc.h
- MMC_SET_BLOCKLEN : lpc_sdmmc.h
- MMC_SET_DSR : lpc_sdmmc.h
- MMC_SET_RELATIVE_ADDR : lpc_sdmmc.h
- MMC_SET_WRITE_PROT : lpc_sdmmc.h
- MMC_STOP_TRANSMISSION : lpc_sdmmc.h
- MMC_WRITE_BLOCK : lpc_sdmmc.h
- MMC_WRITE_DAT_UNTIL_STOP : lpc_sdmmc.h
- MMC_WRITE_MULTIPLE_BLOCK : lpc_sdmmc.h
- MODE_CFG_CCITT : crc_001.h
- MODE_CFG_CRC16 : crc_001.h
- MODE_CFG_CRC32 : crc_001.h
- mode_poll : i2c.c
- Modifier : HIDClassCommon.h
- MOUSE_EPNUM : Descriptors.h
- MOUSE_EPSIZE : Descriptors.h
- Mouse_HID_Interface : Mouse.c
- MouseReport : Descriptors.c
- move_window() : ff.c
- MRT0_INTFLAG : mrt_8xx.h
- MRT1_INTFLAG : mrt_8xx.h
- MRT2_INTFLAG : mrt_8xx.h
- MRT3_INTFLAG : mrt_8xx.h
- MRT_IRQHandler() : mrt.c
- MRT_MODE_ONESHOT : mrt_001.h
- MRT_MODE_REPEAT : mrt_001.h
- MS_ACQUIRE_DELAY : sdif_18xx_43xx.h , sdmmc_17xx_40xx.c
- MS_CBW_SIGNATURE : MassStorageClassCommon.h
- MS_ClassRequests_t : MassStorageClassCommon.h
- MS_COMMAND_DIR_DATA_IN : MassStorageClassCommon.h
- MS_COMMAND_DIR_DATA_OUT : MassStorageClassCommon.h
- MS_CommandBlockWrapper_t : MassStorageClassCommon.h
- MS_CommandStatusCodes_t : MassStorageClassCommon.h
- MS_CommandStatusWrapper_t : MassStorageClassCommon.h
- MS_CSCP_BulkOnlyTransportProtocol : MassStorageClassCommon.h
- MS_CSCP_MassStorageClass : MassStorageClassCommon.h
- MS_CSCP_SCSITransparentSubclass : MassStorageClassCommon.h
- MS_CSW_SIGNATURE : MassStorageClassCommon.h
- MS_Descriptor_ClassSubclassProtocol_t : MassStorageClassCommon.h
- MS_Device_ConfigureEndpoints() : MassStorageClassDevice.h , MassStorageClassDevice.c
- MS_Device_ProcessControlRequest() : MassStorageClassDevice.c , MassStorageClassDevice.h
- MS_Device_ReadInCommandBlock() : MassStorageClassDevice.c
- MS_Device_ReturnCommandStatus() : MassStorageClassDevice.c
- MS_Device_USBTask() : MassStorageClassDevice.h , MassStorageClassDevice.c
- MS_ENUMERROR_InvalidConfigDescriptor : MassStorageClassHost.h
- MS_ENUMERROR_NoCompatibleInterfaceFound : MassStorageClassHost.h
- MS_ENUMERROR_NoError : MassStorageClassHost.h
- MS_ENUMERROR_PipeConfigurationFailed : MassStorageClassHost.h
- MS_ERROR_LOGICAL_CMD_FAILED : MassStorageClassHost.h
- MS_Host_ConfigurePipes() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_EnumerationFailure_ErrorCodes_t : MassStorageClassHost.h
- MS_Host_GetInquiryData() : MassStorageClassHost.h , MassStorageClassHost.c
- MS_Host_GetMaxLUN() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_GetReturnedStatus() : MassStorageClassHost.c
- MS_Host_PreventAllowMediumRemoval() : MassStorageClassHost.h , MassStorageClassHost.c
- MS_Host_ReadDeviceBlocks() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_ReadDeviceCapacity() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_RequestSense() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_ResetMSInterface() : MassStorageClassHost.h , MassStorageClassHost.c
- MS_Host_SendCommand() : MassStorageClassHost.c
- MS_Host_SendReceiveData() : MassStorageClassHost.c
- MS_Host_TestUnitReady() : MassStorageClassHost.c , MassStorageClassHost.h
- MS_Host_USBTask() : MassStorageClassHost.h
- MS_Host_WaitForDataReceived() : MassStorageClassHost.c
- MS_Host_WriteDeviceBlocks() : MassStorageClassHost.h , MassStorageClassHost.c
- MS_REQ_GetMaxLUN : MassStorageClassCommon.h
- MS_REQ_MassStorageReset : MassStorageClassCommon.h
- MS_SCSI_COMMAND_Fail : MassStorageClassCommon.h
- MS_SCSI_COMMAND_Pass : MassStorageClassCommon.h
- MS_SCSI_COMMAND_PhaseError : MassStorageClassCommon.h
- MSC_BS_CBW : usbd_msc.h
- MSC_BS_CSW : usbd_msc.h
- MSC_BS_DATA_IN : usbd_msc.h
- MSC_BS_DATA_IN_LAST : usbd_msc.h
- MSC_BS_DATA_IN_LAST_STALL : usbd_msc.h
- MSC_BS_DATA_OUT : usbd_msc.h
- MSC_BS_ERROR : usbd_msc.h
- MSC_CBW_Signature : usbd_msc.h
- MSC_CSW_Signature : usbd_msc.h
- MSC_PROTOCOL_BULK_ONLY : usbd_msc.h
- MSC_PROTOCOL_CBI_INT : usbd_msc.h
- MSC_PROTOCOL_CBI_NOINT : usbd_msc.h
- MSC_REQUEST_GET_MAX_LUN : usbd_msc.h
- MSC_REQUEST_RESET : usbd_msc.h
- MSC_SUBCLASS_QIC157 : usbd_msc.h
- MSC_SUBCLASS_RBC : usbd_msc.h
- MSC_SUBCLASS_SCSI : usbd_msc.h
- MSC_SUBCLASS_SFF8020I_MMC2 : usbd_msc.h
- MSC_SUBCLASS_SFF8070I : usbd_msc.h
- MSC_SUBCLASS_UFI : usbd_msc.h
- msDelay() : lpc_arch.h , lpc43xx_systick.c , lpc17xx_40xx_emac.h , lpc18xx_43xx_emac.c , lpc18xx_43xx_emac.h , lwip_tcpecho_freertos.c , lpc17xx_40xx_emac.c , lwip_tcpecho_freertos.c
- msec : lcd.c
- msg_obj : ccan_rom.c
- msg_received_counter : ccan.c
- MSleep() : main.c , dualcore_common.h
- MT48LC4M32_config : sysinit_keil_mcb_18574357.c
- Mult : EHCI.h
- mute_status : i2s.c
- mute_toggle() : i2s.c
- mutex_init() : lwip_fs.c
- mutex_lock() : lwip_fs.c
- mutex_unlock() : lwip_fs.c
- mwDFU_GetMemSize() : usbd_api.h
- mwDFU_init() : usbd_api.h
- mwHID_GetMemSize() : usbd_api.h
- mwHID_init() : usbd_api.h
- mwMSC_GetMemSize() : usbd_api.h
- mwMSC_init() : usbd_api.h
- mwUSB_DataInStage() : usbd_api.h
- mwUSB_DataOutStage() : usbd_api.h
- mwUSB_RegisterClassHandler() : usbd_api.h
- mwUSB_RegisterEpHandler() : usbd_api.h
- mwUSB_SetupStage() : usbd_api.h
- mwUSB_StallEp0() : usbd_api.h
- mwUSB_StatusInStage() : usbd_api.h
- mwUSB_StatusOutStage() : usbd_api.h