| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Enumerations | Functions | Variables
USBController.h File Reference
`#include "../../../Common/Common.h"`
`#include "USBMode.h"`
`#include "Events.h"`
`#include "USBTask.h"`
`#include "USBInterrupt.h"`
`#include "Host.h"`
`#include "OTG.h"`
`#include "Pipe.h"`
`#include "HostStandardReq.h"`
`#include "PipeStream.h"`
`#include "Device.h"`
`#include "Endpoint.h"`
`#include "DeviceStandardReq.h"`
`#include "EndpointStream.h"`

Go to the source code of this file.

## Macros
#define | USB_STREAM_TIMEOUT_MS 100
Endpoint Direction Masks
#define | ENDPOINT_DIR_MASK 0x80
#define | ENDPOINT_DIR_OUT 0x00
#define | ENDPOINT_DIR_IN 0x80
Endpoint/Pipe Type Masks
#define | EP_TYPE_MASK 0x03
#define | EP_TYPE_CONTROL 0x00
#define | EP_TYPE_ISOCHRONOUS 0x01
#define | EP_TYPE_BULK 0x02
#define | EP_TYPE_INTERRUPT 0x03
USB Controller Option Masks
#define | USB_OPT_REG_DISABLED (1 << 1)
#define | USB_OPT_REG_ENABLED (0 << 1)
#define | USB_OPT_MANUAL_PLL (1 << 2)
#define | USB_OPT_AUTO_PLL (0 << 2)

## Enumerations
enum | USB_Modes_t { USB_MODE_None = 0, USB_MODE_Device = 1, USB_MODE_Host = 2, USB_MODE_UID = 3 }

## Functions
static PRAGMA_ALWAYS_INLINE bool | USB_VBUS_GetStatus (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
| Determines if the VBUS line is currently high (i.e. the USB host is supplying power).
static PRAGMA_ALWAYS_INLINE void | USB_Detach (void) ATTR_ALWAYS_INLINE
static PRAGMA_ALWAYS_INLINE void | USB_Attach (void) ATTR_ALWAYS_INLINE
void | USB_Init (uint8_t corenum, uint8_t mode)
void | USB_Disable (uint8_t corenum, uint8_t mode)
void | USB_ResetInterface (uint8_t corenum, uint8_t mode)

## Variables
volatile uint8_t | USB_CurrentMode []
volatile uint8_t | USB_Options