| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions | Variables
sdmmc_18xx_43xx.c File Reference
`#include "chip.h"`
`#include "string.h"`

Go to the source code of this file.

## Macros
#define | SD_INT_ERROR

## Functions
static int32_t | sdmmc_execute_command (LPC_SDMMC_T *pSDMMC, uint32_t cmd, uint32_t arg, uint32_t wait_status)
static int32_t | prv_card_acquired (void)
static uint32_t | prv_get_bits (int32_t start, int32_t end, uint32_t *data)
static void | prv_process_csd (LPC_SDMMC_T *pSDMMC)
static int32_t | prv_set_trans_state (LPC_SDMMC_T *pSDMMC)
static int32_t | prv_set_card_params (LPC_SDMMC_T *pSDMMC)
int32_t | Chip_SDMMC_GetState (LPC_SDMMC_T *pSDMMC)
| Get card's current state (idle, transfer, program, etc.)
uint32_t | Chip_SDMMC_Acquire (LPC_SDMMC_T *pSDMMC, mci_card_struct *pcardinfo)
| Function to enumerate the SD/MMC/SDHC/MMC+ cards.
int32_t | Chip_SDMMC_GetDeviceSize (LPC_SDMMC_T *pSDMMC)
| Get the device size of SD/MMC card (after enumeration)
int32_t | Chip_SDMMC_GetDeviceBlocks (LPC_SDMMC_T *pSDMMC)
| Get the number of device blocks of SD/MMC card (after enumeration) Since Chip_SDMMC_GetDeviceSize is limited to 32 bits cards with greater than 2 GBytes of data will not be correct, in such cases users can use this function to get the size of the card in blocks.
int32_t | Chip_SDMMC_ReadBlocks (LPC_SDMMC_T *pSDMMC, void *buffer, int32_t start_block, int32_t num_blocks)
| Performs the read of data from the SD/MMC card.
int32_t | Chip_SDMMC_WriteBlocks (LPC_SDMMC_T *pSDMMC, void *buffer, int32_t start_block, int32_t num_blocks)
| Performs write of data to the SD/MMC card.

## Variables
static mci_card_struct * | g_card_info

## Macro Definition Documentation

#define SD_INT_ERROR

Value:
(MCI_INT_RESP_ERR | MCI_INT_RCRC | MCI_INT_DCRC | \
MCI_INT_RTO | MCI_INT_DTO | MCI_INT_HTO | MCI_INT_FRUN | MCI_INT_HLE | \
MCI_INT_SBE | MCI_INT_EBE)

Definition at line 43 of file sdmmc_18xx_43xx.c.

## Function Documentation

static int32_t prv_card_acquired | ( | void |  | ) |
| static

Definition at line 149 of file sdmmc_18xx_43xx.c.

static uint32_t prv_get_bits | ( | int32_t | start,
|  | int32_t | end,
|  | uint32_t * | data
| ) |  |
| static

Definition at line 156 of file sdmmc_18xx_43xx.c.

static void prv_process_csd | ( | LPC_SDMMC_T * | pSDMMC | ) |
| static

Definition at line 173 of file sdmmc_18xx_43xx.c.

static int32_t prv_set_card_params | ( | LPC_SDMMC_T * | pSDMMC | ) |
| static

Definition at line 275 of file sdmmc_18xx_43xx.c.

static int32_t prv_set_trans_state | ( | LPC_SDMMC_T * | pSDMMC | ) |
| static

Definition at line 239 of file sdmmc_18xx_43xx.c.

static int32_t sdmmc_execute_command | ( | LPC_SDMMC_T * | pSDMMC,
|  | uint32_t | cmd,
|  | uint32_t | arg,
|  | uint32_t | wait_status
| ) |  |
| static

Definition at line 56 of file sdmmc_18xx_43xx.c.

## Variable Documentation

mci_card_struct* g_card_info
| static

Definition at line 40 of file sdmmc_18xx_43xx.c.