| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
LPC13xx Clock output example
Peripheral examples

## Detailed Description

Example description
This example shows how to use the SYSCTL driver to driver a specific clock source on the CLKOUT pin. To use this example, you'll need to connect an oscilloscope to the CLKOUT pin on your board.

Special connection requirements
Observe the clock out on pin PIO0_1 (J6-38) by using oscilloscope.

Build procedures:
LPC13xx example quickstart for Code Red Xpresso
LPC13xx example quickstart for Keil uVision4
LPC13xx example quickstart for IAR EWARM

Supported boards and board setup:
NXP Xpresso LPC1347 board

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
void | SysTick_Handler (void)
| Handle interrupt from SysTick timer.
int | main (void)
| main routine for CLKOUT example

## Variables
static volatile uint32_t | ticks100

## Function Documentation

int main | ( | void |  | ) |

main routine for CLKOUT example

Main program body.

Returns
  Always returns 0

defined(CHIP_LPC175X_6X)

Definition at line 92 of file clkout.c.

void SysTick_Handler | ( | void |  | ) |

Handle interrupt from SysTick timer.

SysTick 1mS tick handler.

Returns
  Nothing

Definition at line 80 of file clkout.c.

## Variable Documentation

volatile uint32_t ticks100
| static

Definition at line 62 of file clkout.c.