| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
gpio_18xx_43xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC18xx/43xx GPIO driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __GPIO_18XX_43XX_H_
33 #define __GPIO_18XX_43XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
49 STATIC INLINE void Chip_GPIO_Init(LPC_GPIO_T *pGPIO)
50 {
51 IP_GPIO_Init(pGPIO);
52 }
53
62 STATIC INLINE void Chip_GPIO_WritePortBit(LPC_GPIO_T *pGPIO, uint32_t port, uint8_t bit, bool setting)
63 {
64 IP_GPIO_WritePortBit(pGPIO, port, bit, setting);
65 }
66
75 STATIC INLINE void Chip_GPIO_WriteDirBit(LPC_GPIO_T *pGPIO, uint32_t port, uint8_t bit, bool setting)
76 {
77 IP_GPIO_WriteDirBit(pGPIO, port, bit, setting);
78 }
79
87 STATIC INLINE bool Chip_GPIO_ReadPortBit(LPC_GPIO_T *pGPIO, uint32_t port, uint8_t bit)
88 {
89 return IP_GPIO_ReadPortBit(pGPIO, port, bit);
90 }
91
99 STATIC INLINE bool Chip_GPIO_ReadDirBit(LPC_GPIO_T *pGPIO, uint32_t port, uint8_t bit)
100 {
101 return IP_GPIO_ReadDirBit(pGPIO, port, bit);
102 }
103
116 STATIC INLINE void Chip_GPIO_IntCmd(LPC_GPIOPININT_T* pGPIOPinInt, uint8_t portNum, uint8_t bitValue, IP_GPIOPININT_MODE_T intMode)
117 {
118 IP_GPIOPININT_IntCmd(pGPIOPinInt, portNum, intMode);
119 }
120
129 STATIC INLINE bool Chip_GPIO_IntGetStatus(LPC_GPIOPININT_T* pGPIOPinInt, uint8_t portNum, uint8_t pinNum, uint8_t intMode)
130 {
131 return IP_GPIOPININT_IntGetStatus(pGPIOPinInt, portNum);
132 }
133
141 STATIC INLINE void Chip_GPIO_IntClear(LPC_GPIOPININT_T* pGPIOPinInt, uint8_t portNum, uint8_t bitValue)
142 {
143 IP_GPIOPININT_IntClear(pGPIOPinInt, portNum);
144 }
145
153 STATIC INLINE void Chip_GPIOGP_IntInit(IP_GPIOGROUPINT_001_T *pGPIOGPINT, uint8_t PortComb, uint8_t PortTrigger)
154 {
155 IP_GPIOGP_IntInit(pGPIOGPINT, PortComb, PortTrigger);
156 }
157
166 STATIC INLINE void Chip_GPIOGP_IntPinAdd(IP_GPIOGROUPINT_001_T *pGPIOGPINT,
167 uint8_t PortNum,
168 uint8_t PinNum,
169 bool ActiveMode)
170 {
171 IP_GPIOGP_IntPinAdd(pGPIOGPINT, PortNum, PinNum, ActiveMode);
172 }
173
181 STATIC INLINE void Chip_GPIOGP_IntPinRemove(IP_GPIOGROUPINT_001_T *pGPIOGPINT, uint8_t PortNum, uint8_t PinNum)
182 {
183 IP_GPIOGP_IntPinRemove(pGPIOGPINT, PortNum, PinNum);
184 }
185
191 STATIC INLINE bool Chip_GPIOGP_IntGetStatus(IP_GPIOGROUPINT_001_T *pGPIOGPINT)
192 {
193 return IP_GPIOGP_IntGetStatus(pGPIOGPINT);
194 }
195
201 STATIC INLINE void Chip_GPIOGP_IntClear(IP_GPIOGROUPINT_001_T *pGPIOGPINT)
202 {
203 IP_GPIOGP_IntClear(pGPIOGPINT);
204 }
205
215 void Chip_GPIO_SetDir(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue, uint8_t out);
216
226 STATIC INLINE void Chip_FIO_SetDir(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue, uint8_t out)
227 {
228 /* Same with Chip_GPIO_SetDir() */
229 Chip_GPIO_SetDir(pGPIO, portNum, bitValue, out);
230 }
231
241 STATIC INLINE void Chip_FIO_SetValue(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue)
242 {
243 /* Same with GPIO_SetValue() */
244 pGPIO->SET[portNum] = bitValue;
245 }
246
256 STATIC INLINE void Chip_FIO_ClearValue(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue)
257 {
258 /* Same with GPIO_ClearValue() */
259 pGPIO->CLR[portNum] = bitValue;
260 }
261
270 STATIC INLINE uint32_t Chip_FIO_ReadValue(LPC_GPIO_T *pGPIO, uint8_t portNum)
271 {
272 /* Same with GPIO_ReadValue() */
273 return pGPIO->PIN[portNum];
274 }
275
285 STATIC INLINE void Chip_GPIO_SetValue(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue)
286 {
287 pGPIO->SET[portNum] = bitValue;
288 }
289
299 STATIC INLINE void Chip_GPIO_ClearValue(LPC_GPIO_T *pGPIO, uint8_t portNum, uint32_t bitValue)
300 {
301 pGPIO->CLR[portNum] = bitValue;
302 }
303
312 STATIC INLINE uint32_t Chip_GPIO_ReadValue(LPC_GPIO_T *pGPIO, uint8_t portNum)
313 {
314 return pGPIO->PIN[portNum];
315 }
316
321 #ifdef __cplusplus
322 }
323 #endif
324
325 #endif /* __GPIO_18XX_43XX_H_ */