| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
eeprom_18xx_43xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC18xx/40xx EEPROM driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef EEPROM_18XX_43XX_H_
33 #define EEPROM_18XX_43XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
44 #define EEPROM_START (0x20040000)
45
46 #define EEPROM_PAGE_SIZE (128)
47
48 #define EEPROM_PAGE_NUM (128)
49
50 #define EEPROM_ADDRESS(page, offset) (EEPROM_START + (EEPROM_PAGE_SIZE * (page)) + offset)
51
57 void Chip_EEPROM_Init(LPC_EEPROM_T *pEEPROM);
58
64 STATIC INLINE void Chip_EEPROM_DeInit(LPC_EEPROM_T *pEEPROM)
65 {
66 IP_EEPROM_DeInit(pEEPROM);
67 }
68
75 STATIC INLINE void Chip_EEPROM_SetAutoProg(LPC_EEPROM_T *pEEPROM, uint32_t mode)
76 {
77 IP_EEPROM_SetAutoProg(pEEPROM, mode);
78 }
79
88 STATIC INLINE void Chip_EEPROM_SetReadWaitState(LPC_EEPROM_T *pEEPROM, uint32_t ws)
89 {
90 IP_EEPROM_SetReadWaitState(pEEPROM, ws);
91 }
92
102 STATIC INLINE void Chip_EEPROM_SetWaitState(LPC_EEPROM_T *pEEPROM, uint32_t ws)
103 {
104 IP_EEPROM_SetWaitState(pEEPROM, ws);
105 }
106
114 STATIC INLINE void Chip_EEPROM_SetCmd(LPC_EEPROM_T *pEEPROM, uint32_t cmd)
115 {
116 IP_EEPROM_SetCmd(pEEPROM, cmd);
117 }
118
124 STATIC INLINE void Chip_EEPROM_EraseProgramPage(LPC_EEPROM_T *pEEPROM)
125 {
126 IP_EEPROM_EraseProgramPage(pEEPROM);
127 }
128
135 STATIC INLINE void Chip_EEPROM_WaitForIntStatus(IP_EEPROM_002_T *pEEPROM, uint32_t mask)
136 {
137 IP_EEPROM_WaitForIntStatus(pEEPROM, mask);
138 }
139
145 STATIC INLINE void Chip_EEPROM_EnablePowerDown(LPC_EEPROM_T *pEEPROM)
146 {
147 IP_EEPROM_EnablePowerDown(pEEPROM);
148 }
149
155 STATIC INLINE void Chip_EEPROM_DisablePowerDown(LPC_EEPROM_T *pEEPROM)
156 {
157 IP_EEPROM_DisablePowerDown(pEEPROM);
158 }
159
166 STATIC INLINE void Chip_EEPROM_EnableInt(LPC_EEPROM_T *pEEPROM, uint32_t mask)
167 {
168 IP_EEPROM_EnableInt(pEEPROM, mask);
169 }
170
177 STATIC INLINE void Chip_EEPROM_DisableInt(LPC_EEPROM_T *pEEPROM, uint32_t mask)
178 {
179 IP_EEPROM_DisableInt(pEEPROM, mask);
180 }
181
187 STATIC INLINE uint32_t Chip_EEPROM_GetIntEnable(LPC_EEPROM_T *pEEPROM)
188 {
189 return IP_EEPROM_GetIntEnable(pEEPROM);
190 }
191
197 STATIC INLINE uint32_t Chip_EEPROM_GetIntStatus(LPC_EEPROM_T *pEEPROM)
198 {
199 return IP_EEPROM_GetIntStatus(pEEPROM);
200 }
201
208 STATIC INLINE void Chip_EEPROM_SetIntStatus(LPC_EEPROM_T *pEEPROM, uint32_t mask)
209 {
210 IP_EEPROM_SetIntStatus(pEEPROM, mask);
211 }
212
219 STATIC INLINE void Chip_EEPROM_ClearIntStatus(LPC_EEPROM_T *pEEPROM, uint32_t mask)
220 {
221 IP_EEPROM_ClearIntStatus(pEEPROM, mask);
222 }
223
228 #ifdef __cplusplus
229 }
230 #endif
231
232 #endif /* EEPROM_18XX_43XX_H_ */