| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_BUS_TIMING_T Struct Reference
IP: CAN register block and driver

## Detailed Description

CAN Bus Timing Structure.

Definition at line 674 of file can_001.h.

`#include "can_001.h"`

## Data Fields
uint16_t | BRP
uint8_t | SJW
uint8_t | TESG1
uint8_t | TESG2
uint8_t | SAM

## Field Documentation

uint16_t BRP

Baud Rate Prescaler

Definition at line 676 of file can_001.h.

uint8_t SAM

0: The bus is sampled once, 1: sampled 3 times

Definition at line 680 of file can_001.h.

uint8_t SJW

SJW value

Definition at line 677 of file can_001.h.

uint8_t TESG1

TESG1 value

Definition at line 678 of file can_001.h.

uint8_t TESG2

TESG2 value

Definition at line 679 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h