| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
LPCOpen examples for the 17xx/40xx devices
LPCOpen examples

## Detailed Description

Supported device and board information
The LPCOpen 17xx/40xx examples are customized to run on boards that use the LPC17xx and LPC40xx devices. For supported devices and boards and links to documentation, see the following page:
Supported 17xx/40xx platforms

IMPORTANT INFORMATION ABOUT INSTALLING LPCOPEN - PLEASE READ!
LPCOpen download and installation information

Optional components needed for some LPCOpen examples
emWin download and installation

Default jumper configuration and board recovery guide
Unless an example specifically changes a jumper setting, a default jumper setup is used for the example. Be sure the board is setup to the correct jumper state prior to using the examples. See the supported board pages for default jumper setup for each board.

If you program something into the board that corrupts the system on boot-up, the debugger may no longer be able to get control of the board to program a new image into it. See the board information page on recovering your board from this state.
Embedded Artists' LPC1788 Developer's Kit
Embedded Artists' LPC4088 Developer's Kit
NXP Xpresso LPC1769 board

Quickstart guides
Select one of the quickstart guides below to get started:
LPC17xx/40xx example quickstart for Keil uVision4
LPC17xx/40xx example quickstart for IAR EWARM
LPC17xx/40xx example quickstart for Code Red Xpresso

## Modules
| FreeRTOS examples
| LWIP examples
| Misc examples
| Peripheral examples
| SWIM examples
| USB examples
| emWin GUI examples
| uCos-III examples