| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
flash_13xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC13xx Flash/EEPROM programming
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __FLASH_EEPROM_13XX_H_
33 #define __FLASH_EEPROM_13XX_H_
34
35 #if defined(CHIP_LPC1347)
36
37 #ifdef __cplusplus
38 extern "C" {
39 #endif
40
47 #define FLASH_ENTRY_LOCATION (0x1fff1ff1)
48
50 #define EEPROM_SIZE (4 << 10)
51
53 #define PART_ID (0x08020543)
54
60 STATIC INLINE uint32_t Chip_FLASH_GetSecNum(uint32_t adr)
61 {
62 return adr >> 12;
63 }
64
71 STATIC INLINE void Chip_FLASH_Execute(FLASH_COMMAND_T *pCommand, FLASH_OUTPUT_T *pOutput)
72 {
73 IP_FLASH_Execute(((FLASH_ENTRY_T) FLASH_ENTRY_LOCATION), pCommand, pOutput);
74 }
75
84 STATIC INLINE void Chip_FLASH_PrepareSectors(FLASH_PREPARE_SECTORS_COMMAND_T *pCommand,
85 FLASH_PREPARE_SECTORS_OUTPUT_T *pOutput)
86 {
87 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
88 }
89
98 STATIC INLINE void Chip_FLASH_CopyRamToFlash(FLASH_COPY_RAM_TO_FLASH_COMMAND_T *pCommand,
99 FLASH_COPY_RAM_TO_FLASH_OUTPUT_T *pOutput)
100 {
101 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
102 }
103
111 STATIC INLINE void Chip_FLASH_EraseSectors(FLASH_ERASE_SECTORS_COMMAND_T *pCommand,
112 FLASH_ERASE_SECTORS_OUTPUT_T *pOutput)
113 {
114 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
115 }
116
123 STATIC INLINE void Chip_FLASH_BlankCheckSectors(FLASH_BLANK_CHECK_SECTORS_COMMAND_T *pCommand,
124 FLASH_BLANK_CHECK_SECTORS_OUTPUT_T *pOutput)
125 {
126 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
127 }
128
134 void Chip_FLASH_ReadPartID(FLASH_READ_PART_ID_OUTPUT_T *pOutput);
135
141 void Chip_FLASH_ReadBootCodeVersion(FLASH_READ_BOOTCODE_VER_OUTPUT_T *pOutput);
142
151 STATIC INLINE void Chip_FLASH_CompareMem(FLASH_COMPARE_MEM_COMMAND_T *pCommand,
152 FLASH_COMPARE_MEM_OUTPUT_T *pOutput)
153 {
154 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
155 }
156
161 void Chip_FLASH_ReInvokeISP(void);
162
168 void Chip_FLASH_ReadUID(FLASH_READ_UID_OUTPUT_T *pOutput);
175 STATIC INLINE void Chip_FLASH_ErasePages(FLASH_ERASE_PAGES_COMMAND_T *pCommand,
176 FLASH_ERASE_PAGES_OUTPUT_T *pOutput)
177 {
178 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
179 }
180
188 STATIC INLINE void Chip_EEPROM_Write(EEPROM_WRITE_COMMAND_T *pCommand,
189 EEPROM_WRITE_OUTPUT_T *pOutput)
190 {
191 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
192 }
193
200 STATIC INLINE void Chip_EEPROM_Read(EEPROM_READ_COMMAND_T *pCommand,
201 EEPROM_READ_OUTPUT_T *pOutput)
202 {
203 Chip_FLASH_Execute((FLASH_COMMAND_T *) pCommand, (FLASH_OUTPUT_T *) pOutput);
204 }
205
210 #ifdef __cplusplus
211 }
212 #endif
213
214 #endif /* defined(CHIP_LPC1347) */
215
216 #endif /* __FLASH_EEPROM_13XX_H_ */