| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Enumerations | Functions
ssp_13xx.h File Reference

Go to the source code of this file.

## Data Structures
struct | SSP_ConfigFormat
struct | SPI_Address_t
struct | Chip_SSP_DATA_SETUP_T

## Macros
#define | SSP_CPHA_FIRST SSP_CR0_CPHA_FIRST
#define | SSP_CPHA_SECOND SSP_CR0_CPHA_SECOND
#define | SSP_CPOL_HI SSP_CR0_CPOL_LO
#define | SSP_CPOL_LO SSP_CR0_CPOL_HI
#define | SSP_SLAVE_MODE SSP_CR1_SLAVE_EN
#define | SSP_MASTER_MODE SSP_CR1_MASTER_EN

## Enumerations
enum | CHIP_SSP_CLOCK_MODE_T { SSP_CLOCK_CPHA0_CPOL0 = (0 << 6), SSP_CLOCK_CPHA0_CPOL1 = (1u << 6), SSP_CLOCK_CPHA1_CPOL0 = (2u << 6), SSP_CLOCK_CPHA1_CPOL1 = (3u << 6), SSP_CLOCK_MODE0 = SSP_CLOCK_CPHA0_CPOL0, SSP_CLOCK_MODE1 = SSP_CLOCK_CPHA1_CPOL0, SSP_CLOCK_MODE2 = SSP_CLOCK_CPHA0_CPOL1, SSP_CLOCK_MODE3 = SSP_CLOCK_CPHA1_CPOL1, SSP_CLOCK_CPHA0_CPOL0 = (0 << 6), SSP_CLOCK_CPHA0_CPOL1 = (1u << 6), SSP_CLOCK_CPHA1_CPOL0 = (2u << 6), SSP_CLOCK_CPHA1_CPOL1 = (3u << 6), SSP_CLOCK_MODE0 = SSP_CLOCK_CPHA0_CPOL0, SSP_CLOCK_MODE1 = SSP_CLOCK_CPHA1_CPOL0, SSP_CLOCK_MODE2 = SSP_CLOCK_CPHA0_CPOL1, SSP_CLOCK_MODE3 = SSP_CLOCK_CPHA1_CPOL1, SSP_CLOCK_CPHA0_CPOL0 = (0 << 6), SSP_CLOCK_CPHA0_CPOL1 = (1u << 6), SSP_CLOCK_CPHA1_CPOL0 = (2u << 6), SSP_CLOCK_CPHA1_CPOL1 = (3u << 6), SSP_CLOCK_MODE0 = SSP_CLOCK_CPHA0_CPOL0, SSP_CLOCK_MODE1 = SSP_CLOCK_CPHA1_CPOL0, SSP_CLOCK_MODE2 = SSP_CLOCK_CPHA0_CPOL1, SSP_CLOCK_MODE3 = SSP_CLOCK_CPHA1_CPOL1, SSP_CLOCK_CPHA0_CPOL0 = (0 << 6), SSP_CLOCK_CPHA0_CPOL1 = (1u << 6), SSP_CLOCK_CPHA1_CPOL0 = (2u << 6), SSP_CLOCK_CPHA1_CPOL1 = (3u << 6), SSP_CLOCK_MODE0 = SSP_CLOCK_CPHA0_CPOL0, SSP_CLOCK_MODE1 = SSP_CLOCK_CPHA1_CPOL0, SSP_CLOCK_MODE2 = SSP_CLOCK_CPHA0_CPOL1, SSP_CLOCK_MODE3 = SSP_CLOCK_CPHA1_CPOL1 }
enum | CHIP_SSP_FRAME_FORMAT_T { SSP_FRAMEFORMAT_SPI = (0 << 4), CHIP_SSP_FRAME_FORMAT_TI = (1u << 4), SSP_FRAMEFORMAT_MICROWIRE = (2u << 4), SSP_FRAMEFORMAT_SPI = (0 << 4), CHIP_SSP_FRAME_FORMAT_TI = (1u << 4), SSP_FRAMEFORMAT_MICROWIRE = (2u << 4), SSP_FRAMEFORMAT_SPI = (0 << 4), CHIP_SSP_FRAME_FORMAT_TI = (1u << 4), SSP_FRAMEFORMAT_MICROWIRE = (2u << 4), SSP_FRAMEFORMAT_SPI = (0 << 4), CHIP_SSP_FRAME_FORMAT_TI = (1u << 4), SSP_FRAMEFORMAT_MICROWIRE = (2u << 4) }
enum | CHIP_SSP_BITS_T { SSP_BITS_4 = (3u << 0), SSP_BITS_5 = (4u << 0), SSP_BITS_6 = (5u << 0), SSP_BITS_7 = (6u << 0), SSP_BITS_8 = (7u << 0), SSP_BITS_9 = (8u << 0), SSP_BITS_10 = (9u << 0), SSP_BITS_11 = (10u << 0), SSP_BITS_12 = (11u << 0), SSP_BITS_13 = (12u << 0), SSP_BITS_14 = (13u << 0), SSP_BITS_15 = (14u << 0), SSP_BITS_16 = (15u << 0), SSP_BITS_4 = (3u << 0), SSP_BITS_5 = (4u << 0), SSP_BITS_6 = (5u << 0), SSP_BITS_7 = (6u << 0), SSP_BITS_8 = (7u << 0), SSP_BITS_9 = (8u << 0), SSP_BITS_10 = (9u << 0), SSP_BITS_11 = (10u << 0), SSP_BITS_12 = (11u << 0), SSP_BITS_13 = (12u << 0), SSP_BITS_14 = (13u << 0), SSP_BITS_15 = (14u << 0), SSP_BITS_16 = (15u << 0), SSP_BITS_4 = (3u << 0), SSP_BITS_5 = (4u << 0), SSP_BITS_6 = (5u << 0), SSP_BITS_7 = (6u << 0), SSP_BITS_8 = (7u << 0), SSP_BITS_9 = (8u << 0), SSP_BITS_10 = (9u << 0), SSP_BITS_11 = (10u << 0), SSP_BITS_12 = (11u << 0), SSP_BITS_13 = (12u << 0), SSP_BITS_14 = (13u << 0), SSP_BITS_15 = (14u << 0), SSP_BITS_16 = (15u << 0), SSP_BITS_4 = (3u << 0), SSP_BITS_5 = (4u << 0), SSP_BITS_6 = (5u << 0), SSP_BITS_7 = (6u << 0), SSP_BITS_8 = (7u << 0), SSP_BITS_9 = (8u << 0), SSP_BITS_10 = (9u << 0), SSP_BITS_11 = (10u << 0), SSP_BITS_12 = (11u << 0), SSP_BITS_13 = (12u << 0), SSP_BITS_14 = (13u << 0), SSP_BITS_15 = (14u << 0), SSP_BITS_16 = (15u << 0) }
enum | CHIP_SSP_MODE_T { SSP_MODE_MASTER = (0 << 2), SSP_MODE_SLAVE = (1u << 2), SSP_MODE_MASTER = (0 << 2), SSP_MODE_SLAVE = (1u << 2), SSP_MODE_MASTER = (0 << 2), SSP_MODE_SLAVE = (1u << 2), SSP_MODE_MASTER = (0 << 2), SSP_MODE_SLAVE = (1u << 2) }

## Functions
STATIC INLINE FlagStatus | Chip_SSP_GetStatus (LPC_SSP_T *pSSP, IP_SSP_STATUS_T Stat)
| Get the current status of SSP controller.
STATIC INLINE void | Chip_SSP_Enable (LPC_SSP_T *pSSP)
| Enable SSP operation.
STATIC INLINE void | Chip_SSP_Disable (LPC_SSP_T *pSSP)
| Disable SSP operation.
STATIC INLINE void | Chip_SSP_EnableLoopBack (LPC_SSP_T *pSSP)
| Enable loopback mode.
STATIC INLINE void | Chip_SSP_DisableLoopBack (LPC_SSP_T *pSSP)
| Disable loopback mode.
void | Chip_SSP_Int_FlushData (LPC_SSP_T *pSSP)
| Clean all data in RX FIFO of SSP.
Status | Chip_SSP_Int_RWFrames8Bits (LPC_SSP_T *pSSP, Chip_SSP_DATA_SETUP_T *xf_setup)
| SSP Interrupt Read/Write with 8-bit frame width.
Status | Chip_SSP_Int_RWFrames16Bits (LPC_SSP_T *pSSP, Chip_SSP_DATA_SETUP_T *xf_setup)
| SSP Interrupt Read/Write with 16-bit frame width.
uint32_t | Chip_SSP_RWFrames_Blocking (LPC_SSP_T *pSSP, Chip_SSP_DATA_SETUP_T *xf_setup)
| SSP Polling Read/Write in blocking mode.
uint32_t | Chip_SSP_WriteFrames_Blocking (LPC_SSP_T *pSSP, uint8_t *buffer, uint32_t buffer_len)
| SSP Polling Write in blocking mode.
uint32_t | Chip_SSP_ReadFrames_Blocking (LPC_SSP_T *pSSP, uint8_t *buffer, uint32_t buffer_len)
| Note here.
void | Chip_SSP_Init (LPC_SSP_T *pSSP)
| Initialize the SSP.
void | Chip_SSP_DeInit (LPC_SSP_T *pSSP)
| Shutdown the SSP.
void | Chip_SSP_SetMaster (LPC_SSP_T *pSSP, bool master)
| Set the SSP operating modes, master or slave.
void | Chip_SSP_SetBitRate (LPC_SSP_T *pSSP, uint32_t bitRate)
| Set the clock frequency for SSP interface.
STATIC INLINE void | Chip_SSP_SetFormat (LPC_SSP_T *pSSP, SSP_ConfigFormat *format)
| Set up the SSP frame format.
STATIC INLINE void | Chip_SSP_Int_Enable (LPC_SSP_T *pSSP)
| Enable SSP interrupt.
STATIC INLINE void | Chip_SSP_Int_Disable (LPC_SSP_T *pSSP)
| Disable SSP interrupt.