| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
usbhs_001.h
Go to the documentation of this file.
1 /*
2 * @brief High-Speed USB registers and control functions
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __USBHS_001_H_
33 #define __USBHS_001_H_
34
35 #include "sys_config.h"
36 #include "cmsis.h"
37
38 #ifdef __cplusplus
39 extern "C" {
40 #endif
41
52 typedef struct {
53 __I uint32_t RESERVED0[64];
54 __I uint32_t CAPLENGTH;
55 __I uint32_t HCSPARAMS;
56 __I uint32_t HCCPARAMS;
57 __I uint32_t RESERVED1[5];
58 __I uint32_t DCIVERSION;
59 __I uint32_t RESERVED2[7];
60 union {
61 __IO uint32_t USBCMD_H;
62 __IO uint32_t USBCMD_D;
63 };
64
65 union {
66 __IO uint32_t USBSTS_H;
67 __IO uint32_t USBSTS_D;
68 };
69
70 union {
71 __IO uint32_t USBINTR_H;
72 __IO uint32_t USBINTR_D;
73 };
74
75 union {
76 __IO uint32_t FRINDEX_H;
77 __I uint32_t FRINDEX_D;
78 };
79
80 __I uint32_t RESERVED3;
81 union {
82 __IO uint32_t PERIODICLISTBASE;
83 __IO uint32_t DEVICEADDR;
84 };
85
86 union {
87 __IO uint32_t ASYNCLISTADDR;
88 __IO uint32_t ENDPOINTLISTADDR;
89 };
90
91 __IO uint32_t TTCTRL;
92 __IO uint32_t BURSTSIZE;
93 __IO uint32_t TXFILLTUNING;
94 __I uint32_t RESERVED4[2];
95 __IO uint32_t ULPIVIEWPORT;
96 __IO uint32_t BINTERVAL;
97 __IO uint32_t ENDPTNAK;
98 __IO uint32_t ENDPTNAKEN;
99 __I uint32_t RESERVED5;
100 union {
101 __IO uint32_t PORTSC1_H;
102 __IO uint32_t PORTSC1_D;
103 };
104
105 __I uint32_t RESERVED6[7];
106 __IO uint32_t OTGSC;
107 union {
108 __IO uint32_t USBMODE_H;
109 __IO uint32_t USBMODE_D;
110 };
111
112 __IO uint32_t ENDPTSETUPSTAT;
113 __IO uint32_t ENDPTPRIME;
114 __IO uint32_t ENDPTFLUSH;
115 __I uint32_t ENDPTSTAT;
116 __IO uint32_t ENDPTCOMPLETE;
117 __IO uint32_t ENDPTCTRL[6];
118 } IP_USBHS_001_T;
119
124 #ifdef __cplusplus
125 }
126 #endif
127
128 #endif /* __USBHS_001_H_ */