| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Mouse Device
USB examples

## Detailed Description

Example description
This example implements a HID device which is used for mouse configuration.

When the example is run and the board is connected to a PC with a USB cable it will enumerate on the PC as a HID mouse device and the joystick (SW2) on the EA Baseboard will generate mouse movement on your PC.

Special connection requirements
Need to connect with base board for using buttons and joystick

Build procedures:
LPC11xx example quickstart for Code Red Xpresso
LPC11xx example quickstart for Keil uVision4
LPC11xx example quickstart for IAR EWARM

Supported boards and board setup:
NXP Xpresso LPC11U14 board
NXP Xpresso LPC11C24 board

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Main definitions
| ROM stack support