| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Audio Output Device
USB examples

## Detailed Description

Example description
This example implements an audio interface class device mode device that enumerates as audio device (USB speakers) and sends the samples sent to it from the host to the audio circuitry on the board.

On the PC select Control Panel->Hardware and Sound->Sound When the example is first run a new entry in the Sound dialog box will appear titled Speakers and have a description that reads "4-LPCUSBlib Audio Out Demo". Below this description should be the word Ready.

To test the audio output click on this entry in the Sound dialog box. Then click on the Configure button to bring up the Speaker Setup dialog box. In this box press the Test button. Sound should be played through the left side of your headphones first, then the right side.

Special connection requirements
Need config jumpers follow : JP 22 : 2-3 JP 23 : 2-3 JP 24 : 2-3 JP 25 : 2-3 JP 26 : 2-3 JP 27 : 2-3 JP 29 : 3-4

Build procedures:
LPC17xx/40xx example quickstart for Keil uVision4
LPC17xx/40xx example quickstart for IAR EWARM
LPC17xx/40xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Embedded Artists' LPC1788 Developer's Kit
Embedded Artists' LPC4088 Developer's Kit

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Functions prototypes
| Main definitions