| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
sys_config.h
Go to the documentation of this file.
1 /*
2 * @note
3 * Copyright(C) NXP Semiconductors, 2012
4 * All rights reserved.
5 *
6 * @par
7 * Software that is described herein is for illustrative purposes only
8 * which provides customers with programming information regarding the
9 * LPC products. This software is supplied "AS IS" without any warranties of
10 * any kind, and NXP Semiconductors and its licensor disclaim any and
11 * all warranties, express or implied, including all implied warranties of
12 * merchantability, fitness for a particular purpose and non-infringement of
13 * intellectual property rights. NXP Semiconductors assumes no responsibility
14 * or liability for the use of the software, conveys no license or rights under any
15 * patent, copyright, mask work right, or any other intellectual property rights in
16 * or to any products. NXP Semiconductors reserves the right to make changes
17 * in the software without notification. NXP Semiconductors also makes no
18 * representation or warranty that such application will be suitable for the
19 * specified use without further testing or modification.
20 *
21 * @par
22 * Permission to use, copy, modify, and distribute this software and its
23 * documentation is hereby granted, under NXP Semiconductors' and its
24 * licensor's relevant copyrights in the software, without fee, provided that it
25 * is used in conjunction with NXP Semiconductors microcontrollers. This
26 * copyright, permission, and disclaimer notice must appear in all copies of
27 * this code.
28 */
29
30 #ifndef __SYS_CONFIG_H_
31 #define __SYS_CONFIG_H_
32
37 /* Build for 407x/8x chip family */
38 #define CHIP_LPC407X_8X
39
40 /* For the LPC4074, the __FPU_PRESENT definition should be set to 0 */
41 // #define __FPU_PRESENT 0
42
43 /* Build for RMII interface */
44 #define USE_RMII
45
46 /* Un-comment DEBUG_ENABLE for IO support via the UART */
47 #define DEBUG_ENABLE
48
49 /* Board UART used for debug output */
50 #define DEBUG_UART LPC_UART0
51
52 /* Crystal frequency into device */
53 #define CRYSTAL_MAIN_FREQ_IN (12000000)
54
55 /* Crystal frequency into device for RTC/32K input */
56 #define CRYSTAL_32K_FREQ_IN (32768)
57
58 /* Enable DMA in SDC driver */
59 #define SDC_DMA_ENABLE
60
65 #endif /* __SYS_CONFIG_H_ */