| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
LPC13xx FreeRTOS blinky example
FreeRTOS examples

## Detailed Description

Example description
Welcome to the FreeRTOS basic blinky example. This example starts up FreeRTOS and creates 3 tasks that blink up to 3 LEDs (if the boards support them) at different rates.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC13xx example quickstart for Code Red Xpresso
LPC13xx example quickstart for Keil uVision4
LPC13xx example quickstart for IAR EWARM

Supported boards and board setup:
NXP Xpresso LPC1347 board

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
static void | prvSetupHardware (void)
static | portTASK_FUNCTION (vLEDTask0, pvParameters)
static | portTASK_FUNCTION (vLEDTask1, pvParameters)
static | portTASK_FUNCTION (vLEDTask2, pvParameters)
int | main (void)
| main routine for FreeRTOS blinky example

## Function Documentation

int main | ( | void |  | ) |

main routine for FreeRTOS blinky example

Main program body.

Returns
  Nothing, function should not exit

defined(CHIP_LPC175X_6X)

Definition at line 118 of file freertos_blinky.c.

static portTASK_FUNCTION | ( | vLEDTask0 | ,
|  | pvParameters |
| ) |  |
| static

Definition at line 78 of file freertos_blinky.c.

static portTASK_FUNCTION | ( | vLEDTask1 | ,
|  | pvParameters |
| ) |  |
| static

Definition at line 89 of file freertos_blinky.c.

static portTASK_FUNCTION | ( | vLEDTask2 | ,
|  | pvParameters |
| ) |  |
| static

Definition at line 100 of file freertos_blinky.c.

static void prvSetupHardware | ( | void |  | ) |
| static

Definition at line 72 of file freertos_blinky.c.