| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Functions
CHIP: LPC17xx/40xx SPIFI Driver
LPC17xx/40xx chip specific drivers

## Detailed Description

## Macros
#define | SPIFLASH_BASE_ADDRESS (0x28000000)
#define | SPIFI_ROM_PTR (0x1FFF1954)

## Functions
STATIC INLINE void | Chip_SPIFI_Init (void)
| Initialize the SPIFI.
STATIC INLINE void | Chip_SPIFI_DeInit (void)
| Shutdown the SPIFI.

## Macro Definition Documentation

#define SPIFI_ROM_PTR (0x1FFF1954)

SPIFI API ROM address

Definition at line 49 of file spifi_17xx_40xx.h.

#define SPIFLASH_BASE_ADDRESS (0x28000000)

SPIFI memory base address

Definition at line 47 of file spifi_17xx_40xx.h.

## Function Documentation

STATIC INLINE void Chip_SPIFI_DeInit | ( | void |  | ) |

Shutdown the SPIFI.

Returns
  None

Definition at line 64 of file spifi_17xx_40xx.h.

STATIC INLINE void Chip_SPIFI_Init | ( | void |  | ) |

Initialize the SPIFI.

Returns
  None

Definition at line 55 of file spifi_17xx_40xx.h.